1. Acknowledgements

______________________________________________________________________________________________ On behalf of the M.I.T. X Consortium, we would like to thank all who have participated in the design, definition, and implementation of PEX.

This work began when, at the first X3D meeting at MIT in June, 1987, Digital Equipment Corporation and Sun

Microsystems, Inc. jointly proposed that a protocol be defined based upon an initial working draft developed by

Digital. This draft was influenced by comments from professional colleagues. We recognize especially the authors of that first document: Randi J. Rost, Jeffrey Friedberg, Jeffrey S. Saltz, Pete Nishimoto, and William H. Clifford,

Jr., all of Digital Equipment Corporation. They provided a head start for this major undertaking.

We owe a major debt to the PEX architecture team which met frequently between June, 1987 and August, 1991 to argue and debate issues. Members of the PEX Architecture Team: Jeffrey Friedberg, John McConnell, Pete

Nishimoto, Randi J. Rost, and Jeffrey S. Saltz of Digital Equipment Corporation; Dave Gorgen, Tom Gross, and Jeff

Stevenson of Hewlett-Packard Company; David Plunkett of Solbourne Computer; Jan Hardenbergh of Stardent

Computer, Inc.; and Marty Hess, and Jim Van Loo of Sun Microsystems.

Our sincerest thanks are also extended to Bertram Herzog of the University of Michigan, who served as chairman of the X3D organization and was responsible for overseeing a fair and timely process designed to bring the PEX project to fruition.

Several members of the X3D group provided valuable comments to the PEX architecture team. We note especially the contributions of James Michener of Hewlett-Packard Company, and Todd Newman and Raymond Drewry of

Digital Equipment Corporation who attended architecture team meetings and provided much-needed insight at critical points during the evolution of PEX. Others who have participated actively in technical discussions include

Sally C. Barry, Andy Vesper, and Ray Shapiro of Digital Equipment Corporation.

We also give thanks to early implementors of PEX, including the PEX Sample Implementation team at Sun

Microsystems, for providing useful review and sanity checks of the PEX specification documents. The PEX-SI team at Sun includes Marty Hess, Lisa Chabot, Cheryl Huntington, Erwin Hom, Nash Aragam, Tom Gaskins, John

Recker, and Chris Nicholas.

Robert Scheifler, Director of the X Consortium at M.I.T., provided invaluable critique and advice that ensured that our efforts conformed to the spirit and definition of the X Window System. Jim Fulton of the X Consortium also contributed to meetings and to technical discussions.

To Randi Rost, the first PEX Document Editor, go the thanks of all, for translating all the decisions into the written word. Sally Barry and Jeff Friedberg are gratefully acknowledged for providing thorough and painstaking review of many intermediate drafts of these early PEX documents. Sally Barry, document editor for PEX 5.0, gratefully acknowledges the invaluable assistance and encouragement of Jeff Friedberg, Jan Hardenbergh, and Randi Rost, during the production of the PEX 5.0 specifications. Paula Womack, document editor for PEX 5.1, acknowledges

Ken Garnett of Shographics, for his thorough and timely review of the protocol specification.

In addition the careful review by the PEX teams at all the various companies that are working on PEX implementations has greatly helped the accuracy and precision of this document.

Thanks also to the individuals that worked on the X11, PHIGS, and PHIGS-PLUS specification documents, from which some PEX descriptions were obtained.

Finally, we acknowledge the contributions of all of the other participants in this effort that have not been explicitly named. The contributions of so many individuals has helped to ensure that PEX will be a useful and long-lived extension to the X Window System.PEX Version 5.1, 31-August-1992

2. PEX Protocol Specification

______________________________________________________________________________________________ 2.1. Request Processing

Workstation regeneration and requests which process output commands are not guaranteed to be atomic with respect to concurrent rendering to the same destination drawable. However atomicity of execution is guaranteed for each individual output command primitive, excluding Execute Structure, GSE, GDP 3D, and GDP 2D. Also, requests and output commands will be executed in sequential order for a given connection.

2.2. Protocol Format

All PEX† protocol formats are based on the formats specified by the XWindowSystemProtocol, Version11‡, which is referred to as X11 throughout the remainder of this document. The PEX protocol will adhere to the philosophy and requirements of X11.

2.2.1. Request Format

Every X11 request contains a 4-byte header which contains an 8-bit major opcode, an 8-bit data field, and a 16-bit length field. The header is followed by zero or more additional bytes of data, the length of which is specified by the length field. Since PEX is a proper extension of X11, the 8-bit major opcode contains the opcode assigned for the

PEX extension by X11. The length field contains the length of the request in units of four bytes, including the header. The data (or minor opcode) field contains the PEX opcode for this request.

2.2.2. Reply Format

Every reply consists of at least 32 bytes. A header is contained in these 32 bytes. The header of a reply consists of a

32-bit length field, a 16-bit sequence number field, and an 8-bit type field. Zero or more additional bytes follow the header as specified in the length field. The length field specifies the length of the data following the 32 byte reply header and is in units of four bytes. Unused bytes within a reply are not guaranteed to be zero. The sequence number field contains the least significant 16 bits of the sequence number of the corresponding request. The type field defines the type of reply generated.

2.2.3. Error Format

Error reports are 32 bytes long. Every error includes an 8-bit error code. This error code is used to signify the specific PEX error that occurred. Every error reply also includes the major opcode (the extension reporting the error is identified by the major opcode), the minor opcode (the extension opcode which caused the error), and the least significant 16 bits of the sequence number of the request which had failed. Also included is an 8-bit type field which designates the packet as being an error packet. Unused bytes within an error are not guaranteed to be zero.

__________________ † X3D-PEX and PEX are trademarks of the Massachusetts Institute of Technology

‡"X Window System" is a trademark of the Massachusetts Institute of Technology

PEX Version 5.1, 31-August-1992

2.2.4. Event Format

Events are 32 bytes long. Every event contains an 8-bit type code. The most significant bit in this field is set if the event was generated from a SendEvent request. Event codes 64-127 are reserved for extensions. The core X11 protocol does not define a mechanism for expressing interest in events generated by extensions.

PEX Version 5.1, 31-August-1992

2.3. Syntax

Curly braces {...} enclose a set of alternatives. Square brackets [...] enclose a list of structure components. When embedded in descriptions, request names are printed in boldface (e.g., PEXCreateStructure). Request parameters are lower case, use the underscore (_) for separation, and are printed in italics (e.g., item_mask). Defined constants, registered enumerated type mnemonics, or alternative values have an initial capital letter, may use capital letters for separation, and are printed in italics (e.g., RGBFloat). Defined types are printed in all caps, use the underscore for separation, and are printed in the standard font (e.g., COORD_3D).

Requests are described as follows:

Name: PEXSampleRequest

Request:arg1 : type1 argN : typeN

Reply: result1 : type1 resultM : typeM

Errors: kind1,..., kindK

Description:Functional description goes here

If no reply description is given, then the request has no reply (it is asynchronous), but errors may still be reported.

2.4. Naming Conventions

PEX requests use a consistent naming convention. The verbs that are commonly used in request names are described here.Create Create an instance of a resource

Free Mark a resource as no longer accessible by clients, and deallocate the system resources it uses (e.g. memory) if it is not referenced by any other resources

Copy Copy attributes from one resource to another of the same type

Get Return resource attributes from the server to the client

Change Modify attributes of a resource

Set Modify a selected attribute of a resource

Destroy Remove an instance of a resource and all references to it, and deallocate the memory associated with it

Delete Remove some portion of a resource

Fetch Return structure elements from the server to the client

Store Send structure elements from the client to a structure resource in the server

Begin Perform an initialization step of some kind

End Perform a termination step of some kind

PEX Version 5.1, 31-August-1992

2.5. Common Types

The types listed in this section define the common types used in the PEX protocol specification.

2.5.1. LISTofFOO

A type name of the form LISTofFOO means a counted list of elements of type FOO; the size of the length field may vary (it is not necessarily the same size as FOO). In cases where the number of items in the list is easily computed, the number of items may not be supplied. In all other cases in the PEX protocol (except for LISTofVALUE), the length field is explicit.

2.5.2. BITMASK and LISTofVALUE

The types BITMASK and LISTofVALUE are somewhat special. Various requests contain arguments of the form:

item_mask: BITMASK item_list : LISTofVALUE used to allow the client to specify a subset of a heterogeneous collection of "arguments". The item_maskspecifies which arguments are to be provided; each such argument is assigned a unique bit position. The representation of

BITMASK may contain more bits than there are defined arguments; unused bits in the item_maskmust be zero (or the extension will generate a Valueerror). The item_listcontains one item for each one bit in the mask, from least to most significant bit in the mask.

2.5.3. Floating Point Format - FLOAT

The PEX protocol allows floating-point values to be passed in various floating-point formats. All floating-point arguments will be specified as FLOAT, which is defined to be the floating-point type contained in the format word associated with the request. Furthermore, items such as MATRIX, VECTOR, and COORD will be in the floatingpoint format specified by the format word associated with the request.

2.5.4. Colors

In PEX, colors are typically passed as a color type and a value. The color type specifies whether the color is an index value or a direct color value of some type. PEX servers are required to be able to deal with indexed colors and at least one type of direct color. Indexed colors are specified using an index which is used to obtain the color from a color lookup table. Direct colors are specified directly as RGB, HSV, HLS, or CIELUV color values of some form.

The list of registered direct color formats can be found in the "Extension Information" section. PEX servers are free to store direct color values in whatever implementation-dependent format they choose, but they must be capable of converting those values back into the originally-specified color type when queried by the client.

2.5.5. Element Types

Chapter 3 describes the set of output commands that are recognized by a PEX implementation. These output commands are distinguished by a 16-bit ELEMENT_TYPE value. This value contains a 16-bit unsigned short that defines the actual type of output command. The high-order bit of the element type is used to signify whether the output command is a standard PEX output command (high-order bit equals zero) or whether the output command is a proprietary addition to the set of standard PEX output commands. Servers are expected to be able to create structure elements containing non-standard PEX output commands, but the execution of such output commands can be a no-op. Since the contents of these output commands is unknown, no floating-point conversions or byteswapping will be performed on non-standard output commands that are not supported by the server. Unlike the use of the PHIGS-style GSE and GDP output commands, this extension mechanism allows vendors to gracefully add fully-integrated functionality to the standard PEX extension, and permits an implementation to ignore output commands with which it is not familiar.PEX Version 5.1, 31-August-1992

2.5.6. Types

The PEX Protocol types are as follows:

ASF_ATTRIBUTE : {MarkerTypeASF,MarkerScaleASF,MarkerColorASF,

TextFontIndexASF,TextPrecASF,CharExpansionASF,

CharSpacingASF, TextColorASF,LineTypeASF,

LineWidthASF,LineColorASF,CurveApproxASF,

PolylineInterpASF,InteriorStyleASF,InteriorStyleIndexASF,

SurfaceColorASF,SurfaceInterpASF,ReflectionModelASF,

ReflectionAttrASF,BFInteriorStyleASF,BFInteriorStyleIndexASF,

BFSurfaceColorASF,BFSurfaceInterpASF,BFReflectionModelASF,

BFReflectionAttrASF,SurfaceApproxASF,SurfaceEdgesASF,

SurfaceEdgeTypeASF,SurfaceEdgeWidthASF,SurfaceEdgeColorASF}

ASF_SPECIFIER : [enables, asfs : BITMASK]

ASF_VALUE : {Bundled,Individual}

ATEXT_STYLE : ENUM_TYPE_INDEX (used with ATextStyleenumerated type)

BITMASK : CARD32

BITMASK_SHORT : CARD16

BOOLEAN : {False, True}

BUFFER_MODE : {Single,Double}

CARD8 : unsigned 8-bit integer

CARD16 : unsigned 16-bit integer

CARD32 : unsigned 32-bit integer

CHARACTER : {CARD8, CARD16, CARD32}

COLOR : {TABLE_INDEX, DIRECT_COLOR†}

CLIP_INDICATOR : {Clip, NoClip}

COLOR_APPROX_MODEL : ENUM_TYPE_INDEX (used with ColorApproxModelenumerated type)

COLOR_APPROX_TYPE : ENUM_TYPE_INDEX (used with ColorApproxTypeenumerated type)

COLOR_MODEL : ENUM_TYPE_INDEX (used with RenderingColorModel enumerated type)

COLOR_SPECIFIER : [color_type : COLOR_TYPE, color_value : COLOR]

COLOR_TYPE : ENUM_TYPE_INDEX (used with ColorTypeenumerated type)

COMPOSITION : {PreConcatenate, PostConcatenate, Replace}

CONSTANT_NAME : CARD16

CONTOUR : {Disjoint, Nested,Intersecting, Unknown}

COORD : {COORD_2D, COORD_3D, COORD_4D}

COORD_2D : [x, y : FLOAT]

COORD_3D : [x, y, z : FLOAT]

COORD_4D : [wx, wy, wz, w : FLOAT]

COORD_TYPE : {Rational, NonRational}

CULL_MODE : {None,BackFaces, FrontFaces}

CURVE_APPROX : [approx_method : CURVE_APPROX_METHOD, tolerance : FLOAT]

CURVE_APPROX_METHOD : ENUM_TYPE_INDEX (used with CurveApproxMethodenumerated type)

DC_HIT_BOX_DATA : [pick_position: DEVICE_COORD_2D, pick_distance: FLOAT]

DEVICE_COORD : [x, y : INT16, z : FLOAT]

DEVICE_COORD_2D : [x, y : INT16]

DEVICE_RECT : [xmin, ymin, xmax, ymax : INT16]

DIRECT_COLOR : direct color value†

DISPLAY_STATE : {NotEmpty,Empty}

__________________ † See the "Extension Information" section for a list of the registered color types.

PEX Version 5.1, 31-August-1992

DISPLAY_UPDATE : ENUM_TYPE_INDEX (used with DisplayUpdateMode enumerated type)

DRAWABLE_ID : {WINDOW_ID, PIXMAP_ID}

DYNAMIC_TYPE : {IMM,IRG,CBS}

ECHO_MODE : {NoEcho,Echo, Unecho}

EDGE : OPT_SWITCH

EDIT_MODE : {StructureInsert, StructureReplace}

ELEMENT_INFO : [type : ELEMENT_TYPE, length : CARD16]

ELEMENT_POS : [whence : {Beginning,Current, End}, offset : INT32]

ELEMENT_RANGE : [position1, position2 : ELEMENT_POS]

ELEMENT_REF : [structure_id : STRUCTURE_ID, offset : CARD32]

ELEMENT_TYPE : CARD16

ENUM_TYPE :{MarkerType,ATextStyle,InteriorStyle, HatchStyle,

LineType,SurfaceEdgeType,PickDeviceType,

PolylineInterpMethod, CurveApproxMethod,ReflectionModel,

SurfaceInterpMethod, SurfaceApproxMethod,

ModelClipOperator, LightType,ColorType,

FloatFormat, HLHSRMode,PromptEchoType,

DisplayUpdateMode, ColorApproxType,ColorApproxModel,

GDP, GDP3, GSE,TrimCurveApproxMethod,

RenderingColorModel, ParametricSurfaceCharacteristics,

Escape, PickOneMethod,PickAllMethod}

ENUM_TYPE_INDEX : INT16

EXTENT_INFO : [lower_left : COORD_2D, upper_right : COORD_2D, concatpoint : COORD_2D]

FACET : [facet_data : OPT_DATA, vertices : LISTofVERTEX]

FLOAT : floating point value†

FLOAT_FORMAT : ENUM_TYPE_INDEX (used with FloatFormat enumerated type)

FONT_ID : {PEX_FONT_ID, X11_FONT_ID}

HALFSPACE : [point : COORD_3D, vector : VECTOR_3D]

HALFSPACE_2D : [point : COORD_2D, vector : VECTOR_2D]

HATCH_STYLE : ENUM_TYPE_INDEX (used with HatchStyleenumerated type)

HLHSR_MODE : ENUM_TYPE_INDEX (used with HLHSRModeenumerated type)

INT8 : signed 8-bit integer

INT16 : signed 16-bit integer

INT32 : signed 32-bit integer

INTERIOR_STYLE : ENUM_TYPE_INDEX (used with InteriorStyle enumerated type)

ISTRING : LISTofMONO_ENCODING

LIGHT_TYPE : ENUM_TYPE_INDEX (used with LightTypeenumerated type)

LINE_TYPE : ENUM_TYPE_INDEX (used with LineTypeenumerated type)

LOOKUP_TABLE_ID : RESOURCE_ID

MARKER_TYPE : ENUM_TYPE_INDEX (used with MarkerTypeenumerated type)

MATCH_DRAW_TYPE :{DontCare, Window,Pixmap, Buffer}

MATRIX : FLOAT[4][4]‡

__________________ † See the "Extension Information" section for a list of the registered floating point formats.

PEX Version 5.1, 31-August-1992

MATRIX_3X3 : FLOAT[3][3]‡

MONO_ENCODING : [char_set : CARD16, char_set_width : {csByte,csShort, csLong}, encoding_state : CARD8, string : LISTofCHARACTER]

NAME : CARD32

NAME_SET_ID : RESOURCE_ID

NAME_SET_PAIR : [incl: NAME_SET_ID, excl: NAME_SET_ID]

NPC_SUBVOLUME : [min : COORD_3D, max : COORD_3D]

OPERATOR : ENUM_TYPE_INDEX (used with ModelClipOperator enumerated type)

OPT_COLOR : optional COLOR†

OPT_DATA : [color : OPT_COLOR, normal : OPT_NORMAL, edge : OPT_SWITCH ]

OPT_NORMAL : optional VECTOR_3D†

OPT_SWITCH : optional SWITCH†

OUTPUT_CMD : [element_type : ELEMENT_TYPE, size : CARD16, data : ‡ ]

PC_BITMASK : CARD32[3]

PEX_FONT_ID : RESOURCE_ID

PHIGS_WKS_ID : RESOURCE_ID

PIPELINE_CONTEXT_ID : RESOURCE_ID

PICK_ALL_METHOD : ENUM_TYPE_INDEX (used with PickAllMethodenumerated type)

PICK_ALL_STATE : {MoreHits, NoMoreHits, MayBeMoreHits}

PICK_DATA : {DC_HIT_BOX_DATA, NPC_SUBVOLUME}

PICK_DEVICE_TYPE : ENUM_TYPE_INDEX (used with PickDeviceTypeenumerated type)

PICK_ELEMENT_REF : [s_id : STRUCTURE_ID, offset : CARD32, pickid : CARD32]

PICK_MEASURE_ID : RESOURCE_ID

PICK_ONE_METHOD : ENUM_TYPE_INDEX (used with PickOneMethodenumerated type)

PICK_RECORD : [pick_type: PICK_DEVICE_TYPE, hit_box: PICK_DATA ]

PICK_STATUS : {NoPick, Ok, Aborted}

PIXMAP_ID : RESOURCE_ID

POLYLINE_INTERP : ENUM_TYPE_INDEX (used with PolylineInterpMethod enumerated type)

PROMPT_ECHO_TYPE : ENUM_TYPE_INDEX (used with PromptEchoTypeenumerated type)

PSC_TYPE : ENUM_TYPE_INDEX (used with ParametricSurfaceCharacteristics enumerated type)

PSURF_CHAR : [psc_type : PSC_TYPE, psc_data : LISTofCARD8]

REFLECTION_ATTR : [ambient_coef : FLOAT, diffuse_coef : FLOAT,

__________________ ‡ Matrices are effectively passed as one-dimensional arrays of floating point values. For a 4×4 matrix, the matrix element used to represent the x translation value will be the fourth element in the array, the element containing the y translation value will be the eighth element, etc. 3×3 matrices are handled analogously.

† Indicates a parameter (or portion of a parameter) that may or may not be present in the request. However, its presence or absence can always be inferred from previous parameters in the request.

‡ See Section 3 - Output Commands for a description of each of the data records that can be passed/returned as an output command. PEX Version 5.1, 31-August-1992

specular_coef : FLOAT, specular_conc : FLOAT, transmission_coef : FLOAT, specular_color : COLOR_SPECIFIER]

REFLECTION_MODEL : ENUM_TYPE_INDEX (used with ReflectionModelenumerated type)

RENDERER_ID : RESOURCE_ID

RENDERER_STATE : {Idle, Rendering, Picking}

RENDERER_TARGET : [depth: CARD8, type: MATCH_DRAW_TYPE, visual: VISUAL_ID ]

RESOURCE_ID : 32-bit identifier

SEARCH_CONTEXT_ID : RESOURCE_ID

SHAPE : {Convex,Nonconvex,Complex,Unknown}

STRING : LISTofCARD8

STRUCTURE_ID : RESOURCE_ID

STRUCTURE_INFO : [id: RESOURCE_ID, priority: FLOAT]

SURFACE_APPROX : [approx_method : SURFACE_APPROX_METHOD, u_tolerance, v_tolerance : FLOAT]

SURFACE_APPROX_METHOD : ENUM_TYPE_INDEX (used with SurfaceApproxMethodenumerated type)

SURFACE_EDGE_TYPE : ENUM_TYPE_INDEX (used with SurfaceEdgeTypeenumerated type)

SURFACE_INTERP : ENUM_TYPE_INDEX (used with SurfaceInterpMethod enumerated type)

SWITCH : {Off,On}

TABLE_ENTRY : [data : * ]

TABLE_INDEX : CARD16

TABLE_TYPE : {LineBundle,MarkerBundle, TextBundle,InteriorBundle,

EdgeBundle,Pattern, TextFont,Color, View,Light,

DepthCue, ColorApprox}

TEXT_ALIGNMENT : [vertical : TEXT_VALIGNMENT, horizontal : TEXT_HALIGNMENT]

TEXT_HALIGNMENT : {HalignNormal, HalignLeft, HalignRight, HalignCenter}

TEXT_PATH : {PathRight, PathLeft, PathUp, PathDown}

TEXT_PRECISION : {String, Char, Stroke}

TEXT_VALIGNMENT : {ValignNormal, ValignTop,ValignCap, ValignHalf,

ValignBase,ValignBottom}

TRIM_CURVE : [visibility : SWITCH, order : CARD16, type : COORD_TYPE, approx_method : TRIM_CURVE_APPROX_METHOD, tolerance : FLOAT, tmin, tmax : FLOAT, knots : LISTofFLOAT, points : LISTofCOORD]

TRIM_CURVE_APPROX_METHOD : ENUM_TYPE_INDEX (used with TrimCurveApproxMethod enumerated type)

TYPE_OR_TABLE_INDEX : {ENUM_TYPE_INDEX, TABLE_INDEX}

UPDATE_STATE : {NotPending, Pending}

VECTOR_2D : [x, y : FLOAT]

VECTOR_3D : [x, y, z : FLOAT]

VERTEX : [point : COORD_3D, data : OPT_DATA]

__________________ * See the section "Lookup Tables" for a description of each of the data records that can be passed/returned as a table entry.

PEX Version 5.1, 31-August-1992

VIEWPORT : [min : DEVICE_COORD, max : DEVICE_COORD, use_drawable : BOOLEAN]

VIEW_REP : [index : TABLE_INDEX, clip_flags : BITMASK, clip_limits : NPC_SUBVOLUME, orientation : MATRIX, mapping : MATRIX]

VISUAL_ID : RESOURCE_ID

VISUAL_STATE : {Correct, Deferred, Simulated}

WINDOW_ID : RESOURCE_ID

WKS_BITMASK : CARD32[2]

X11_FONT_ID : RESOURCE_ID

PEX Version 5.1, 31-August-1992

2.5.7. Errors

If an error occurs while processing a request that modifies a PEX resource then it is possible that some portion of the resource (or some subset of the resource attributes) will have been altered.

The PEX Protocol uses the same set of error codes as the X11 Protocol when applicable. Additional error codes are provided for PEX-specific errors. The following error codes can be returned by the various PEX requests:

ColorTypeThe specified color type is not supported.

FloatingPointFormat

The specified floating point format is not supported.

Label The specified label does not exist in the structure.

LookupTable

A value for a lookup table argument is illegal or does not name a defined lookup table resource.

NameSetA value for a name set argument is illegal or does not name a defined name set resource.

OutputCommand

A value for some parameter of an output command is illegal, out of range, or otherwise inappropriate.

Path A value for a structure network path contains inappropriate or illegal values.

PEXFontA value for a PEX font argument is illegal or does not name a defined PEX font resource.

PhigsWKSA value for a PHIGS workstation argument is illegal or does not name a defined PHIGS workstation resource.

PickMeasure

A value for a pick measure argument is illegal or does not name a defined pick measure resource.

PipelineContext

A value for a pipeline context argument is illegal or does not name a defined pipeline context resource.

RendererA value for a renderer argument is illegal or does not name a defined renderer resource.

RendererState

A renderer was in the Rendering state when a PEXBeginRendering request was received.

SearchContext

A value for a search context argument is illegal or does not name a defined search context resource.

StructureA value for a structure argument is illegal or does not name a defined structure resource.

2.6. Events

All PEX events will use the same mechanisms as X events.

PEX defines a new event, MaxHitsReached. PEXGetImpDepConstants can be used to determine whether this event is supported. This event is returned during a client side pick all traversal to indicate that the maximum number

PEX Version 5.1, 31-August-1992 of hits has been reached. The event includes the renderer identifier. Upon receiving the event, the client should terminate the pick traversal and decide whether an additional pass is necessary.

2.7. Padding

Certain values that must line up on 2- or 4-byte boundaries may necessitate the insertion of pad bytes in some requests. The value of pad bytes is undefined.PEX Version 5.1, 31-August-1992

2.8. Extension Information

These requests return static information about the PEX extension and what it supports. Information about specific capabilities and tradeoffs should be found in the documentation describing a particular PEX server implementation

(e.g., what is the "best" HLHSR method or floating point format or direct color format to use, whether quick update really does anything, what range of line and surface edge widths are supported, etc.)

2.8.1. Get Extension Information

Name: PEXGetExtensionInfo

Request:client_protocol_major_version : CARD16 client_protocol_minor_version : CARD16

Reply: protocol_major_version : CARD16 protocol_minor_version : CARD16 vendor : STRING release_number : CARD32 subset_info: CARD32

Errors: None

Description:The client_protocol_major_version and the client_protocol_minor_version indicate what version of the protocol the client expects the server to implement. The protocol version numbers returned indicate the protocol the PEX extension actually supports. This might not equal the version sent by the client. A PEX extension can (but need not) support more than one version simultaneously. The protocol_major_version and the protocol_minor_version are a mechanism to support future revisions of the PEX protocol which may be necessary. In general, the major version would increment for incompatible changes, and the minor version would increment for small, upward-compatible changes. Servers that support the protocol defined in this document will return a protocol_major_version of five, and a protocol_minor_version of one. The vendor parameter is a string of ISO-LATIN1 characters that describes the vendor that supplied the PEX extension. The release number is a 32-bit value whose semantics are controlled by the vendor. The top 16 bits of subset_infoare reserved for use by vendors and the bottom 16 bits contain information about whether the PEX server is a full PEX implementation or whether it supports some combination of the standard subsets.

If the 16 low-order bits of subset_infoare zero, the extension is a complete PEX implementation. If the lowest-order bit of subset_infois set, then the PEX extension supports "immediate rendering". If the nextto-lowest-order bit of subset_infois set, then the PEX extension supports "PHIGS workstation". If the third-lowest bit of subset_infois set, then the PEX extension supports "structure rendering". If a server is sent a request that is not in the PEX subset supported by that server, it will return a Requesterror. See

Appendix A for the definition of "immediate rendering", "PHIGS workstation", and "structure rendering" subsets.

The string "X3D-PEX" should be returned by the X request ListExtensions to indicate the presence of the

PEX extension. The same string should be used by clients in the X request QueryExtension.

PEX Version 5.1, 31-August-1992

2.8.2. Get Enumerated Type Information

Name: PEXGetEnumeratedTypeInfo

Request:drawable_id : DRAWABLE_ID enum_types: LISTofENUM_TYPE item_mask: BITMASK

Reply: types: LISTofLISTofVALUE

Errors: Drawable, Match, Value

Description:This request returns information about the enumerated types specified by enum_types. It returns information about the enumerated types that are supported for drawables that have the same root window and depth as the drawable indicated by drawable_id. The item_maskindicates the data that is to be returned to describe each enumerated type. The components of an enumerated type descriptor (and the corresponding bits of item_mask)are:

index : ENUM_TYPE_INDEX mnemonic : STRING

If only the indexbit is set in item_mask,a list of index values (type ENUM_TYPE_INDEX) will be returned for the defined values for each enumerated type specified in the enum_typeslist. If only the mnemonicbit is set in item_mask,only descriptor strings that use the ISO-Latin1 encoding will be returned for the defined values (type STRING). If both the indexand mnemonicbits are set, an index/mnemonic pair will be returned for each of the defined values for each of the requested enumerated types. If neither bit is set, a list of counts will be returned, where each count represents the number of supported types for each entry in enum_types.

The various enumerated types and registered values are listed below. Each registered value is followed by the mnemonic string that is returned and a brief description. Strings are returned using the ISO-Latin1 character set. The strings are returned exactly as shown below. Any enumerated type values less than zero are implementation-dependent (consult the implementation documentation for their descriptions), and any numbers greater than the listed values are reserved for future registration.

MarkerType

The marker type specifies the shape of the marker primitive that is to be drawn when rendering marker primitives. The registered values are:

1 Dot "." which is always displayed as the smallest displayable dot (the marker_scale attribute is ignored) with the dot at the marker position.

2 Cross "+" (cross or plus sign) with intersection at the marker position.

3 Asterisk "*" with intersection at the marker position.

4 Circle "o" with center at marker position.

5 X "x" with intersection at the marker position.

ATextStyleThe annotation text style specifies the style that is to be used when rendering annotation text

PEX Version 5.1, 31-August-1992 primitives. The registered values are:

1 NotConnected The annotation text primitive will be drawn with no line connecting it to the annotation text reference point.

2 Connected The annotation text primitive will be connected to the annotation text reference point with a line, which will be drawn using the current set of line attributes.

LineTypeThe line type specifies the style that is to be used when rendering polyline and curve primitives. The registered values are:

1 Solid Draw the polyline or curve with a solid, unbroken line.

2 Dashed Draw the polyline or curve with a line that is dashed.

3 Dotted Draw the polyline or curve with a line that is dotted.

4 DashDot Draw the polyline or curve with a line that contains alternating dots and dashes.

It is implementation-dependent whether the sequence for the Dashed, Dotted, and DashDot line types is restarted or continued at the start of the polyline, at the start of a clipped segment of a polyline, and at each vertex of a polyline.

PolylineInterpMethod

The polyline interpolation method specifies the style that is to be used when rendering polyline primitives that have colors specified per-vertex. Depth-cueing is applied as a post-process to polylines regardless of the polyline interpolation method. The registered values are:

1 None No interpolation will be performed between polyline vertices.

If color values are supplied that differ for the endpoints of a polyline segment, it is implementation-dependent whether the color of the ith vertex will be used to draw the line between the ith and (i+1)th vertices (if n is the number of vertices, the color at the nth will be ignored), or whether they will be used to compute an average color which will be used for the entire segment.

2 Color The polyline’s vertex colors (if present) are used. Color values along each polyline segment are then computed by linearly interpolating between the color values at the vertices.

CurveApproxMethod

The curve approximation method specifies the method that is to be used when rendering non-uniform rational B-spline (NURB) curve primitives. The registered values are:

1 (imp. dep.) This value for CurveApproxMethodis supported on every implementation, but may differ from one to the next.

It may have the same mnemonic and definition as one of the other types, or it may be a method that is not in the list of registered types. tolerance is not used for this method.

PEX Version 5.1, 31-August-1992

2 ConstantBetweenKnots This technique tessellates the curve with equal parametric increments between successive pairs of knots. The tolerance value controls tesselation of the curve. If the tolerance value is not an integer value, it is truncated and only the integer portion will be used. If tolerance is less than or equal to zero, the curve will be evaluated only at the parameter limits, and at the knots that are within the specified parameter range. If tolerance is greater than zero, the curve will be evaluated at the parameter limits, at the knots that are within the specified parameter range, and at the number of positions specified by tolerance between each pair of knots.

3 WCS_ChordalSize This technique tessellates the curve until the length of each line segment (chord) in world coordinates is less than the tolerance.

4 NPC_ChordalSize This technique tessellates the curve until the length of each line segment (chord) in normalized project coordinates is less than the tolerance.

5 DC_ChordalSize This technique tessellates the curve until the length of each line segment (chord) in device coordinates is less than the tolerance.

6 WCS_ChordalDev This technique tessellates the curve until the maximum deviation (in world coordinates) between the line and the curve is less than the tolerance.

7 NPC_ChordalDev This technique tessellates the curve until the maximum deviation (in normalized projection coordinates) between the line and the curve is less than the tolerance.

8 DC_ChordalDev This technique tessellates the curve until the maximum deviation (in device coordinates) between the line and the curve is less than the tolerance.

9 WCS_Relative This technique maintains a relative level of quality based on the tolerance value independent of scaling in world coordinates.

The tolerance must be between 0 and 1 with values closer to 1 specifying a better relative quality.

10 NPC_Relative This technique maintains a relative level of quality based on the tolerance value independent of scaling in normalized projection coordinates. The tolerance must be between 0 and 1 with values closer to 1 specifying a better relative quality.

11 DC_Relative This technique maintains a relative level of quality based on the tolerance value independent of scaling in device coordinates.

The tolerance must be between 0 and 1 with values closer to 1 specifying a better relative quality.

InteriorStyle

The interior style specifies the style that is to be used when rendering surface primitives. The

PEX Version 5.1, 31-August-1992 registered values are:

1 Hollow The interiors of surface primitives are not filled, but the boundary is drawn using the surface color. If the surface primitive is clipped as a result of modeling, view, or workstation clipping, the boundary must be drawn along the clipped boundary as well.

2 Solid The interiors of surface primitives are filled using the surface color.

3 Pattern The interiors of surface primitives are filled using the pattern table entry specified by the interior style index.

4 Hatch The interiors of surface primitives are filled using the surface color and the hatch style whose index is specified by the interior style index.

5 Empty The interior of the surface primitive is not drawn at all.

HatchStyleThe hatch style specifies the method that is to be used to render surface primitives when the interior style is set to Hatch. There are currently no registered hatch styles.

SurfaceEdgeType

The surface edge type specifies the style that is to be used when rendering surface edges. The

1 Solid Draw the surface edge with a solid, unbroken line.

2 Dashed Draw the surface edge with a line that is dashed.

3 Dotted Draw the surface edge with a line that is dotted.

4 DashDot Draw the surface edge with a line that contains alternating dots and dashes.

It is implementation-dependent whether the sequence for the Dashed, Dotted, and DashDot edge types is restarted or continued at the start of the edge, at the start of a clipped segment of an edge, and at each vertex.

ReflectionModel

The reflection model specifies the method that is used to perform the light source shading computation when rendering surface primitives. The input to the light source shading computation is known as the intrinsic color and the output is known as the shaded color. If a normal exists at the point at which the reflection model is to be evaluated, it will be used. Otherwise, if a normal exists for the facet containing the point, it will be used to evaluate the reflection model. If no normal exists, the reflection model is evaluated, if possible, without a normal. The registered values are:

1 NoShading No light source shading computation is performed. The surface color is not affected by light source illumination

(effectively, shaded color ≡ intrinsic color).

2 Ambient Only the ambient terms of the lighting equation are used.

The shaded color will be the intrinsic color as seen under

PEX Version 5.1, 31-August-1992 ambient light.

3 Diffuse Only the ambient and diffuse terms of the lighting equation are used. The shaded color will be the intrinsic color as seen under ambient light, plus a diffuse reflection component from each light source.

4 Specular The ambient, diffuse, and specular terms of the lighting equation are all used during the light source shading computation. The shaded color will be the same as for

Diffuse,plus a specular reflection component from each light source.

SurfaceInterpMethod

The surface interpolation method specifies the method that is used to compute color values in surface interiors when rendering surface primitives. Depth-cueing is applied as a post-process to surface primitives regardless of the surface interpolation method. The registered values are:

1 None The color resulting from a single light source computation is used for the entire surface. No interpolation will be performed across surface interiors or edges.

2 Color The colors are computed at the vertices of the surface according to the current reflection_model. These color values are then linearly interpolated across the interior of the surface or the edges.

3 DotProduct The lighting equation dot products are computed at the vertices. These dot products are linearly interpolated and the light source shading computation is applied using these values to compute the color value at each pixel in the interior of a surface or along a surface edge.

4 Normal An attempt is made to interpolate the normal across the facet and perform the light source shading computation as accurately as possible at each pixel in the interior of a surface or along a surface edge.

SurfaceApproxMethod

The surface approximation method specifies how to display non-uniform rational B-spline surface primitives. The registered values are:

1 (imp. dep.) This value for SurfaceApproxMethodis supported on every implementation, but may differ from one to the next.

It may have the same mnemonic and definition as one of the other types, or it may be a method that is not in the list of registered types. The tolerance values are not used for this method.

2 ConstantBetweenKnots This technique tessellates the surface with equal parametric increments between successive pairs of knots. The two tolerance values control tesselation in each of the two parameter dimensions.

PEX Version 5.1, 31-August-1992

If the tolerance values are not integer values, they are truncated and only the integer portions of each will be used. If u_tolerance is less than or equal to zero, the surface will be evaluated only at the u parameter limits in the u direction, and at the u knots that are within the specified parameter range. If u_tolerance is greater than zero, the surface will be evaluated at the u parameter limits in the u direction, at the u knots that are within the specified parameter range, and at the number of positions specified by u_tolerance between each pair of knots. The value of v_tolerance is used similarly to control the evaluation in the vdirection.

3 WCS_ChordalSize This technique tessellates the surface until the length of each line segment (chord) in world coordinates in the u parameter direction is less than the specified u tolerance value, and the length of every line segment in world coordinates in the vparameter direction is less than the specified vtolerance value.

4 NPC_ChordalSize This technique tessellates the surface until the length of each line segment (chord) in normalized projection coordinates in the u parameter direction is less than the specified u tolerance value, and the length of every line segment in normalized projection coordinates in the vparameter direction is less than the specified vtolerance value.

5 DC_ChordalSize This technique tessellates the surface until the length of each line segment (chord) in device coordinates in the u parameter and the length of every line segment in device coordinates in

6 WCS_PlanarDev This technique tessellates the surface into facets. The technique subdivides the surface until the absolute value of the maximum deviation, in world coordinates, between any facet and the surface is less than u_tolerance.

7 NPC_PlanarDev This technique tessellates the surface into facets. The maximum deviation, in normalized projection coordinates, between any facet and the surface is less than u_tolerance.

8 DC_PlanarDev This technique tessellates the surface into facets. The maximum deviation, in device coordinates, between any facet and

9 WCS_Relative This technique maintains a relative level of quality based on the specified u_tolerance value independent of scaling in world coordinates. u_tolerance must be between 0 and 1 with values closer to 1 specifying a better relative quality.

v_tolerance is not used for this method.

PEX Version 5.1, 31-August-1992

10 NPC_Relative This technique maintains a relative level of quality based on the specified u_tolerance value independent of scaling in normalized projection coordinates. u_tolerance must be between 0 and 1 with values closer to 1 specifying a better relative quality. v_tolerance is not used for this method.

11 DC_Relative This technique maintains a relative level of quality based on the device coordinates. u_tolerance must be between 0 and 1 with values closer to 1 specifying a better relative quality.

v_tolerance is not used for this method.

TrimCurveApproxMethod

The trim curve approximation method specifies the method that is to be used for trim curves when rendering non-uniform rational B-spline (NURB) surface primitives with trim curves. The registered values are:

1 (imp. dep.) This value for TrimCurveApproxMethodis supported on every implementation, but may differ from one to the next.

It may have the same mnemonic and definition as one of the other types, or it may be a method that is not in the list of registered types.

2 ConstantBetweenKnots This technique tessellates the trim curve with equal parametric increments between successive pairs of knots. The tolerance value controls tesselation of the trim curve. If the tolerance value is not an integer value, it is truncated and only the integer portion will be used. If tolerance is less than or equal to zero, the trim curve will be evaluated only at the parameter limits, and at the knots that are within the specified parameter range. If tolerance is greater than zero, the trim curve will be evaluated at the parameter limits, at the knots that are within the specified parameter range, and at the number of positions specified by tolerance between each pair of knots.

ModelClipOperator

The model clip operator defines the operation that is to be used to combine the specified halfspaces with the current composite modeling clipping volume. The registered values are:

1 Replace The specified halfspaces are used to create a new composite modeling clipping volume that replaces the current composite modeling clipping volume.

2 Intersection The specified halfspaces are intersected with the current composite modeling clipping volume to compute a new composite

LightTypeThe light type defines the characteristics of the light sources that can be used in light source shading computations. The registered values are:

PEX Version 5.1, 31-August-1992

1 Ambient A light source that affects all surface primitives uniformly.

Ambient light sources have only a color attribute.

2 WCS_Vector A light source that is specified in world coordinates with a color and a direction vector.

3 WCS_Point A light source that is specified in world coordinates with a color, a position, and two attenuation coefficients.

4 WCS_Spot A light source that is specified in world coordinates with a color, a position, a direction vector, a concentration exponent, two attenuation coefficients and a spread angle.

ColorTypeThe color type defines the format of color values. The registered values are:

0 Indexed A color that is passed as an unsigned 16-bit integer (i.e., it is of type TABLE_INDEX). The integer value is used as an index into a color lookup table. Dereferencing of an indexed color value occurs at the time of rendering, at the time when the actual color value is needed for rendering an output primitive.

1 RGBFloat A color that is passed as three floating point values, in the order red [0-1], green [0-1], blue [0-1]. A color in this format has a type defined by:

COLOR_RGB_FLOAT: [r, g, b : FLOAT]

2 CIEFloat A color that is passed as three floating point values, in the order u [0-1], v [0-1] (CIELUV diagram coefficients), and luminance [0-1]. A color in this format has a type defined by:

COLOR_CIE_FLOAT: [u, v, luminance : FLOAT]

3 HSVFloat A color that is passed as three floating point values, in the order hue [0-1] (angle in fractions of a circle, with red being zero), saturation [0-1], and value [0-1]. A color in this format has a type defined by:

COLOR_HSV_FLOAT: [hue, saturation, value : FLOAT]

4 HLSFloat A color that is passed as three floating point values, red being zero), lightness [0-1], and saturation [0-1].

A color in this format has a type defined by:

COLOR_HLS_FLOAT: [hue, lightness, saturation : FLOAT]

5 RGBInt8 A color that is passed as a unit of four bytes, in the order red, green, blue. A color in this format has a type defined by:

COLOR_RGB_INT8: [r, g, b, pad : CARD8]

6 RGBInt16 A color that is passed as a unit of eight bytes, in the order red, green, blue. A color in this format has a type defined by:

COLOR_RGB_INT16: [r, g, b, pad : CARD16]

PEX Version 5.1, 31-August-1992

FloatFormat

The floating point format defines the format of floating point values. The registered values are:

1 IEEE_754_32 An IEEE 754 standard 32-bit floating point value.

2 DEC_F_Floating A DEC F-floating value.

3 IEEE_754_64 An IEEE 754 standard 64-bit floating point value.

4 DEC_D_Floating A DEC D-floating value.

HLHSRMode

The HLHSR mode defines the method used to do hidden line/hidden surface removal. The registered values are:

1 Off All output primitives are drawn in the order they are processed. No attempt will be made to remove hidden surfaces.

2 ZBuffer Visibility is resolved at each pixel using a depth-, or z-buffering technique. The z-buffering method and the number of bits of precision in the z values is device-dependent. This technique permits visibility to be computed without an intermediate storage area for transformed data, can be used to incrementally add primitives to an image, and is an HLHSR method which is of linear order.

3 Painters Output primitives are buffered as they are processed.

When an "end rendering" occurs with flush=True, the primitives in the buffer are sorted based on the average depth and rendered back-to-front. This technique is fairly fast for small numbers of primitives, but requires an intermediate storage area. This technique does not guarantee totally correct results, since it fails in cases involving cyclically overlapping or interpenetrating objects, and in other, even simpler, cases.

4 Scanline Output primitives are buffered as they are received.

in the buffer are sorted and visibility is computed in scan line order. This technique can be fairly fast for small numbers of polygons, but uses an intermediate storage area to buffer output primitives and must perform a sorting step.

5 HiddenLineOnly Only visible lines will be drawn. Output primitives may be buffered as they are received. When an "end rendering" occurs with flush=True, the primitives in the buffer are sorted and a hidden line computation is performed.

6 ZBufferId This is the same as ZBuffer,except that the

HLHSR_identifieris used to enable and disable z-buffering during traversal. An HLHSR_idof zero disables z-buffering and an HLHSR_identifier of one enables z-buffering.

PEX Version 5.1, 31-August-1992

PickDeviceType

The pick device type specifies the type of pick device that is to be used for workstation picking (via a pick device and a pick measure) or renderer picking. If a pick measure is created using one of the registered pick device types then the pick_data_rec component of the pick device descriptor is ignored and the default prompt and echo type is EchoPrimitive. The pick_data_rec component of the pick device descriptor is used in conjunction with non-registered pick device types. The registered values are:

1 DC_HitBox The pick aperature is specified by a pick position and a pick distance, both in device coordinates.

The shape of the hit box (square, circle, etc.) is implementation-dependent. The pick distance defines the half-width or radius of the hit box.

2 NPC_HitVolume The pick aperature is specified by two points that describe a parallelpiped in NPC space.

PickOneMethod

The pick one method specifies the pick criteria that is to be used for renderer pick one traversals. The registered values are:

1 Last The last picked primitive is returned

2 ClosestZ The primitive which has the z value closest to the front clipping plane in the pick aperature is returned. If several primitives are equally close to the front clipping plane then any of these primitives may be returned.

3 VisibleAny Any picked primitive which is visible (after taking the current

HLHSR mode into account) may be returned.

4 VisibleClosest The primitive which is both visible (after taking the current

HLHSR mode into account) and closest to the pick position is returned.

The algorithm for determining which primitive is closest to the pick position is implementation dependent.

PickAllMethod

The pick all method specifies the pick criteria that is to be used for renderer pick all traversals. The

1 All All primitives which are contained in or intersect the pick aperature are returned.

2 Visible Only visible primitives which are contained in or intersect the pick aperature are returned.

PromptEchoType

The prompt echo type defines the method used to do prompting and echoing during picking operations. The registered values are:

1 EchoPrimitive Use an implementation-dependent technique that at least highlights the picked primitive for a short period of time.

PEX Version 5.1, 31-August-1992

2 EchoStructure Echo the contiguous group of primitives with the same pick ID as the picked primitive, or all of the primitives of the structure with the same pick ID as the picked primitive

(the extension is free to implement either semantic for this type).

3 EchoNetwork Echo the entire posted structure network that contains the picked primitive.

DisplayUpdateMode

The display update mode defines the manner in which changes will affect the displayed image. The registered values are:

1 VisualizeEach Visualize each change as it occurs. (PHIGS - ASAP)

2 VisualizeEasy Visualize only the changes that are "easy to do" (PHIGS -

WAIT/UWOR). Things that are "easy to do" are those that have a dynamic modification of IMMor can be updated without a regeneration of the displayed image. The effective result of such an action is equivalent to having performed a regeneration, but without the expense of a complete retraversal and without clearing the display space.

3 VisualizeNone Visualize none of the changes (PHIGS - WAIT/NIVE). The changes are applied, but the image is not regenerated until there is an explicit request to do so.

4 SimulateSome Visualize the easy changes and simulate those changes that can be simulated. (PHIGS - WAIT/UQUM)

5 VisualizeWhenever All changes will eventually be visualized. If regenerations are necessary, they will be performed at the server’s convenience. One regeneration may cause a number of changes to be visualized. The client can issue an update workstation request to guarantee that all changes have been visualized.

(PHIGS - ASTI/NIVE)

It should be noted that implicit image regenerations may be performed when the display update is one of VisualizeEachor VisualizeWhenever. If such a regeneration occurs, the display surface will be cleared and any output that was not generated by traversing the posted structure list (such as output from core X) will be lost. VisualizeEasy,VisualizeNone,and SimulateSomewill not cause implicit regenerations to occur.

ColorApproxType

The color approximation type describes the way that a renderer will transform rendering pipeline color values into displayable pixel values. The registered values are:

1 ColorSpace The rendering pipeline color is converted into a color with three individual color components.

2 ColorRange The rendering pipeline color is converted into a single color index.

This enumerated type allows applications to control whether the color value produced through illumination and depth-cueing computations is transformed into a single value (e.g., for display on an

8-bit pseudo color display) or into three values (e.g., for display on a 24-bit direct color display).

PEX Version 5.1, 31-August-1992

ColorApproxModel

The color approximation model describes the space in which any color filtering or sampling will be performed during the color approximation phase of rendering. The registered values are:

1 RGB red, green, blue

2 CIE CIELUV diagram u, v coordinates plus luminance

3 HSV hue, saturation, value

4 HLS hue, lightness, saturation

5 YIQ (NTSC) luminance (Y), inphase (wideband orange-cyan), and quadrature (narrowband magenta-green)

RenderingColorModel

The rendering color model defines the color model to be used for color interpolation within the rendering pipeline. Reflectance equations should have the appearance of being performed in the color space specified by the rendering color model.

0 (imp. dep.) An implementation-dependent color space

1 RGB red, green, blue color model

2 CIE CIELUV diagram u, v coordinates plus luminance color model

3 HSV hue, saturation, value color model

4 HLS hue, lightness, saturation color model

ParametricSurfaceCharacteristics

1 None No additional surface characteristics beyond the current surface attributes

2 (imp. dep.) An implementation-dependent method that displays the shape of the surface. This method does not distinguish between front and back facing portions of the surface. The appearance of the representation is controlled by the appropriate set of primitive attributes for the representation. It is implementation-dependent how the representation interacts with any interior rendering indicated by the interior attributes. The data record is ignored for this type.

3 IsoparametricCurves Isoparametric curves are drawn on the surface. The data record contains the number of curves to draw in each of the parameter dimensions and their placement. If the placement is Uniform,the specified number of curves are evenly spaced between the parameter limits of the surface; curves are also drawn at the parameter limits. If the placement is NonUniform,the specified number of curves are evenly spaced between each pair of knots; curves are also drawn at the knots. In both cases only the portions of isoparametric curves are drawn that are within the interior of the surface as defined by any trimming curves. This method does not distinguish between front and back facing portions of the surface. The tessellation and appearance of the isoparametric curves are controlled by the surface approximation criteria and the polyline attributes, respectively. The isoparametric curves are drawn in addition to any interior rendering indicated by the interior style or back interior style attributes. Isoparametric curves have higher visual priority than the primitive’s filled or hollow interiors, but lower

PEX Version 5.1, 31-August-1992 priority than the primitive’s edges.

4 MC_LevelCurves Level curves are drawn on the surface. The curves correspond to the intersections of the surface and a finite set of planes perpendicular to a modelling coordinate direction vector. The positions of the planes are specified by a sequence of intersection points along an infinite line defined by a modelling coordinate origin point, P 0, and a direction vector, V→ .

Pi = P 0 + ti V→

The ti are a sequence of parameters specifying the intersection points. They are in the range:

−∞ < ti < ∞

The Pi are the intersection points of the perpendicular planes with the infinite line. P 0 is a specified origin point in modelling coordinates, and V→ is the specified direction vector in modelling coordinates. The i-th plane is perpendicular to the direction vector, V→ , and intersects the infinite line at point Pi . The data record consists of the origin point, P 0; the direction vector,

V→ ; and the list of parameters, ti .

This method does not distinguish between front and back facing portions of the surface. The tessellation and appearance of the level curves are controlled by the surface approximation criteria and the polyline attributes, respectively. The curves are drawn in addition to any interior rendering indicated by the interior style or back interior style attributes. Level curves have higher visual priority than the primitive’s filled or hollow interiors, but lower

5 WC_LevelCurves Level curves are drawn on the surface. The curves correspond point in world coordinates, and V→ is the specified

PEX Version 5.1, 31-August-1992 direction vector in world coordinates. The i-th plane is perpendicular to the direction vector, V→ , and intersects the infinite line at point Pi . The data record consists of the origin point, P 0; the direction vector,

V→ ; and the list of parameters, ti .

This method does not distinguish between front and back facing portions of the surface. The tessellation and appearance of the level curves are controlled by the surface approximation criteria and the polyline attributes, respectively. The curves are drawn in addition to any interior rendering indicated by the interior style or back interior style attributes. Level curves have higher visual priority than the primitive’s filled or hollow interiors, but lower priority than the primitive’s edges.

GDP The GDP type specifies the (2D) Generalized Drawing Primitives (GDPs) that are supported by the

PEX extension implementation. There are currently no registered GDPs.

GDP3The GDP3 type specifies the (3D) Generalized Drawing Primitives (GDP3s) that are supported by the

PEX extension implementation. There are currently no registered GDP3s.

GSE The GSE type specifies the Generalized Structure Elements (GSEs) that are supported by the PEX extension implementation. There are currently no registered GSEs.

EscapeThe Escape type specifies the Escape Requests that are supported by the PEX extension implementation. The registered escapes are described in appendix E, they are:

1 SetEchoColor modify the renderer’s echo color

PEX Version 5.1, 31-August-1992

2.8.3. Get Implementation-Dependent Constants

Name: PEXGetImpDepConstants

Request:fp_format : FLOAT_FORMAT drawable_example : DRAWABLE_ID names : LISTofCONSTANT_NAME

Reply: constants : LISTofVALUE

Errors: Drawable, Match, Value, FloatingPointFormat

Description:This request allows a client to query one or more of the implementation-dependent constants in a PEX server extension. A single CARD32 or FLOAT is returned for each value requested. These values are returned in order, with one return value in constants for each requested value in names. Floating-point values will be returned in the format specified by fp_format. The implementation-dependent constants that are returned are based on the values that would be used for a drawable with the same root and depth as drawable_example.

PEX defines a number of standard constant names that all PEX extensions must be able to return. These standard constant names are 16-bit integers with the high order bit equal to zero. Additional proprietary implementation-dependent constants can be defined and returned by PEX server extensions using 16-bit integers with the high order bit equal to one. The standard constant names consist of:

NominalLineWidth CARD32 Width (in pixels) of "standard" line or curve.

NumSupportedLineWidths CARD32 Number of supported line or curve widths (a value of 0 indicates that all line widths, including fractional widths, between min and max line width are supported).

MinLineWidth CARD32 Width (in pixels) of thinnest line or curve that can be drawn.

MaxLineWidth CARD32 Width (in pixels) of thickest line or curve that can be drawn.

NominalEdgeWidth CARD32 Width (in pixels) of "standard" edge.

NumSupportedEdgeWidths CARD32 Number of supported edge widths (a value of 0 indicates that all edge widths, including fractional widths, between min and max edge width are supported).

MinEdgeWidth CARD32 Width (in pixels) of thinnest edge that can be drawn.

MaxEdgeWidth CARD32 Width (in pixels) of thickest edge that can be drawn.

NominalMarkerSize CARD32 Largest dimension (either height or width, in pixels) of

"standard" marker.

NumSupportedMarkerSizes CARD32 Number of supported marker sizes (a value of 0 indicates that all marker sizes, including fractional values, between min and max marker size are supported).

PEX Version 5.1, 31-August-1992

MinMarkerSize CARD32 Largest dimension (either height or width, in pixels) of smallest marker that may be drawn. (This minimum is exclusive of the marker type Dot which is always drawn as the smallest displayable point).

MaxMarkerSize CARD32 Largest dimension (either height or width, in pixels) of largest marker that may be drawn. (This maximum is exclusive

ChromaticityRedU FLOAT Returns the CIEYUV u chromaticity coefficient for the red channel of the (properly adjusted) display device.

ChromaticityRedV FLOAT Returns the CIEYUV vchromaticity coefficient for the red channel

LuminanceRed FLOAT Returns the CIEYUV luminance value for the red channel of the

(properly adjusted) display device.

ChromaticityGreenU FLOAT Returns the CIEYUV u chromaticity coefficient for the green channel

ChromaticityGreenV FLOAT Returns the CIEYUV vchromaticity coefficient for the green channel

LuminanceGreen FLOAT Returns the CIEYUV luminance value for the green channel of the

ChromaticityBlueU FLOAT Returns the CIEYUV u chromaticity coefficient for the blue channel

ChromaticityBlueV FLOAT Returns the CIEYUV vchromaticity coefficient for the blue channel

LuminanceBlue FLOAT Returns the CIEYUV luminance value for the blue channel of the

ChromaticityWhiteU FLOAT Returns the CIEYUV u chromaticity coefficient for the reference white of the (properly adjusted) display device.

ChromaticityWhiteV FLOAT Returns the CIEYUV vchromaticity coefficient for the reference

LuminanceWhite FLOAT Returns the CIEYUV luminance value for the reference white of the

MaxNamesetNames CARD32 Maximum number of names allowed in a name set.

The names are between zero and (MaxNamesetNames- 1)

MaxModelClipPlanes CARD32 Maximum number of modeling clipping planes that may be defined.

TransparencySupported CARD32 Returns True or False, depending on whether the transmission coefficient is utilized in the light source shading computations.

PEX Version 5.1, 31-August-1992

DitheringSupported CARD32 Returns True or False, depending on whether the dithering hint actually causes dithering to occur.

MaxNonAmbientLights CARD32 Maximum number of non-ambient light sources that may be enabled at one time.

MaxNURBOrder CARD32 Maximum non-uniform rational B-spline order supported.

MaxTrimCurveOrder CARD32 Maximum order for trim curves.

BestColorApproxValues CARD32 Returns the constant ColorApproxPowersOf2 to indicate whether it is a significant performance win if the color approximation multiplier values are powers of two so that pixels can be composed using shifts and adds, or ColorApproxAnyValues if it makes little or no difference.

DoubleBufferingSupported CARD32 Returns True or False depending on whether or not the server supports double-buffering.

MaxHitsEventSupported CARD32 Returns True or False, depending on whether the

MaxHitsReachedevent is supported.

PEX Version 5.1, 31-August-1992

2.8.4. Match Renderer Targets

Name: PEXMatchRendererTargets

Request:drawable_id : DRAWABLE_ID depth : CARD8 type: MATCH_DRAW_TYPE visual : VISUAL_ID max_targets : CARD32

Reply: targets : LISTofRENDERER_TARGETS

Errors: Drawable, Value

Description:This returns information about the visual, depth and drawables the server can support. drawable_id tells the server which screen the client is interested in and, depth, visual and typespecify which data is of interest.

Wildcarding can be accomplished by specifying zero for the depth, zero for the visual and DontCare for the type.This matches all depths, visuals and/or drawable types. max_targets is the maximum number of targets the client wants returned.

2.8.5. Escape

Name: PEXEscape

Request:escape_id : CARD32 escape_data : LISTofCARD8

Errors: Value, escape-specific

Description:This request can be used to send registered PEX escapes or vendor-specific escapes that do not generate a reply. Registered escapes are defined in Appendix E. For registered escapes, escape_id is a positive number. For vendor-specific escapes the escape_id is encoded as follows: the high bit is set, the next 15 bits contain the vendor_id and the low-order 16 bits contain the vendor-specific request_id. vendor_id is a unique number, assigned on request by the MIT registry, that identifies the vendor. The supported escapes can be determined using PEXGetEnumeratedTypeInfo.

For vendor-specific escapes, it is up to the vendor to specify how escape_data is encoded. For example, one vendor may choose to always pass a floating point format as the first value in escape_data while another may choose to pass a sub-request number. As with all X requests, this request must be a multiple of 4 bytes.

If the escape_id is not recognized by the server, or if the escape_id refers to an escape that generates a reply, a Value error will be generated. All other errors returned by this request are escape-specific. This request will not generate any new events or errors. The X extension mechanism must be used for vendor-

PEX Version 5.1, 31-August-1992 specific requests that generate new events or new errors.

2.8.6. Escape With Reply

Name: PEXEscapeWithReply

Request:escape_id : CARD32 escape_data : LISTofCARD8

Reply: escape_id : CARD32 escape_reply_data : LISTofCARD8

Errors: Value, escape-specific

Description:This request can be used to send registered PEX escapes or vendor-specific escapes that generate a reply.

The supported escapes can be determined using PEXGetEnumeratedTypeInfo. At this point in time there are no registered escapes that have replies.

For vendor-specific escapes, it is up to the vendor to specify how escape_data and escape_reply_data are encoded. The vendor should define encodings which follow the conventions in the encoding document.

The encoding of escape_id is described in PEXEscape. If the escape_id is not recognized by the server, or if the escape_id refers to an escape that does not generate a reply, a Value error will be generated. All other errors returned by this request are escape-specific. This request will not generate any new events or errors.

The X extension mechanism must be used for vendor-specific requests that generate new events or new errors. PEX Version 5.1, 31-August-1992

3. Output Commands

______________________________________________________________________________________________ This section defines output commands. Output commands are commands that are capable of being processed by a renderer or stored as structure elements. The format of each of the commands is listed below. Output commands may be passed to the server to be processed immediately by a renderer with the PEXRenderOutputCommands request. Output commands may be passed to the server to be stored in a structure with the PEXStoreElements request. Output commands may be retrieved by a client from a structure resource with the PEXFetchElements request.

Output commands are always executed in exactly the same fashion, no matter whether they are processed immediately by a renderer or processed as part of a structure traversal. When sent to the server via a

PEXRenderOutputCommands request, output commands are processed until one is found to be in error, or until the entire list has been processed. If an output command is discovered to contain an error, it is discarded, as are all others following it in the list of output commands and an OutputCommanderror is returned to the client. Similarly, if a PEXStoreElements command is used to transmit a list of output commands to the server, the first erroneous output command and all output commands following it in the list will be discarded, and an OutputCommanderror will be reported to the client. Thus it is not possible for a structure resource to contain any elements with illegal or inappropriate values.

OutputCommanderrors are only generated by the PEXRenderOutputCommands or PEXStoreElements requests.

The error checking performed for these two types of requests is identical. When output commands are processed by a renderer, attribute specifications that are not supported by the server, out-of-range table indices, or undefined table indices are mapped to their default values; no errors will be reported.

3.1. Data Formats

Each of the requests listed above takes a format parameter of type FLOAT_FORMAT. For those requests sending data from the client to the server, this format word is used to indicate to the server the format of any floating point values that are contained in the request. For those requests requiring data to be sent back to the client, the format is used to indicate to the server how it should format the floating point data in the reply sent back to the client.

Color values are typically passed as a color type and a value. The color type specifies whether the color is an index value or a direct color value of some type. In the case of the "with data" output primitives (which may contain many color values), the color type is specified just once and all of the color values in the output command must be of the indicated color type. PEX servers are required to be able to deal with indexed colors and at least one type of direct color. Indexed colors are specified using an index which is used to obtain the color from a color lookup table.

Direct colors are specified directly as RGB, HSV, HLS, or CIELUV color values of some form. The list of registered direct color formats can be found in the "Extension Information" section. PEX servers are free to store direct color values in whatever implementation-dependent format they choose, but they must be capable of converting those values back into the originally-specified color type when queried by the client.

3.2. Errors

Errors that can be reported when passing a list of output commands to a PEX server are described in the following sections. Specific errors that the PEX server checks for when storing or processing a particular type of output command are explained in the "Output Command Descriptions" section.

3.2.1. FloatingPointFormat Errors

The floating point format is specified once in each PEXStoreElements or PEXRenderOutputCommands request.

If the request specifies a floating point format that is not supported by the PEX server, a FloatingPointFormat error

PEX Version 5.1, 31-August-1992 is reported and none of the output commands are processed, even if they do not contain floating point values. All output commands in the list are ignored.

3.2.2. ColorType Errors

The color type is generally specified with each color or, in some cases, once per output command. If an output command specifies a color type that is not supported by the PEX server, an OutputCommanderror is reported. All previous output commands in the list are processed, and the output command containing the unsupported color type and any subsequent output commands are ignored.

3.2.3. Length Errors

If an output command exceeds the length of the output command list, processing of the list stops and an

OutputCommanderror is reported. All previous output commands in the list are processed, and the output command that exceeds the request length and any subsequent output commands are ignored.

3.2.4. OutputCommand Errors

If an illegal value is specified in an output command, all processing of the list stops and an OutputCommanderror is reported. All previous output commands in the list are processed, and the output command that contains the illegal value and any subsequent output commands are ignored.

Not all unsupported values are illegal. Some enumerated types allow for implementation dependent values (for example, negative line types). In general, output commands that contain these types can have arbitrary values specified. When the output command is rendered, values that are not supported by the PEX server are rendered with a default value and do not report errors.

A second category of enumerated types have a fixed set of legal values which are all required to be implemented by a conforming PEX server and cannot be inquired (for example, text path). If the PEX server finds a value outside the range of legal values, an OutputCommanderror is reported, as described above.

A third category of enumerated types have a fixed set of legal values, but they are not all required to be implemented by a PEX server. Values supported by the PEX server can be inquired (for example, interior style). When the output command is rendered, values that are not supported by the PEX server are rendered with a default value and do not report errors.

If an output command contains a bitmask value, the PEX server must return an OutputCommanderror if any undefined bits are set. Usually, these errors are not specifically mentioned in the output command descriptions below.

The client is not required to pass unit length normal vectors to the PEX server in output commands. The effect of rendering output primitives with normal vectors that are not unit length is implementation dependent.

3.3. Output Command Descriptions

The list below describes the format of the output commands that are supported. Each output command is a structure of type OUTPUT_COMMAND, which contains a 16-bit opcode that uniquely defines the output command (as well as uniquely identifying the structure element if the command is stored in a structure), a 16-bit size field which specifies the length of the output command in units of four bytes, and the data needed to specify the output command. The high-order bit of the opcode field is reserved to indicate whether the output command is one of the standard PEX output commands (high-order bit equals zero) or a non-standard or proprietary output command

(high-order bit equals one). PEX Version 5.1, 31-August-1992

Marker type marker_type : MARKER_TYPE

When processed by a renderer, this command will modify the renderer’s marker_type attribute. If the specified marker type is not supported by the PEX server, marker type 3 (MarkerAsterisk)is used.

Any integer value may be specified as the marker type in this output command.

Marker scale scale : FLOAT

When processed by a renderer, this command will modify the renderer’s marker_scale attribute. The specified scale is multiplied by the nominal marker size (see PEXGetImpDepConstants) and the result is mapped to the nearest marker size supported by the server.

Marker color index color : TABLE_INDEX

When processed by a renderer, this command will modify the renderer’s marker_color attribute, setting the color type to Indexedand the color value to the index specified by color. If the specified color index is not defined, color index one is used. If color index one is not defined, the default values listed in Appendix D are used.

An OutputCommanderror is reported if the color index in this output command is 65535.

Marker color color : COLOR_SPECIFIER color type and value as specified. If the color type is Indexedand the specified color index is not defined, color index one is used. If color index one is not defined, the default values listed in Appendix D are used.

An OutputCommanderror is reported if the color type is Indexedand the color index is 65535.

Marker bundle index index: TABLE_INDEX

When processed by a renderer, this command will modify the renderer’s marker_bundle_index attribute. If an undefined marker bundle index is specified by this output command, then default bundle index one is used. If table index one is not defined, the default values listed in Appendix D are used.

An OutputCommanderror is reported if the bundle index in this output command is zero.

Text font index

When processed by a renderer, this command will modify the renderer’s text_font_indexattribute. The text_font_indexselects which entry in the text font table (i.e., which font group) will be used to render text primitives. If an undefined text font index is specified by this output command, the default index one is used.

If table index one is not defined, the default values listed in Appendix D are used.

An OutputCommanderror is reported if the text font index in this output command is zero.

Text precision precision : TEXT_PRECISION

When processed by a renderer, this command will modify the renderer’s text_precision attribute.

When a text or annotation text output primitive is interpreted, all of the ISTRING fragments in the text string are rendered in the same text precision. That is, if the font group selected by the current text font index

PEX Version 5.1, 31-August-1992 consists of both X and PEX fonts, and if some of the ISTRING fragments in the string are rendered in X fonts, the text precision of the entire string must be dropped to at least Char precision.

If a char_set value is not available in the current font group, then the entire string is rendered using the default font group. If a char_set value is not available in the default font group, then that portion of the string is rendered in an implemenation dependent manner.

Character expansion expansion : FLOAT

When processed by a renderer, this command will modify the renderer’s char_expansion attribute. Only the magnitude of the specified expansion is considered. The specified expansion is compared to the minimum and maximum character expansion factors. These values depend on the font files that are in the font groups in the selected font table entry, which in turn depend on which X or PEX font files the client opened. For example, if the client opens all PEX font files (that is, all scalable and rotatable stroke fonts), then a continuous number of expansions are supported. If the expansion is smaller than the minimum character expansion factor, the minimum value is used. If the expansion is larger than the maximum character expansion factor, the maximum value is used.

Character spacing spacing : FLOAT

When processed by a renderer, this command will modify the renderer’s char_spacing attribute.

No errors or defaults are defined.

Text color index color : TABLE_INDEX

When processed by a renderer, this command will modify the renderer’s text_color attribute, setting the color type to Indexedand the color value to the index specified by color. If the specified color index is not defined, color index one is used. If color index one is not defined, the default values listed in Appendix D are used.

An OutputCommanderror is reported if the color index in this output command is 65535.

Text colorcolor : COLOR_SPECIFIER type and value as specified. If the color type is Indexedand the specified color index is not defined, color index one is used. If color index one is not defined, the default values listed in Appendix D are used.

An OutputCommanderror is reported if the color type is Indexedand the color index is 65535.

Character height height : FLOAT

When processed by a renderer, this command will modify the renderer’s char_height attribute. If the specified height or the computed width is not supported, the height or width is mapped to the nearest character height or width supported. These values depend on the font files that are in the font groups in the selected font table entry, which in turn depend on which X or PEX font files the client opened. For example, if the client opens all PEX font files (that is, all scalable and rotatable stroke fonts), then a continuous number of character sizes are supported.

Character up vector up : VECTOR_2D

When processed by a renderer, this command will modify the renderer’s char_up_vector attribute. If the character up vector is degenerate (it has a length of zero), the value <0, 1> is used.

PEX Version 5.1, 31-August-1992

Text pathpath : TEXT_PATH

When processed by a renderer, this command will modify the renderer’s text_path attribute.

An OutputCommanderror is reported if the path is not PathRight, PathLeft, PathUp, or PathDown.

Text alignment alignment : TEXT_ALIGNMENT

When processed by a renderer, this command will modify the renderer’s text_alignmentattribute.

An OutputCommanderror is reported if the horizontal alignment is not HalignNormal, HalignLeft,

HalignCenter, or HalignRight, or if the vertical alignment is not ValignNormal, ValignTop,ValignCap,

ValignHalf, ValignBase,or ValignBottom.

Annotation text height height : FLOAT

When processed by a renderer, this command will modify the renderer’s atext_height attribute. If the specified height or the computed width is not supported, the height or width is mapped to the nearest annotation character height or width supported. These values depend on the font files that are in the font groups in the selected font table entry, which in turn depend on which X or PEX font files the client opened.

For example, if the client opens all PEX font files (that is, all scalable and rotatable stroke fonts), then a continuous number of character sizes are supported.

Annotation text up vector up : VECTOR_2D

When processed by a renderer, this command will modify the renderer’s atext_up_vector attribute. If the annotation text up vector is degenerate (it has a length of zero), the value <0, 1> is used.

Annotation text path path : TEXT_PATH

When processed by a renderer, this command will modify the renderer’s atext_path attribute.

Annotation text alignment

When processed by a renderer, this command will modify the renderer’s atext_alignment attribute.

Annotation text style index: ATEXT_STYLE

When processed by a renderer, this command will modify the renderer’s atext_styleattribute. If the specified style is not supported by the PEX server, annotation style 1 (ATextNotConnected)is used.

Any integer value may be specified as the style in this output command.

Text bundle index index: TABLE_INDEX

When processed by a renderer, this command will modify the renderer’s text_bundle_indexattribute. If an undefined text bundle index is specified by this output command, then default bundle index one is used. If

PEX Version 5.1, 31-August-1992 table index one is not defined, the default values listed in Appendix D are used.

An OutputCommanderror is reported if the bundle index in this output command is zero.

Line typeline_type: LINE_TYPE

When processed by a renderer, this command will modify the renderer’s line_typeattribute. If the specified line type is not supported by the PEX server, line type 1 (LineTypeSolid)is used.

Any integer value may be specified as the line type in this output command.

Line widthwidth : FLOAT

When processed by a renderer, this command will modify the renderer’s line_width attribute. The specified line width is multiplied by the nominal line width (see PEXGetImpDepConstants). The result is mapped to the nearest line width supported by the server.

Line color index color : TABLE_INDEX

When processed by a renderer, this command will modify the renderer’s line_color attribute, setting the color type to Indexedand the color value to the index specified by color. If the specified color index is not defined, color index one is used. If color index one is not defined, the default values listed in Appendix D are used.

An OutputCommanderror is reported if the color index in this output command is 65535.

Line colorcolor : COLOR_SPECIFIER type and value as specified. If the color type is Indexedand the specified color index is not defined, color index one is used. If color index one is not defined, the default values listed in Appendix D are used.

An OutputCommanderror is reported if the color type is Indexedand the color index is 65535.

Curve approximation approx : CURVE_APPROX

When processed by a renderer, this command will modify the renderer’s curve_approx attribute. If the specified method is not supported by the PEX server, method 1 (implementation dependent) is used.

Any integer value may be specified as the curve approximation method in this output command.

Polyline interpolation method polyline_interp : POLYLINE_INTERP

When processed by a renderer, this command will modify the renderer’s polyline_interp attribute. If the specified interpolation method is not supported by the PEX server, method 1 (PolylineInterpNone) is used.

Any integer value may be specified as the interpolation method in this output command.

Line bundle index index: TABLE_INDEX

When processed by a renderer, this command will modify the renderer’s line_bundle_indexattribute. If an undefined line bundle index is specified by this output command, then default bundle index one is used. If

PEX Version 5.1, 31-August-1992

Surface interior style interior_style : INTERIOR_STYLE

When processed by a renderer, this command will modify the renderer’s interior_style attribute. If the specified style is not supported, style 1 (InteriorStyleHollow)is used.

An OutputCommanderror is reported if the style is not InteriorStyleHollow,InteriorStyleSolid,

InteriorStylePattern, InteriorStyleHatch, or InteriorStyleEmpty.

Surface interior style index index: TYPE_OR_TABLE_INDEX

When processed by a renderer, this command will modify the renderer’s interior_style_index attribute. If the current interior_style is InteriorStylePattern or InteriorStyleHatch, the specified index is used to further define the rendering style of surface primitives. For InteriorStylePattern, if the specified pattern table index is not defined, table index one is used.† For InteriorStyleHatch, the index determines the hatch style and may be positive or negative. If the specified hatch style is not supported, style one is used. If hatch style one is not supported, the result is implementation dependent.

Surface color index color : TABLE_INDEX

When processed by a renderer, this command will modify the renderer’s surface_color attribute, setting the color type to Indexedand the color value to the index specified by color. If the specified color index is not defined, color index one is used. If color index one is not defined, the default values listed in Appendix D are used.

An OutputCommanderror is reported if the color index in this output command is 65535.

Surface color color : COLOR_SPECIFIER color type and value as specified. If the color type is Indexedand the specified color index is not defined, color index one is used. If color index one is not defined, the default values listed in Appendix D are used.

An OutputCommanderror is reported if the color type is Indexedand the color index is 65535.

Surface reflection attributes attr : REFLECTION_ATTR

When processed by a renderer, this command will modify the renderer’s reflection_attr attribute.

No errors or defaults are defined.

Surface reflection model reflection_model : REFLECTION_MODEL

When processed by a renderer, this command will modify the renderer’s reflection_model attribute. If the specified reflection model is not supported by the PEX server, method 1 (ReflectionNoShading)is used.

Any integer value may be specified as the reflection model in this output command.

Surface interpolation method surface_interp : SURFACE_INTERP

__________________ † PHIGS requires that the interior style index must be greater than zero for InteriorStylePattern, but this is difficult for PEX to enforce, so a default action is defined instead.PEX Version 5.1, 31-August-1992

When processed by a renderer, this command will modify the renderer’s surface_interp attribute. If the specified interpolation method is not supported by the PEX server, method 1 (SurfaceInterpNone) is used.

Any integer value may be specified as the interpolation method in this output command.

Backface surface interior style interior_style : INTERIOR_STYLE

When processed by a renderer, this command will modify the renderer’s bf_interior_style attribute. If the specified style is not supported, style 1 (InteriorStyleHollow)is used.

An OutputCommanderror is reported if the style is not InteriorStyleHollow,InteriorStyleSolid,

InteriorStylePattern, InteriorStyleHatch, or InteriorStyleEmpty.

Backface surface interior style index index: TYPE_OR_TABLE_INDEX

When processed by a renderer, this command will modify the renderer’s bf_interior_style_indexattribute. If the current bf_interior_style is InteriorStylePattern or InteriorStyleHatch, the specified index is used to further define the rendering style of backfacing surface primitives. For InteriorStylePattern, if the specified pattern table index is not defined, table index one is used.‡ For InteriorStyleHatch, the index determines the hatch style and may be positive or negative. If the specified hatch style is not supported, style one is used. If hatch style one is not supported, the result is implementation dependent.

Backface surface color index color : TABLE_INDEX

When processed by a renderer, this command will modify the renderer’s bf_surface_color attribute, setting the color type to Indexedand the color value to the index specified by color. If the specified color index is not defined, color index one is used. If color index one is not defined, the default values listed in Appendix D are used.

An OutputCommanderror is reported if the color index in this output command is 65535.

Backface surface color color : COLOR_SPECIFIER color type and value as specified. If the color type is Indexedand the specified color index is not defined, color index one is used. If color index one is not defined, the default values listed in Appendix D are used.

An OutputCommanderror is reported if the color type is Indexedand the color index is 65535.

Backface surface reflection attributes attr : REFLECTION_ATTR

When processed by a renderer, this command will modify the renderer’s bf_reflection_attr attribute.

No errors or default are defined.

Backface surface reflection model reflection_model : REFLECTION_MODEL

When processed by a renderer, this command will modify the renderer’s bf_reflection_modelattribute. If the specified reflection model is not supported by the PEX server, method 1 (ReflectionNoShading)is used.

__________________ ‡ PHIGS requires that the backface interior style index must be greater than zero for InteriorStylePattern, but this is difficult for PEX to enforce, so a default action is defined instead.PEX Version 5.1, 31-August-1992

Any integer value may be specified as the reflection model in this output command.

Backface surface interpolation method surface_interp : SURFACE_INTERP

When processed by a renderer, this command will modify the renderer’s bf_surface_interp attribute. If the specified interpolation method is not supported by the PEX server, method 1 (SurfaceInterpNone) is used.

Any integer value may be specified as the interpolation method in this output command.

Surface approximation approx : SURFACE_APPROX

When processed by a renderer, this command will modify the renderer’s surface_approx attribute. If the specified method is not supported by the PEX server, method 1 (implementation dependent) is used.

Any integer value may be specified as the surface approximation method in this output command.

Facet culling mode culling_mode: CULL_MODE

When processed by a renderer, this command will modify the renderer’s culling_modeattribute.

An OutputCommanderror is reported if the mode is not None,BackFaces, or FrontFaces.

Facet distinguish flag distinguish : BOOLEAN

When processed by a renderer, this command will modify the renderer’s distinguish attribute.

An OutputCommanderror is reported if the mode is not True or False.

Pattern size size: VECTOR_2D

When processed by a renderer, this command will modify the renderer’s pattern_size attribute. Only the magnitudes of the specified pattern size components are considered. If the current interior_style is

InteriorStylePattern, the specified pattern size components are used. If either component is zero, the output command is ignored.

Pattern reference point point : COORD_2D

When processed by a renderer, this command will modify the renderer’s pattern_ref_pt, pattern_ref_vec1, and pattern_ref_vec2 attributes. The zcoordinate of the reference point will be set to zero, pattern_ref_vec1 will be set to <1,0,0>, and pattern_ref_vec2 will be set to <0,1,0>.

No errors or defaults are defined.

Pattern reference point and vectors ref_pt : COORD_3D vector1 : VECTOR_3D vector2 : VECTOR_3D pattern_ref_vec2 attributes. If the pattern vectors define a degenerate case (that is, if one of the vectors is zero length or if the vectors are parallel), the output command is ignored.

Interior bundle index index: TABLE_INDEX PEX Version 5.1, 31-August-1992

When processed by a renderer, this command will modify the renderer’s interior_bundle_index attribute. If an undefined interior bundle index is specified by this output command, then default bundle index one is used. If table index one is not defined, the default values listed in Appendix D are used.

An OutputCommanderror is reported if the bundle index in this output command is zero.

Surface edge flag onoff: SWITCH

When processed by a renderer, this command will modify the renderer’s surface_edges attribute.

An OutputCommanderror is reported if the flag is not On or Off.

Surface edge type edge_type: SURFACE_EDGE_TYPE

When processed by a renderer, this command will modify the renderer’s surface_edge_type attribute. If the specified edge type is not supported by the PEX server, edge type 1 (SurfaceEdgeSolid)is used.

Any integer value may be specified as the edge type in this output command.

Surface edge width width : FLOAT

When processed by a renderer, this command will modify the renderer’s surface_edge_width attribute. The specified edge width is multiplied by the nominal edge width (see PEXGetImpDepConstants). The result is mapped to the nearest edge width supported by the PEX server.

Surface edge color index color : TABLE_INDEX

When processed by a renderer, this command will modify the renderer’s surface_edge_color attribute, setting the color type to Indexedand the color value to the index specified by color. If the specified color index is not defined, color index one is used. If color index one is not defined, the default values listed in Appendix D are used.

An OutputCommanderror is reported if the color index in this output command is 65535.

Surface edge color color : COLOR_SPECIFIER the color type and value as specified. If the color type is Indexedand the specified color index is not defined, color index one is used. If color index one is not defined, the default values listed in Appendix D are used.

An OutputCommanderror is reported if the color type is Indexedand the color index is 65535.

Edge bundle index index: TABLE_INDEX

When processed by a renderer, this command will modify the renderer’s edge_bundle_indexattribute. If an undefined edge bundle index is specified by this output command, then default bundle index one is used. If

Set individual ASF attribute : ASF_ATTRIBUTE source : ASF_VALUE PEX Version 5.1, 31-August-1992

When processed by a renderer, this command will modify the specified ASF (aspect source flag) attribute in the renderer. Depending on the value of attribute, one of the following rendering pipeline attributes will be modified:

marker_type_asf interior_style_asf marker_scale_asf interior_style_index_asf marker_color_asf surface_color_asf text_font_index_asf surface_interp_asf text_prec_asf reflection_model_asf char_expansion_asf reflection_attr_asf char_spacing_asf bf_interior_style_asf text_color_asf bf_interior_style_index_asf line_type_asf bf_surface_color_asf line_width_asf bf_surface_interp_asf line_color_asf bf_reflection_model_asf curve_approx_asf bf_reflection_attr_asf polyline_interp_asf surface_approx_asf surface_edges_asf surface_edge_type_asf surface_edge_width_asf surface_edge_color_asf

An OutputCommanderror is reported if attribute does not refer to a valid ASF attribute or if source is not set to Bundledor Individual.

Local transform 3D comp_type: COMPOSITION matrix : MATRIX

When processed by a renderer, this command will modify the renderer’s local_transform attribute. If comp_typeis PreConcatenate, the specified matrix is pre-concatenated to the local model transformation matrix. If comp_typeis PostConcatentate, the specified matrix is post-concatenated to the local modeling transform. If comp_typeis Replace, the specified matrix replaces the local modeling transform.

An OuputCommanderror is reported if the composition type is not PreConcatenate, PostConcatenate or

Replace.

Local transform 2D matrix : MATRIX_3X3

When processed by a renderer, this command will modify the renderer’s local_transform attribute. This command is identical to local transform 3D except that the specified matrix is a 3 × 3 matrix instead of a 4 × 4 matrix. Before the concatenation occurs, the 3 × 3 matrix represented by

� gda heb jfc � will be expanded to a 4 × 4 matrix as follows:� gda heb jfc �→ � g0da h0eb 010 j0fc �

An OutputCommanderror is reported if the composition type is not PreConcatenate, PostConcatenate or

Replace. PEX Version 5.1, 31-August-1992

Global transform 3D matrix : MATRIX

When processed by a renderer, this command will replace the renderer’s global_transform attribute.

No errors or defaults are defined.

Global transform 2D matrix : MATRIX_3X3

When processed by a renderer, this command will replace the renderer’s global_transform attribute. This command is identical to "Global transform 3D" except that the specified matrix is a 3 × 3 matrix instead of a 4

× 4 matrix. Before the replacement occurs, the 3 × 3 matrix represented by

� gda heb jfc � will be expanded to a 4 × 4 matrix as follows:� gda heb jfc �→ � g0da h0eb 010 j0fc �

Model clipclip_switch: CLIP_INDICATOR

When processed by a renderer, this command will modify the renderer’s model_clipattribute.

An OutputCommanderror is reported if the model clip indicator is not Clip or NoClip.

Set model clip volume 3D operator : OPERATOR halfspaces : LISTofHALFSPACE

When processed by a renderer, this command will modify the renderer’s model_clip_volumeattribute. Each halfspace is defined by a point in modeling coordinates and a vector defining the normal to the plane which is the boundary of the half space. The normal points in the direction of the halfspace, and the point is considered to be on the plane.

Each half-space is transformed by the current composite modeling transformation and combined with the current model clipping volume using the operater specified by operator. The model clip volume which results is not affected by subsequent changes to the composite modeling transformation. If the specified operator is not supported by the PEX server or if any halfspace is degenerate, the output command is ignored.

Set model clip volume 2D halfspaces : LISTofHALFSPACE_2D to be on the plane. The z component of each point and vector are assumed to be zero.

PEX Version 5.1, 31-August-1992 not supported by the PEX server or if any halfspace is degenerate, the output command is ignored.

Restore model clip volume

When processed by a renderer, this command will modify the renderer’s model_clip_volumeattribute. The modeling clipping volume will be restored to its state as of the last structure invocation, or to the default state if no structure was invoked.

No errors or defaults are defined.

View indexindex: TABLE_INDEX

When processed by a renderer, this command will modify the renderer’s view_indexattribute. If the specified view index is not defined, index zero is used. If view index zero is not defined, the default values listed in

Appendix D are used.

An OutputCommanderror is reported if the index is 65535.

Light source state enable : LISTofCARD16 disable : LISTofCARD16

When processed by a renderer, this command will modify the renderer’s light_state attribute. The current light_state is modified by activating ("turning on") each light source whose index is specified in the enable list, and by deactivating ("turning off") each light source whose index is specified in the disable list. If any light in the enable or disable list references an undefined Light table entry, the light is ignored.

An OutputCommanderror is reported if a light in either the enable or disable list is zero, or if the same light is specified in both the lists.

Depth cue index index: TABLE_INDEX

When processed by a renderer, this command will modify the renderer’s depth_cue_indexattribute. If the specified depth cue index is not defined, index zero is used. If depth cue index zero is not defined, the default values listed in Appendix D are used.

Pick IDpickid: CARD32

When processed by a renderer, this command will modify the renderer’s pick_idattribute.

HLHSR identifier id : CARD32

When processed by a renderer, this command will modify the renderer’s HLHSR_identifierattribute. This output command is a noop for all registered HLHSR modes except ZBufferId. If the renderer’s HLHSR_mode is set to ZBufferIdthen a zero value will disable z-buffering and a value of one will enable it. For nonregistered HLHSR modes the effect of this command is implementation dependent. If the specified HLHSR identifier is not supported by the PEX server, the HLHSR identifier used is implementation dependent.

Color approximation index

When processed by a renderer, this command will modify the renderer’s color_approx_index attribute. If the specified color approximation index is not defined, index zero is used. If index zero is not defined, the default

PEX Version 5.1, 31-August-1992 values listed in Appendix D are used.

An OutputCommanderror is reported if the index is 65535.

Rendering color model model: COLOR_MODEL

When processed by a renderer, this command will modify the renderer’s rdr_color_model attribute. If the specified color model is not supported by the PEX server, model 0 (implementation dependent) is used.

Any integer value may be specified as the color model in this output command.

Parametric surface characteristics psc : PSURF_CHAR

When processed by a renderer, this command will modify the renderer’s psurf_char attribute. If the specified type is not supported by the PEX server, type 1 (None)is used.

Any integer value may be specified as the characteristics type in this output command. If an inconsistent value is specified in the data record, an OutputCommanderror is reported. (For example, if the type is

IsoparametricCurves and the curve placement is not Uniformor NonUniform,or if the type is

MC_LevelCurvesor WC_LevelCurvesand the direction vector has zero length.)

Add names to name set names : LISTofNAME

When processed by a renderer, this command will add names to the renderer’s name set. If any name in the set of normal or inverted name set names is outside the supported range (see PEXGetImpDepConstants), that name is ignored.†

Remove names from name set

When processed by a renderer, this command will remove names from the renderer’s name set. If any name in the set of normal or inverted name set names is outside the supported range (see PEXGetImpDepConstants), that name is ignored.‡

Execute structure s_id : STRUCTURE_ID

When processed by a renderer, this output command transfers flow-of-control to the specified structure.

Processing of output commands will then commence with the first structure element in the structure specified by s_id. When all of the elements in the called structure have been processed, control will be returned. When this command is executed, all of the rendering pipeline attribute values in the renderer are saved. Then, the current global modeling transform is set to the current composite modeling transform and the current local modeling matrix is set to the identity matrix. When control is returned, the saved rendering pipeline attribute values are restored.

If s_id references a non-existent structure, an OutputCommanderror is reported.* Note that it is not possible to have traversal time errors due to non-existent structures, since PEXDestroyStructures removes all references to structures it deletes.

Label label : INT32

__________________ † PHIGS defines no errors for Add Names To Set.

‡ PHIGS defines no errors for Remove Names From Set.

* PHIGS specifies that if the specified structure is non-existent, a new empty structure is created. In PEX, it is the client’s responsibility to ensure that references to non-existent structure resource identifiers do not occur.

PEX Version 5.1, 31-August-1992

When processed by a renderer, this output command is a no-op. Its main usefulness is when used as a structure element to maintain the specified label as an aid to navigation during structure editing.

No errors or defaults are defined.

Application data data : LISTofCARD8 structure element in order to maintain the specified client application data.

No errors or defaults are defined. Note that byte-swapping and floating point conversion are not done on this type of output command.

GSE id : INT32

When processed by a renderer, the effect of this command is implementation-dependent. Because of floating point and color format discrepancies across a network interface, it is not anticipated that the GSE will provide a useful extension mechanism, but it is provided for PHIGS compatibility purposes. If the specified GSE identifier is not supported by the PEX server, the output command is ignored. Note that byte-swapping and floating point conversions may not be done on this type of output command.

Marker 3Dpoints : LISTofCOORD_3D

When processed by a renderer, this command will cause marker primitives to be rendered. A marker is a geometric primitive with only one geometric attribute - its position. The list points contains a list of 3D coordinates, each of which specifies the position of a marker in modeling coordinates.

During the rendering process, the marker’s position is transformed to a position in device coordinates. A marker has no geometric size, so geometric transformations will not affect the displayed size of the marker.

The marker’s color is transformed only by the depth-cueing computation (the light-source shading stage of the rendering pipeline affects only surfaces) and mapped to a device color. The clipping of markers whose position is inside the clipping volume but whose rendering is outside the clipping volume is implementationdependent.

Depending on the setting of the marker attribute ASF values, the marker_color, marker_type, and marker_scale attributes are either obtained directly from the current marker attribute values or from the marker_bundle_index’th entry in the renderer’s marker_bundle.

Marker 2Dpoints : LISTofCOORD_2D

When processed, this command will cause marker primitives to be drawn. This primitive functions exactly as the 3D marker primitive except that modeling coordinate positions are specified using only x-and ycoordinates, and the z-coordinateis always assumed to be zero.

Text 3Dorigin : COORD_3D vector1 : VECTOR_3D vector2 : VECTOR_3D string : ISTRING PEX Version 5.1, 31-August-1992

When processed by a renderer, this command will cause a text string to be rendered. The parameter string contains the text string to be rendered. A string is a list of data records, each of which contains char_set, char_set_width and encoding_state fields, as well as a list of the characters that actually make up that portion of the string. The char_set field is an index into the current font group. Font groups have individual fonts numbered starting at one, so a value of three would select the third font in the font group currently being used.

If a char_set value is not available in the current font group, then the entire string will be rendered using the default font group. If a char_set value is not available in the default font group, then that portion of the string will be rendered in an implementation-dependent manner. The char_set_width indicates whether characters in the string are 8-, 16-, or 32-bit values. Characters in the string are byte-swapped by the PEX server, if necessary. The encoding_state field is provided for use by clients and is not interpreted by the server.

The text string is located on a plane defined by its position and direction vectors. The origin of the string is a point in modeling coordinates indicated by origin, and the string’s direction is indicated by the direction vectors vector1 and vector2. Vector1defines the positive x-axisof the text local coordinate system. Vector2 defines the positive y-axisof the text local coordinate system.

Depending on the setting of the text attribute ASF values, the text_color, text_precision, char_expansion, char_spacing, and text_font_indexattributes are either obtained directly from the current text attribute values or from the text_bundle_index’thentry in the renderer’s text_bundle. The char_height, char_up_vector, text_path, and text_alignmentattributes are also used when drawing the text primitive. An attempt is made to render the text string as accurately as possible with the font group named by the current text_font_index. The directions specified by char_up_vector and text_path will be relative to the text local coordinate system.

During the rendering process, a string’s position is transformed to a position in device coordinates. The string’s color is transformed only by the depth-cueing computation (the light-source shading stage of the rendering pipeline affects only surfaces) and mapped to a device color. The text string is clipped depending on the current text precision value. If the text precision is String, clipping is done in an implementationdependent fashion. If the text precision is Char, clipping is done on at least a character-by-characterbasis. If the text precision is Stroke,clipping is performed at the clipping boundaries for each character.

If either of the text direction vectors is zero length or if the vectors are parallel, the vectors <1,0,0> and

<0,1,0> are used.

Text 2Dorigin : COORD_2D string : ISTRING

When processed, this command will cause a text primitive to be drawn. This primitive functions exactly as the 3D text primitive except that it has no direction vectors, the modeling coordinate position is specified using only x-and y-coordinates, and the z-coordinateis always assumed to be zero.

No errors or defaults are defined.

Annotation text 3D origin : COORD_3D offset: COORD_3D

When processed by a renderer, this command will cause an annotation text string to be rendered. The parameter string contains the text string to be rendered. A string is a list of data records, each of which contains char_set, char_set_width and encoding_state fields, as well as a list of the characters that actually make up that portion of the string. The char_set field is an index into the current font group. Font groups have individual fonts numbered starting at one, so a value of three would select the third font in the font group currently being used. If a char_set value is not available in the current font group, then the entire string will be rendered using the default font group. If a char_set value is not available in the default font group, then that portion of the string will be rendered in an implementation-dependent manner. The char_set_width indicates whether characters in the string are 8-, 16-, or 32-bit values. Characters in the string are byte-

PEX Version 5.1, 31-August-1992 swapped by the PEX server, if necessary. The encoding_state field is provided for use by clients and is not interpreted by the server.

The origin of the string is a point in modeling coordinates indicated by origin. An offset value in normalized projection coordinates is specified by offset. The point at which the annotation text string is to be placed is called the annotation point, and is computed by adding offsetto the transformed origin point. The zcomponent of the annotation point specifies the the x-yplane in normalized projection coordinate space on which the annotation text string will be placed.

Depending on the setting of the text attribute ASF values, the text_color, text_precision, char_expansion, char_spacing, and text_font_indexattributes are either obtained directly from the current text attribute values or from the text_bundle_index’thentry in the renderer’s text_bundle. The atext_height, atext_path, atext_alignment, atext_up_vector, and atext_styleattributes are also used when rendering the text string.

The annotation text string’s color is transformed only by the depth-cueing computation (the light-source shading stage of the rendering pipeline affects only surfaces) and mapped to a device color. The entire annotation text primitive is clipped if origin is clipped. If origin is not clipped by modeling, view, or workstation clipping, the annotation text will be clipped according to text clipping rules and the connection line, if present, will be clipped according to polyline clipping rules, except that modeling clipping will be ignored. The current set of polyline attributes will be used to draw the connection line if it is to be drawn.

No errors or defaults are defined.

Annotation text 2D origin : COORD_2D offset: COORD_2D string : ISTRING

When processed, this command will cause an annotation text primitive to be drawn. This primitive functions exactly as the 3D annotation text primitive except that origin and offset positions are specified using only xand y-coordinates, and the z-coordinateis always assumed to be zero.

Polyline 3D vertices : LISTofCOORD_3D

When processed by a renderer, this command will cause a polyline to be rendered. The polyline is defined by the list of vertices that are specified in vertices, each of which is a coordinate in the modeling coordinate system. The vertices are joined together by line segments. The first vertex of a polyline is connected to the second, the second connected to the third, and so on. The last vertex is not connected to the first.

Depending on the setting of the line attribute ASF values, line_color, line_type,and line_width attributes are either obtained directly from the current line attribute values or from the line_bundle_index’thentry in the renderer’s line_bundle.

Polylines have no geometric width, only length, so transformations will affect only the displayed length of a polyline. The polyline colors are transformed only by the depth-cueing computation (the light-source shading stage of the rendering pipeline affects only surfaces) and mapped to device colors. Polylines are not displayed if they are outside the currently defined clipping volume. Polylines that cross the clipping volume are clipped, and only the portion(s) inside the clipping volume is (are) displayed.

At structure creation time, if the polyline has fewer than two vertices, it is stored in the structure, but when this output command is interpreted, it has no visual effect. In immediate mode, such a primitive is ignored.

Polyline 2D vertices : LISTofCOORD_2DPEX Version 5.1, 31-August-1992

When processed, this command will cause a polyline primitive to be drawn. This primitive functions exactly as the 3D polyline primitive except that modeling coordinate positions are specified using only x-and ycoordinates, and the z-coordinateis always assumed to be zero.

At structure creation time, if the polyline has fewer than two vertices, it is stored in the structure, but when this output command is interpreted, it has no visual effect. In immediate mode, such a primitive is ignored.

Polyline set 3D with data color_type : COLOR_TYPE vert_attributes : BITMASK_SHORT vertices : LISTofLISTofVERTEX

When processed by a renderer, this command will cause a series of polylines to be rendered. The behavior of this primitive is identical to that of the 3D polyline primitive, except that multiple polylines can be drawn, and additional information can be specified at each polyline vertex. Color values that are passed will be of the type specified by color_type. The parameter vert_attributes indicates the attributes which are specified at each polyline vertex. The components of the vertex attributes bitmask are, in order:

color COLOR

If any of the attribute bits is set, the corresponding attributes must be present for each vertex, and they must be passed after the coordinate data for each vertex in the order that they appear in the list above.

If color values are passed per vertex, they are considered to be part of the primitive and are used instead of the line_color attribute. In addition, the use of per-vertex colors is affected by the polyline_interp attribute, which is obtained directly from the polyline_interp value if the polyline_interp_asf attribute is set to Individual or from the line_bundle_index’thentry in the renderer’s line_bundle. The polyline_interp attribute defines how color values between the vertices are to be computed.

At structure creation time, if any polyline in the set has fewer than two vertices, it is stored in the structure, but when this output command is interpreted, the polyline with insufficient data has no visual effect. In immediate mode, such a polyline is ignored.

Non-uniform B-spline curve order : CARD16 type: COORD_TYPE tmin: FLOAT tmax: FLOAT knots: LISTofFLOAT points : LISTofCOORD

When processed by a renderer, this command will cause a non-uniform B-spline curve to be rendered. The order is specified as a positive integer. The spline shape is specified using a list of knots in the parametric coordinate space, plus a list of control points that are specified in modeling coordinates. In general, the number of control points must be at least as large as the order. The number of control points plus the spline order must equal the number of knots. The knotssequence must form a non-decreasing sequence of numbers.

The typeparameter specifies whether the curve is Rational or NonRational. If the typeis Rational, then the point list must be provided as homogeneous modeling coordinates (COORD_4D), otherwise the the point list must be provided as non-homogeneous modeling coordinates (COORD_3D).

The parameter range values tminand tmaxspecify the range over which the B-spline curve is evaluated. Tmin must be less than tmax,tminmust be greater than or equal to the order’th knot value, and tmaxmust be less than or equal to the (k+1-order)’th knot value, where k is the number of knots.

Depending on the setting of the line attribute ASF values, line_color, line_type,line_width, and curve_approx attributes are either obtained directly from the current line attribute values or from the line_bundle_index’th entry in the renderer’s line_bundle.PEX Version 5.1, 31-August-1992

When an output command of this type is interpreted, if the curve order is not supported by the PEX server, the output command has no visual effect. In immediate mode, such a primitive is ignored.

Several conditions may cause an OutputCommanderror to be reported: typeis not Rational or NonRational, order is less than one, there are fewer control points than the order, the order is inconsistent with the number of knots and control points, the knots are not non-decreasing, tminand tmaxare inconsistent with the knots, or a Rational control point has a w coordinate that is less than or equal to zero.

Fill area 3D shape : SHAPE ignore_edges : BOOLEAN vertices : LISTofCOORD_3D

When processed by a renderer, this command will cause a fill area primitive to be rendered. A fill area is defined by a list of vertices which are to be joined together to form a planar surface. (Fill areas are not strictly required to be planar, but strange shading artifacts can occur if a fill area is not planar or nearly so.) The first vertex of a fill area is connected to the second, the second connected to the third, and so on. The last vertex is implicitly connected to the first.

During the rendering process, the fill area vertices are transformed to positions in device coordinates. The surface colors are transformed by the light source shading computation (which utilizes the interior style and the reflection model) and are further modified by the depth-cueing computation and mapped to device colors.

Fill areas are not displayed if they are outside the currently-defined clipping volume. Fill areas that cross the clipping volume are clipped, and only the portion(s) inside the clipping volume is (are) displayed.

A fill area can cross over itself to create a complex shape. The odd-even rule is used for determining the points that lie in the interior of a fill area. The shape parameter is passed as a hint as to the type of fill area that is defined by the vertices. A shape hint of Unknownmeans that nothing is known about the shape of the fill area. A shape of Complexmeans that the fill area edges may self-intersect. A shape of Nonconvexmeans that the edges do not self-intersect, but the fill area is not wholly convex. Convexmeans that all of the interior angles of the fill area are convex. Fill areas that are of a higher complexity than indicated by their shape hint are drawn in an implementation-dependent manner. PEX server extensions may ignore the shape hint and treat all fill area primitives as shape Unknown. The ignore_edges parameter specifies whether or not surface edge attributes are to be applied to the fill area primitives. If it is True, no surface edges will ever be drawn for the fill area. If False, surface edges will be drawn using the current surface edge attributes if the surface edge flag is On. Depending on the setting of the surface edge attribute ASF values, the surface_edges, surface_edge_color, surface_edge_type, and surface_edge_width attributes are either obtained directly from the current surface edge attribute values or from the edge_bundle_index’thentry in the renderer’s edge_bundle.

Depending on the setting of the surface attribute ASF values, the surface_color, interior_style, interior_style_index, surface_interp, and reflection_model attributes are either obtained directly from the current surface attribute values or from the interior_bundle_index’th entry in the renderer’s interior_bundle.

If, when rendered, the fill area is determined to be front-facing with respect to the point of view, the surface_color (obtained as previously described) and reflection_attr attributes are used to compute the color(s) of the fill area. If the fill area is determined to be back-facing with respect to the point of view, the bf_surface_color and bf_reflection_attr attributes are used instead. Regardless of the orientation of the fill area, if the interior_style is Pattern, the pattern_size, pattern_ref_pt, pattern_ref_vec1, and pattern_ref_vec2 attributes may be used to pattern the fill area.

At structure creation time, if the fill area has fewer than three vertices, it is stored in the structure, but when this output command is interpreted, it has no visual effect. In immediate mode, such a primitive is ignored.

An OutputCommanderror is reported if the shape or ignore_edges parameter is invalid.

Fill area 2D shape : SHAPE PEX Version 5.1, 31-August-1992 ignore_edges : BOOLEAN vertices : LISTofCOORD_2D

When processed, this command will cause a fill area primitive to be drawn. This primitive functions exactly as the 3D fill area primitive except that modeling coordinate positions are specified using only x-and ycoordinates, and the z-coordinateis always assumed to be zero.

At structure creation time, if the fill area has fewer than three vertices, it is stored in the structure, but when this output command is interpreted, it has no visual effect. In immediate mode, such a primitive is ignored.

An OutputCommanderror is reported if the shape or ignore_edges parameter is invalid.

Fill area 3D with data shape : SHAPE color_type : COLOR_TYPE facet_attributes : BITMASK_SHORT vert_attributes : BITMASK_SHORT facet : FACET

When processed by a renderer, this command will cause a fill area to be rendered. The behavior of this primitive is identical to that of the 3D fill area primitive, except that additional information can be specified for the fill area itself and for each vertex. Color values that are passed will be of the type specified by color_type.

The parameter facet_attributes indicates the attributes which are specified for the fill area. The components of the facet attributes bitmask are, in order:

color COLOR normal VECTOR_3D

If any of the attribute bits is set, the corresponding attribute must be present in the data that defines the fill area facet and they must be passed in the order that they appear in the list above. If a color value is passed per facet, it is taken to be the intrinsic color of the front face of the facet. If a normal is passed per facet, it is taken to be the normal to the facet.

The parameter vert_attributes specifies the attributes which are specified at each fill area vertex. The components of the vertex attributes bitmask are, in order:

If any of the attribute bits is set, the corresponding attributes must be present for each vertex, and they must be passed after the coordinate data for each vertex in the order that they appear in the list above.

If color values are passed per vertex, they are considered to be part of the primitive and are used instead of the surface_color attribute. Vertex colors will be utilized rather than facet colors if both are provided. If normals are passed per vertex, they are taken to be the normals at the vertices of the fill area. In addition, the use of per-vertex colors is affected by the surface_interp attribute, which is obtained directly from the surface_interp value if the surface_interp_asf attribute is set to Individual or from the interior_bundle_index’th entry in the renderer’s interior_bundle. The surface_interp attribute defines how color values between the vertices are to be computed.

All normals are assumed to be unit vectors. The effect of rendering with facet or vertex normals that are not unit vectors is implementation dependent.

The shape parameter is passed as a hint as to the type of fill area that is defined by the vertices. A shape hint of Unknownmeans that nothing is known about the shape of the fill area. A shape of Complexmeans that the fill area edges may self-intersect. A shape of Nonconvexmeans that the edges do not self-intersect, but the fill

PEX Version 5.1, 31-August-1992 area is not wholly convex. Convexmeans that all of the interior angles of the fill area are convex. Fill areas that are of a higher complexity than indicated by their shape hint are drawn in an implementation-dependent manner. PEX server extensions may ignore the shape hint and treat all fill area primitives as shape Unknown.

The ignore_edges parameter specifies whether or not surface edge attributes are to be applied to the fill area primitives. If it is True, no surface edges will ever be drawn for the fill area. If False, surface edges will be drawn using the current surface edge attributes if the surface edge flag is On.

At structure creation time, if the fill area has fewer than three vertices, it is stored in the structure, but when this output command is interpreted, it has no visual effect. In immediate mode, such a primitive is ignored.

An OutputCommanderror is reported if the shape or ignore_edges parameter is invalid.

Fill area set 3D shape : SHAPE ignore_edges : BOOLEAN contour_hint : CONTOUR vertices : LISTofLISTofCOORD_3D

When processed by a renderer, this command will cause a fill area set primitive to be drawn. This primitive is essentially a set of fill area primitives which, together, define a polygon with islands or holes. The planarity of the resulting polygon is not verified, but the results of processing a non-planar fill area set are implementation dependent. The ignore_edges parameter will be applied to all of the fill areas in the fill area set.

The shape parameter is passed as a hint as to the type of contours that comprise the fill area set. A shape hint of Unknownmeans that nothing is known about the shape of the constituent contours. A shape of Complex means that some contours of the fill area set may have edges that self-intersect. A shape of Nonconvexmeans that none of the contours of the fill area set have edges that self-intersect, but some may not be wholly convex.

Convexmeans that all of the interior angles of all of the contours are convex. Contours that are of a higher complexity than indicated by their shape hint are drawn in an implementation-dependent manner. PEX server extensions may ignore the shape hint and treat all constituent contours as shape Unknown.

The contour_hint parameter provides further information as to the relationships between contours in the fill area set. If contour_hint is Disjoint, all contours will be spatially disjoint. No overlapping or intersection occurs between any contours in the fill area set. If contour_hint is Nested,contours will either be disjoint or wholly contained within another contour. No contour will have edges that intersect or are coincident with edges of any other contour. If contour_hint is Intersecting, separate contours may have edges that are coincident or overlap. If contour_hint is Unknown,nothing is known about the interrelationships between contours. Fill area sets with contours that have higher complexity interrelationships than that indicated by their contour hint are drawn in an implementation-dependent manner. PEX server extensions may ignore the contour hint and treat all fill area sets as Unknown.

At structure creation time, if any of the contours of the fill area set has fewer than three vertices, or if there are no contours defined, the output command is stored in the structure, but when this output command is interpreted, it has no visual effect. In immediate mode, such a primitive is ignored.

Fill area set 2D vertices : LISTofLISTofCOORD_2D

When processed, this command will cause a fill area set primitive to be drawn. This primitive functions exactly as the 3D fill area set primitive except that modeling coordinate positions are specified using only xand y-coordinates, and the z-coordinateis always assumed to be zero.

PEX Version 5.1, 31-August-1992

At structure creation time, if any of the contours of the fill area set has fewer than three vertices, or if there are no contours defined, the output command is stored in the structure, but when this output command is interpreted, it has no visual effect. In immediate mode, such a primitive is ignored.

An OutputCommanderror is reported if the shape or ignore_edges parameter is invalid.

Fill area set 3D with data shape : SHAPE ignore_edges : BOOLEAN contour_hint : CONTOUR color_type : COLOR_TYPE facet_attributes : BITMASK_SHORT vert_attributes : BITMASK_SHORT facet_data : OPT_DATA vertices : LISTofLISTofVERTEX

When processed by a renderer, this command will cause a fill area set to be rendered. The behavior of this primitive is identical to that of the 3D fill area set primitive, except that additional information can be specified for each of the fill area sets, for each edge, and for each vertex. Color values that are passed will be of the type specified by color_type.

The parameter facet_attributes indicates the attributes which are specified in the facet_data parameter. The components of the facet attributes bitmask are, in order:

color COLOR normal VECTOR_3D

If any of the attribute bits is set, the corresponding attributes must be present in the facet_data parameter and must be passed in the order that they appear in the list above. If a color value is passed as part of facet_data, it is taken to be the intrinsic color of the front face of the fill area set.

The parameter vert_attributes specifies the attributes which are specified at each fill area set vertex. The components of the vertex attributes bitmask are, in order:

edges SWITCH

If any of the attribute bits is set, the corresponding attributes must be present for each vertex, and they must be passed after the coordinate data for each vertex in the order that they appear in the list above.

If color values are passed as part of facet_data or as part of the vertices list, they are considered to be part of the primitive and are used instead of the surface_color attribute. Vertex colors will be utilized rather than facet colors if both are provided. If normals are passed per vertex, they are taken to be the normals at the vertices of the fill area. If surface edge flags are specified per vertex, each flag specifies whether to draw the edge from the vertex with which the flag is specified to the next vertex. (E.g., for a facet with four vertices, the edge flag associated with vertex #1 indicates whether to draw edge #1-#2, edge flag #2 specifies edge #2-

#3, edge flag #3 specifies edge #3-#4, and edge flag #4 specifies edge #4-#1.) Surface edges are always drawn with the surface edge color, never with per facet or per vertex colors.

In addition, the use of per-vertex colors is affected by the surface_interp attribute, which is obtained directly from the surface_interp value if the surface_interp_asf attribute is set to Individual or from the interior_bundle_index’th entry in the renderer’s interior_bundle. The surface_interp attribute defines how color values between the vertices are to be computed.

PEX Version 5.1, 31-August-1992

An OutputCommanderror is reported if the shape, ignore_edges, or contour_hint parameter is invalid.

Triangle strip color_type : COLOR_TYPE facet_attributes : BITMASK_SHORT vert_attributes : BITMASK_SHORT facet_data : LISTofOPT_DATA vertices : LISTofVERTEX

When processed by a renderer, this command will cause a triangle strip primitive to be drawn. Color values that are passed will be of the type specified by color_type. The parameter facet_attributes indicates the attributes which are specified for each facet of the triangle strip. The components of the facet attributes bitmask are, in order:color COLOR normal VECTOR_3D

If any of the attribute bits is set, the corresponding attribute must be present in facet_data, which is the data that defines each triangular facet. The attributes that are passed in this way must be passed in the order that they appear in the list above. If a color value is passed per facet, it is taken to be the intrinsic color of the front face of the facet. If a normal is passed per facet, it is taken to be the normal to the facet. There will be n-2 entries in the facet_data list, where n is the number of entries in the vertices list.

The parameter vert_attributes specifies the attributes which are specified at each triangle strip vertex. The components of the vertex attributes bitmask are, in order:

color COLOR

If any of the attribute bits is set, the corresponding attribute must be present for each vertex, and it must be passed after the coordinate data for each vertex. The attributes that are passed in this way must be passed in the order that they appear in the list above.

If color values are passed per vertex, they are considered to be part of the primitive and are used instead of the surface_color attribute. Vertex colors will be utilized rather than facet colors if both are provided. If normals are passed per vertex, they are taken to be the normals at the vertices of the facet.

All normals are assumed to be unit vectors. The effect of rendering with facet or vertex normals that are not unit vectors is implementation dependent.

The triangle strip is created from the vertex array. The strip is composed of n-2 triangles, where n is the number of vertices. The first triangle is formed from the first three vertices in the list, the second triangle is formed by the second through the fourth vertices in the list, etc., up to the last triangle, which is formed by the last three vertices in the list.

All attributes that affect the representation of fill area sets also affect the representation of the triangle strip primitive.

At structure creation time, if the triangle strip has fewer than three vertices, the output command is stored in the structure, but when this output command is interpreted, it has no visual effect. In immediate mode, such a primitive is ignored.

Quadrilateral mesh shape : SHAPE m_pts: CARD16 n_pts : CARD16 vert_attributes : BITMASK_SHORTPEX Version 5.1, 31-August-1992 facet_data : LISTofOPT_DATA vertices : LISTofVERTEX

When processed by a renderer, this command will cause a quadrilateral mesh primitive to be rendered. The shape parameter is passed as a hint as to the type of quadrilaterals that comprise the primitive. A shape hint of

Unknownmeans that nothing is known about the shape of the constituent quadrilaterals. A shape of Complex means that the some quadrilaterals may have edges that self-intersect. A shape of Nonconvexmeans that none of the quadrilaterals have edges that self-intersect, but some may not be wholly convex. Convexmeans that all of the interior angles of all of the quadrilaterals are convex. Quadrilaterals that are of a higher complexity than indicated by their shape hint are drawn in an implementation-dependent manner. Color values that are passed will be of the type specified by color_type.

The parameter facet_attributes indicates the attributes which are specified for each facet of the quadrilateral mesh. The components of the facet attributes bitmask are, in order:

color COLOR normal VECTOR_3D

If any of the attribute bits is set, the corresponding attribute must be present in facet_data, which is the data that defines each quadrilateral facet. The attributes that are passed in this way must be passed in the order that they appear in the list above. If a color value is passed per facet, it is taken to be the intrinsic color of the front face of the facet. If a normal is passed per facet, it is taken to be the normal to the facet.

The parameter vert_attributes specifies the attributes which are specified at each quadrilateral mesh vertex.

The components of the vertex attributes bitmask are, in order:

If any of the attribute bits is set, the corresponding attribute must be present for each vertex, and it must be passed after the coordinate data for each vertex. The attributes that are passed in this way must be passed in the order that they appear in the list above.

If color values are passed per vertex, they are considered to be part of the primitive and are used instead of the surface_color attribute. Vertex colors will be utilized rather than facet colors if both are provided. If normals are passed per vertex, they are taken to be the normals at the vertices of the facet.

All normals are assumed to be unit vectors. The effect of rendering with facet or vertex normals that are not unit vectors is implementation dependent.

The surface will be created from a vertex array that is stored in row major order (i.e., the column number varies fastest as vertices are stored in the array). The (ith,jth), (i+1th,jth), (i+1th,j+1th) and (ith,j+1th) vertices are connected to create a single facet. Adjacent vertices are interconnected until the entire facet network is processed. There are m_pts× n_pts entries in the vertices array, and there are (m_pts-1)× (n_pts-1) entries in the facet_data array if any per-facet attributes are passed. m_ptsis the number of columns in the vertex array and n_pts is the number of rows.

It is allowable for the boundary of a single facet to not reside in a single plane. The treatment of the vertex attributes in this case is implementation-dependent.

All attributes that affect the representation of fill area sets also affect the representation the quadrilateral mesh primitive.

At structure creation time, if either m_ptsor n_pts is less than two, the output command is stored in the structure, but when this output command is interpreted, it has no visual effect. In immediate mode, such a primitive is ignored.

An OutputCommanderror is reported if the shape parameter is invalid.

PEX Version 5.1, 31-August-1992

Set of fill area sets shape : SHAPE color_type : COLOR_TYPE fas_attributes : BITMASK_SHORT vert_attributes : BITMASK_SHORT edge_attributes : BITMASK_SHORT contour_hint : CONTOUR contours_all_1 : BOOLEAN num_fas: CARD16 num_verts: CARD16 num_edges: CARD16 num_contours : CARD16 per_fas_data : LISTofOPT_DATA per_vert_data : LISTofVERTEX per_edge_data : LISTofSWITCH contours : LISTofLISTofLISTofCARD16

When processed by a renderer, this command will draw a set of fill area sets that may be connected (i.e., individual fill area sets may share geometry and attribute information at vertices). Shading calculations and transformations need only be performed once per shared vertex instead of once for every fill area set that shares the vertex. Similarly, data can be transmitted across the network once per unique vertex instead of once for every fill area set sharing the vertex.

The shape parameter is passed as a hint as to the type of contours that comprise each of the fill area sets. A shape hint of Unknownmeans that nothing is known about the shape of the constituent contours. A shape of

Complexmeans that some contours of the fill area sets may have edges that self-intersect. A shape of

Nonconvexmeans that none of the contours of the fill area sets have edges that self-intersect, but some may not be wholly convex. Convexmeans that all of the interior angles of all of the contours are convex. (Note that a fill area set with more than one contour is always allowed to have contours that intersect. It is quite possible that the only times that the fastest rendering code path can be taken are if the number of contours in a fill area set is equal to one or if contours_all_1 is True, and the shape flag for the set of fill area sets primitive is Convex.) Contours that are of a higher complexity than indicated by their shape hint are drawn in an implementation-dependent manner. PEX server extensions may ignore the shape hint and treat all constituent contours as shape Unknown.

The contour_hint parameter provides further information as to the relationships between contours in each of the fill area sets. If contour_hint is Disjoint, all contours will be spatially disjoint. No overlapping or intersection occurs between any contours in any of the fill area sets. If contour_hint is Nested,contours will either be disjoint or wholly contained within another contour. No contour will have edges that intersect or are coincident with edges of any other contour. If contour_hint is Intersecting, separate contours may have edges that are coincident or overlap. If contour_hint is Unknown,nothing is known about the interrelationships between contours. Fill area sets with contours that have higher complexity interrelationships than that indicated by their contour hint are drawn in an implementation-dependent manner. PEX server extensions may ignore the contour hint and treat all fill area sets as Unknown.

Color values that are passed will be of the type specified by color_type.

The parameter fas_attributes indicates the attributes that are specified for each fill area set. The components of the fas_ attributes bitmask are, in order:

color COLOR normal VECTOR_3D

If any of the attribute bits is set, the corresponding attribute must be present in per_fas_data, which contains one data record for each fill area set. The attributes that are passed in this way must be passed in the order that they appear in the list above. If a color value is passed, it is taken to be the intrinsic color of the front face of

PEX Version 5.1, 31-August-1992 the fill area set. If a normal is passed, it is taken to be the normal to the fill area set. If fas_attributes is null, the per_fas_data list will be null as well. Otherwise, there will be num_fasentries in per_facet_data.

The parameter vert_attributes indicates the attributes that are provided at each vertex in the list of unique vertices specified by per_vert_data. The components of the vertex attributes bitmask are, in order:

color COLOR normal VECTOR_3D

If any of the attribute bits is set, the corresponding attribute must be present for each vertex in the per_vert_data list, and it must be passed after the coordinate data for each vertex. The attributes that are passed in this way must be passed in the order that they appear in the list above. If color values are passed per vertex, they are considered to be part of the primitive and are used instead of the surface_color attribute. If normals are passed per vertex, they are taken to be the normal at the indicated vertex, and will be used by all contours that share the vertex. There will always be num_vertsentries in the per_vert_data list.

All normals are assumed to be unit vectors. The effect of rendering with facet or vertex normals that are not unit vectors is implementation dependent.

The parameter edge_attributes specifies the attributes that are specified at each edge. The components of the edge attributes bitmask are, in order:

edges SWITCH

If any of the attribute bits is set, the corresponding attribute must be present for each edge in the list per_edge_data. If none of the attribute bits are set, the list per_edge_data will be an empty list. Otherwise, it will contain num_edgesentries, each of which contains a switch indicating whether or not the corresponding edge should be drawn. This list is a flattened list without counts, so if it is nonempty, it is up to the PEX server extension to maintain a pointer to the proper position in this list while processing the data in contours.

If edge switches are supplied, each flag specifies whether to draw the edge from the vertex with which the flag is specified to the next vertex. (E.g., for a contour with four vertices, the edge flag associated with vertex #1 indicates whether to draw edge #1-#2, edge flag #2 specifies edge #2-#3, edge flag #3 specifies edge #3-#4, and edge flag #4 specifies edge #4-#1.) Surface edges are always drawn with the surface edge color, never with per-fill-area-set or per-vertex colors.

The connectivity of the primitive is defined by the contours array. The number of contours in the first fill area set is contained as the first entry in the contours array. The number of contours is followed by a list of data records, one for each of the contours in the fill area set. If this number is n, then the next n data records in the contours array are used to define the first fill area set. The value following the contour count contains the number of vertices in the first contour of the first fill area set. If this number is m,then the next mvalues in the array comprise the data record for the first contour. This data record contains the indices for the vertices of the first contour. Depending on n, the next value in the list is either the number of vertices in the second contour for the first fill area set, or it is the number of contours in the second fill area set. As a special case, if contours_all_1 is True, then the contour count field in each fill area set is guaranteed to be one.

Vertices are numbered with indices starting from zero (i.e., the first vertex is referenced as vertex 0).

All attributes that affect the representation of fill area sets also affect the representation of the set of fill area sets primitive.

An OutputCommanderror is reported if any of the edge flags in the per_edge_data array is not On or Off,or if any of the shape, contour_hint, or contours_all_1 parameters is invalid, or if any of the vertex indices in the contours array is out of range, or if there are not as many edge flags as there are vertex indices in the lists in the contours array.

Non-uniform B-spline surface type: COORD_TYPE u_order : CARD16 PEX Version 5.1, 31-August-1992 v_order : CARD16 u_knots: LISTofFLOAT v_knots: LISTofFLOAT mpts: CARD16 npts : CARD16 points : LISTofCOORD trim_curves : LISTofLISTofTRIM_CURVE

When processed by a renderer, this command will draw a non-uniform B-spline surface. It generates the spline surface as a function of the parametric variables u and v. U_order and v_order indicate the order of the parametric variables and are specified as positive integers. The spline shape is specified using two lists of knots in the parametric coordinate space, plus an array of control points that are specified in modeling coordinates. The u_knotssequence and the v_knotssequence must each form a non-decreasing sequence of numbers. Mptsindicates the number of points in the u direction and npts indicates the number of points in the vdirection. The points are stored in the vertex array in row major order (i.e., the column number varies fastest as vertices are stored in the array) and the rows increase in the direction of increasing v.

The minimum and maximum knot values in u_knotsdefine the range over which the B-spline surface is evaluated in the u parametric direction, and the minimum and maximum knot values in v_knotsdefine the range over which the B-spline surface is evaluated in the vparametric direction.

The typeparameter specifies whether the surface is Rational or NonRational. If the surface_type is Rational, then the point list must be provided as homogeneous modeling coordinates (COORD_4D), otherwise the point list must be provided as non-homogeneous modeling coordinates (COORD_3D).

In addition to the parametric bounds, a list of trimming loops may be specified. Trimming loops serve to further restrict the region in parametric coordinate space over which the B-spline surface is to be evaluated.

Each trimming loop is defined as a list of one or more B-spline trimming curves that are connected head-to-tail. Each trim curve can be Rational or NonRational, have a different order, etc. The list must be explicitly closed, so that the tail of the last B-spline curve joins the head of the first B-spline curve in each trimming loop. Each trimming curve is parameterized independently. If there is a floating point inaccuracy in closure or in head-to-tail connectivity between B-spline curves , closure or connectivity will be assumed. B-spline curves for trimming loops are defined in the parameter space of the surface and may not go outside the parameter space of the surface. When no trimming loops are specified, the rectangular parameter limits of the surface are rendered as the edges of the surface based on the edge flag attribute.

Trimming loops define the region of the surface that is to be rendered based on the following two rules: (1) a point is in the portion of the surface to be rendered if any ray projected from it to infinity has an odd number of intersections with trimming loops, and (2) traveling in the direction of a trimming loop, the portion of the surface to be trimmed away should be on the right and the portion to be retained should be on the left. In other words, a loop defined in counterclockwise order will cause the interior of the loop to be retained and the exterior to be clipped away. A clockwise loop will cause the exterior of the loop to be retained and the interior to be trimmed away. If loops are nested, they must alternate in direction. In all cases, the outermost loop must be counterclockwise. No B-spline curve may intersect itself and no trimming loop may intersect itself or any other trimming loop. Trimming loops that do not obey these rules will result in an implementation-dependent rendering.

Each B-spline curve has a visibility flag that controls its visibility for the purposes of surface edge display.

Depending on the settings of a renderer’s surface edge attributes and the visibility flags associated with trim curves, the B-spline curves in trimming loops may be drawn as surface edges.

All attributes that affect the representation of fill area sets also affect the representation of the non-uniform Bspline surface primitive. In addition, the surface_approx attribute is used to determine how to approximate the B-spline surface and the psurf_char attribute is used to specify the appearance of the B-spline surface.

PEX Version 5.1, 31-August-1992

If either of the surface orders or any of the trim curve orders is not supported by the PEX server, the output command has no visual effect. In immediate mode, such a primitive is ignored.

Several conditions may cause an OutputCommanderror to be reported: typeis not Rational or NonRational, order is less than one, there are fewer control points in either the u or v direction than the order, the order is inconsistent with the number of knots and control points, the knots are not non-decreasing, a Rational control point has a w coordinate that is less than or equal to zero, a trim curve order is less than 2, a trim curve does not have enough control points for its order, a trim curve’s order is inconsistent with its number of knots and control points, a trim curve’s knot sequence is not non-decreasing, or a trim curve’s parameter range is inconsistent with its knots.

Cell array 3D point1 : COORD_3D point2 : COORD_3D point3 : COORD_3D dx: CARD32 dy: CARD32 colors : LISTofTABLE_INDEX

When processed by a renderer, this command will cause a cell array primitive to be rendered. Color values that are passed will be of type Indexed. A cell array is a parallelogram of equal-sized cells, each of which is a parallelogram and has a single color. Each cell has a width defined by:

width = dx √� (point1.x − point2.x)2 + (point1.y − point2.y)2 + (point1.z − point2.z)2

_____________________________________________________________ and a height defined by:

height = dy

(point1.x − point3.x)2 + (point1.y − point3.y)2 + (point1.z − point3.z)2

The colors are specified in a one-dimensional array of size dx× dy. The color of each cell is specified by the index of the corresponding element in the colors array. Colors are stored in this array by rows, that is, the column number varies fastest as colors are stored into the array. The first color in the array is the color at the cell at the corner of point1, and subsequent colors represent the colors of cells proceeding to point2.

If any color index is not defined, color index one is used. If color index one is not defined, the default values in Appendix D are used.

An OutputCommanderror is reported if dxor dyis zero.

Cell array 2D point1 : COORD_2D point2 : COORD_2D

When processed, this command will cause a cell array primitive to be drawn. This primitive functions exactly as the 3D cell array primitive except that modeling coordinate positions are specified using only x-and ycoordinates, and the z-coordinateis always assumed to be zero. In addition, the cell array is defined by two points which define a rectangle that is taken to be aligned with the modeling coordinate axes.

in Appendix D are used. PEX Version 5.1, 31-August-1992

An OutputCommanderror is reported if dxor dyis zero.

Extended cell array 3D color_type : COLOR_TYPE point1 : COORD_3D point2 : COORD_3D point3 : COORD_3D dx: CARD32 dy: CARD32 colors : LISTofCOLOR

When processed by a renderer, this command has the same effect as the "cell array 3D" primitive, except that the colors may be passed as indexed or direct color values, depending on the setting of color_type.

If any color index is not defined, color index one is used. If color index one is not defined, the default values in Appendix D are used.

GDP 3Dgdp_id : INT32 points : LISTofCOORD_3D data : LISTofCARD8

When processed by a renderer, the effect of this command is implementation-dependent. Because of floating point and color format discrepancies across a network interface, it is not anticipated that the GDP 3D will provide a useful extension mechanism, but it is provided for PHIGS compatibility purposes.

If the specified GDP identifier is not supported, the output command is ignored. Note that byte-swapping and floating point conversion may not be done on this type of output command.

GDP 2Dgdp_id : INT32 points : LISTofCOORD_2D point and color format discrepancies across a network interface, it is not anticipated that the GDP 2D will

Noop When processed by a renderer, this command will only update the current path. It is useful for client-side accumulate state traversals since it does not generate any output.

PEX Version 5.1, 31-August-1992

4. Lookup Tables

______________________________________________________________________________________________ A lookuptable is a PEX resource that allows clients to create tables of values for various purposes. Lookup tables are used to support a level of indirection for some output primitive attributes as well as for storing view information, light source descriptions, depth-cue information, etc.

Tables may be sparse, therefore tables consist of index/entry pairs. The indexis the number that will be used to reference that entry. Since indices are 16-bit values, index values are allowed to be any value in the range

[0..65535], with the possible exceptions of 0 (some tables allow an index of zero, others do not) and 65535 (tables can have at most 216 − 1 definable entries, so if a table begins at zero, the maximum index value is 65534). An entry is the collection of information (or the data record) that is defined for each type of table. The table descriptions in this section include the definition of an entry for each type of table. A table index refers to an undefined entry if no table entry has ever been associated with that index, or if the associated table entry has been deleted. A table entry may contain one or more data items, depending on the table type. For instance, in the MarkerBundle table type, each entry in the table consists of a marker type value, a marker scale value, and a marker color value.

A lookup table may have predefined entries. Predefined entries are a set of contiguous table entries that are automatically filled in by the server when the table is created. PEXGetTableInfo returns the range of predefined entries. Predefined table entries may be deleted or overwritten.

Each type of table has a specific index value that indicates the default table entry. If a table index references an undefined table entry, the contents of the default table entry will be used. If the default table entry is undefined, then the default attribute values (as listed in Appendix D) will be used as the default entry. The default entry for all tables is one, except for the view, depth cue, and color approximation tables whose default entry is zero.

PEX lookup tables are designed to support PHIGS set/realized semantics. A lookup table entry may be set to a value that is impossible to represent exactly. Such a value will be silently mapped to a reasonable default when rendering to the drawable. When retrieving entry values from a lookup table, clients may request the value as originally specified by the client (value_type= Set),or the value that is actually used when rendering, whether it is the value originally specified or an approximation (value_type= Realized). Since all predefined entries are by definition realizable, predefined lookup table entries will return the same value regardless of whether the Setor the Realized value is requested.

The allowable table types, the range of allowable index values, the default entry, and the format of a table entry for each table type are as follows:

LineBundle (1..65535, default entry = 1)

This type of lookup table is used to maintain attributes for drawing polyline and curve primitives. Depending on the setting of the aspect source flag attributes, polyline and curve attributes may be obtained from a line bundle table. Each entry in this type of table consists of the following:

line_type LINE_TYPE polyline_interp POLYLINE_INTERP curve_approx CURVE_APPROX line_width FLOAT line_color COLOR_SPECIFIER

The attributes stored in a line bundle table are defined and used in the same fashion as the pipeline context attributes of the same name.

MarkerBundle (1..65535, default entry = 1)

This type of lookup table is used to maintain attributes for drawing marker primitives. Depending on the setting of the aspect source flag attributes, marker attributes may be obtained from a marker bundle table.

PEX Version 5.1, 31-August-1992

Each entry in this type of table consists of the following:

marker_type MARKER_TYPE marker_scale FLOAT marker_color COLOR_SPECIFIER

The attributes stored in a marker bundle table are defined and used in the same fashion as the pipeline context attributes of the same name.

TextBundle (1..65535, default entry = 1)

This type of lookup table is used to maintain attributes for drawing text and annotation text primitives.

Depending on the setting of the aspect source flag attributes, text and annotation text attributes may be obtained from a text bundle table. Each entry in this type of table consists of the following:

text_font_index TABLE_INDEX text_precision TEXT_PRECISION char_expansion FLOAT char_spacing FLOAT text_color COLOR_SPECIFIER

The attributes stored in a text bundle table are defined and used in the same fashion as the pipeline context

InteriorBundle (1..65535, default entry = 1)

This type of lookup table is used to maintain attributes for drawing surface primitives. Depending on the setting of the aspect source flag attributes, surface attributes may be obtained from an interior bundle table.

interior_style INTERIOR_STYLE interior_style_index TYPE_OR_TABLE_INDEX surface_color COLOR_SPECIFIER reflection_attr REFLECTION_ATTR reflection_model REFLECTION_MODEL surface_interp SURFACE_INTERP bf_interior_style INTERIOR_STYLE bf_interior_style_index TYPE_OR_TABLE_INDEX bf_surface_color COLOR_SPECIFIER bf_reflection_attr REFLECTION_ATTR bf_reflection_model REFLECTION_MODEL bf_surface_interp SURFACE_INTERP surface_approx SURFACE_APPROX

The attributes stored in an interior bundle table are defined and used in the same fashion as the pipeline context attributes of the same name.

EdgeBundle (1..65535, default entry = 1)

This type of lookup table is used to maintain attributes for drawing edges of surface primitives. Depending on the setting of the aspect source flag attributes, surface edge attributes may be obtained from an edge bundle table. Each entry in this type of table consists of the following:

surface_edges SWITCH surface_edge_type SURFACE_EDGE_TYPE surface_edge_width FLOAT surface_edge_color COLOR_SPECIFIER

PEX Version 5.1, 31-August-1992

The attributes stored in an edge bundle table are defined and used in the same fashion as the pipeline context attributes of the same name.

Pattern (1..65535, default entry = 1)

This type of lookup table can be used to maintain patterns for use when interior_style is set to Pattern.

color_type COLOR_TYPE numx CARD16 numy CARD16 colors LISTofCOLOR

A pattern rectangle is comprised of numx× numycells. Color_type indicates whether the color values are stored as indexed or direct color values. The colors are stored in the array row-by-row. The upper left hand cell in the pattern rectangle is the first one in the list of colors, followed by the remaining cells in the first row.

The color values for cells in the second row follow, and so on.

Color (0..65534, default entry = 1)

This type of lookup table can be used to resolve indirect color references. Consequently, all color values in this type of table must be specified as direct colors.

color DIRECT_COLOR

A ColorTypeerror is generated if an attempt is made to set an entry with a color_type of Indexed.

TextFont (1..65535, default entry = 1)

This type of lookup table is used to maintain a list of font groups. Each font group is a list of resource IDs for either PEX fonts or X11 fonts. Resource IDs for fonts can appear multiple times in a font table, or even within a single table entry. Only PEX fonts are guaranteed to fully realize all of the PEX text attributes.

Specifically, scaling and rotation operations on text strings are not guaranteed to affect text primitives if an

X11 font is used, but they are guaranteed to work if a PEX font is used. Font values are specified as indices when using output commands. A font index can be used with a table of this type in order to obtain the actual font group to be used. Switching between fonts in the font group is accomplished by means of a switching mechanism embedded within strings that are to be rendered. It is up to the client to ensure that all of the character sets that are available in a table of this type are available in the default table entry as well.

font LISTofFONT_ID

If a font is opened, bound to a font table, and then closed, the contents of the font will remain, since the contents are still being referenced by a font table. However, when the font table is queried, the value

AlreadyFreed will be returned for such a font, since it no longer has a valid resource ID by which it can be referenced.

View (0..65534, default entry = 0)

This type of lookup table is used to maintain viewing information. "Views" are then specified as indices, which are used to look up the appropriate information in a view lookup table.

clip_flags BITMASK_SHORT clip_limits NPC_SUBVOLUME orientation MATRIX mapping MATRIX

Orientation is a matrix which maps geometry from the world coordinate system to the viewing reference coordinate system. (This is a right-handed coordinate system and is also known as the eye or viewing coordinate system.) Mapping is a matrix which maps geometry from the viewing reference coordinate system

PEX Version 5.1, 31-August-1992 to the normalized projection coordinate system (also a right-handed coordinate system). This transformation is typically a parallel or perspective projection. The clip_limits specify the minimum and maximum of a rectangular volume in normalized projection coordinates and, clip_flags contains three bits that indicate whether or not clipping should be performed against the sides, back, and front planes of the volume specified by clip_limits. The actual clipping volume for each view is a rectangular parallelpiped that is computed by taking the intersection of the view clipping volume (determined by clip_limits and clip_flags) and the NPC subvolume.

Light (1..65535, default entry = 1)

This type of lookup table is used to maintain light source definitions for use in light source shading computations. light_type LIGHT_TYPE direction VECTOR_3D point COORD_3D concentration FLOAT spread_angle FLOAT attenuation [factor1, factor2 : FLOAT] color COLOR_SPECIFIER

There are four types of light sources currently supported in PEX: ambient, WCSvector, WCSpoint and WCS spot. Depending on the type of light, some of the values in a table entry may be ignored.

An ambient light source is defined by color. It is a non-directional light that affects the color of all surfaces regardless of their orientation. Each ambient light causes a constant amount of intensity to be added to each point in the scene.

A WCS vector light source (or directional light source) is defined by direction and color. A light source of this type is located at infinity so all light rays which emanate from it are parallel when they strike an objects surface.

A WCS point light source (or a positional light source) illuminates equally in all directions and is specified by point, attenuation, and color. point indicates the world coordinate source of the light and attenuation indicates how the intensity of the point light source drops off as a function of distance.

A WCS spot light source simulates the behavior of a spotlight and is specified by direction, point, concentration, spread_angle, attenuation, and color. point indicates the world coordinate source of the light and direction and spread_angle specify a cone of influence. The direction vector is relative to the specified light source position and spread_angle is the half-angle of the cone. The contribution of a spotlight is zero if the point in question lies outside of the cone of influence.

DepthCue (0..65534, default entry = 0)

This type of lookup table is used to maintain depth-cueing information.

mode SWITCH front_plane FLOAT back_plane FLOAT front_scaling FLOAT back_scaling FLOAT

The depth cueing computation modifies colors according to the distance from the viewing position. color indicates the color to which objects will tend when going from the front_plane to the back_plane.

front_scaling and back_scaling represent values by which the colors will be scaled at the front and back depth

PEX Version 5.1, 31-August-1992 cueing planes. The depth cueing computation is performed in NPC space-- front_plane is the distance to the front depth-cueing plane in NPC coordinates and back_plane is the distance to the back depth-cueing plane in

NPC coordinates.

ColorApprox (0..65534, default entry = 0)

This type of lookup table is used to define the way that a renderer will transform rendering pipeline color values into displayable pixel values. Each entry in this type of table contains the following data:

type COLOR_APPROX_TYPE color_model COLOR_APPROX_MODEL max1 CARD16 max2 CARD16 max3 CARD16 mult1 CARD32 mult2 CARD32 mult3 CARD32 weight1 FLOAT weight2 FLOAT weight3 FLOAT base_pixel CARD32 dither SWITCH

After a renderer has performed illumination, depth-cueing, and clipping operations, it is left with a rendering pipeline color that must be converted to a displayable pixel value. The renderer’s current color_approx_index is used to determine which entry in a table of this type is to be used to perform the conversion to a displayable pixel value. As the color value emerges from the rendering pipeline, it is first converted to a color in the color space specified by color_model. (In the case where the rendering pipeline colors are already in the specified color space, this is a null mapping.)

If typeis ColorSpace, each component of the converted color (c1, c2, c3) is scaled by the corresponding maximum value (max1,max2,max3). (max1,max2,max3can be used by the client to indicate the number of entries in the colormap for each color axis, minus 1. For example, to compute a pixel value for a 3-3-2 RGB colormap allocation, the max values would be 7, 7, and 3). The resulting color components are packed into a single pixel value by multiplying the first component by mult1,the second by mult2,the third by mult3,and then adding this to the base_pixel. When the typeis ColorSpace, weight1,weight2,and weight3values are not used.

For a more concrete example, assume that the color_model is set to RGB. During the color approximation stage, each color value that emerges from the rendering pipeline must first be converted to an RGB triple. If the rendering pipeline performs color computations in RGB space then this conversion is a no-op. Each of the three components are then mapped to an integer value as follows:

red = red intensity component mapped into the range [0, max1] green = green intensity component mapped into the range [0, max2] blue = blue intensity component mapped into the range [0, max3] and a single pixel value is formed by computing:

pixel = mult1× red + mult2× green + mult3× blue + base_pixel

If color_type is ColorRange, the values are combined in a different fashion during the color approximation stage. Once again, the rendering pipeline color is first converted into a color in the color space specified by color_model. First, the color components (c1, c2, c3) that emerge from the rendering pipeline are multiplied by their corresponding normalized weight values (weight1,weight2,weight3)and the terms are added together to form a single value. The weight values can be adjusted to allow equal weighting of the components

(weights are all equal) or to minimize or eliminate one or more of the components (one or more weights equal

PEX Version 5.1, 31-August-1992 to 0). For instance, the weight values of 0.30, 0.59, 0.11 can be used to convert an RGB value to a singlevalued intensity according to the NTSC color standard.

Next, the computed value is multiplied by max1(max2and max3are not used) which should be set by the client to represent the number of color map entries in the range, minus 1. For instance, if a client desires to display its computed image on a pseudo-color display using gray scale, it could allocate 100 contiguous color cells in the color map, and set max1to the value of 99, so that intensity values would be mapped into the range

[0,99]. This value is then replicated for each of the three color components, which are then multiplied by mult1,mult2,and mult3respectively. The values are then added together with base_pixel to form the pixel value that is to be written. It is up to the client to provide reasonable multipliers for drawables that are not three-channel in nature. For instance, multipliers of (1.0, 0.0, 0.0) could be used if the target drawable was known to be a window of visual type PseudoColor. PEX implementations are free to optimize the case where one or more of the multipliers is zero.

The use of addition rather than logical OR for composing pixel values permits allocations where the primary components are not allocated into distinct bitplanes. Since some hardware allows a performance improvement if the multiplication values (mult1,mult2,mult3)are powers of two, the PEXGetImpDepConstants request can be used to obtain the constant BestColorApproxValuesin order to get an indication as to whether powers of two are preferred.

Dither is treated as a hint to the renderer as to whether or not some attempt at dithering should be performed.

Whether or not dithering is supported and the dithering algorithm that is used are implementation-dependent

(see PEXGetImpDepConstants).PEX Version 5.1, 31-August-1992

4.1. Lookup Table Resource Management

The lookup table is an X11 resource and carries all of the responsibilities and access rights of X11 resources. These requests manage the creation, freeing, and copying of lookup table resources.

4.1.1. Create Lookup Table

Name: PEXCreateLookupTable

Request:drawable_example : DRAWABLE_ID lut_id : LOOKUP_TABLE_ID table_type : TABLE_TYPE

Errors: IDChoice, Drawable, Match, Value, Alloc, LookupTable

Description:This request creates a lookup table resource for the specified lut_id, for use with drawables with the same root window and depth as the example drawable specified by drawable_example. The table_type parameter indicates the type of lookup table that is to be created. Some entries of a lookup table may be defined at the time the resource is created. The number of predefined entries and their contents are dependent on the type of table and are implementation-dependent.

4.1.2. Copy Lookup Table

Name: PEXCopyLookupTable

Request:src_lut_id : LOOKUP_TABLE_ID dest_lut_id : LOOKUP_TABLE_ID

Errors: LookupTable, Match

Description:This request copies the source lookup table src_lut_id to a destination lookup table dest_lut_id, after first deleting all the entries in the destination lookup table. The dest_lut_id must already exist as a valid resource and it must be of the same type as src_lut_id.

PEX Version 5.1, 31-August-1992

4.1.3. Free Lookup Table

Name: PEXFreeLookupTable

Request:lut_id : LOOKUP_TABLE_ID

Errors: LookupTable

Description:This request deletes the association between the resource ID and the lookup table. The lookup table storage will be freed when no other resource references it.

PEX Version 5.1, 31-August-1992

4.2. Lookup Table Inquiry

These requests inquire lookup table attributes.

4.2.1. Get Table Info

Name: PEXGetTableInfo

Request:drawable_example : DRAWABLE_ID table_type : TABLE_TYPE

Reply: definable_entries : CARD16 num_predefined : CARD16 predefined_min : TABLE_INDEX predefined_max : TABLE_INDEX

Errors: Drawable, Match, Value, LookupTable

Description:This request will return information about lookup tables of the specified table_type if they were to be used with drawables of the same root and depth as drawable_example. Definable_entries is the maximum number of entries that can be defined in this type of table, and includes the number of predefined entries.

Predefined entries can be redefined by the client. All the entries between predefined_min and predefined_max are guaranteed to be defined initially (i.e., predefined entries must have contiguous indices). If num_predefined is zero, then the values for predefined_min and predefined_max are meaningless. PEX Version 5.1, 31-August-1992

4.2.2. Get Predefined Entries

Name: PEXGetPredefinedEntries

Request:fp_format : FLOAT_FORMAT drawable_example : DRAWABLE_ID table_type : TABLE_TYPE start : TABLE_INDEX count : CARD16

Reply: entries : LISTofTABLE_ENTRY

Errors: Drawable, Match, Value, FloatingPointFormat, LookupTable

Description:This request will return the values for predefined table entries of the specified table_type if they were to be used with drawables of the same root and depth as drawable_example. Count table entries will be returned in entries, starting with the table entry specified by start. The values in entries will be in the format defined for table_type. Floating point values in entries will be returned in the floating point format specified in fp_format.

4.2.3. Get Defined Indices

Name: PEXGetDefinedIndices

Request:lut_id : LOOKUP_TABLE_ID

Reply: defined_indices : LISTofTABLE_INDEX

Errors: LookupTable

Description:This request will return in defined_indices a list of all the indices that are currently defined in the lookup table resource specified by lut_id. The entries returned include those predefined by the server and those that have been defined by clients.PEX Version 5.1, 31-August-1992

4.2.4. Get Table Entry

Name: PEXGetTableEntry

Request:fp_format : FLOAT_FORMAT lut_id : LOOKUP_TABLE_ID index: TABLE_INDEX value_type: {Set,Realized}

Reply: status : {Defined, Default} table_type : TABLE_TYPE entry : TABLE_ENTRY

Errors: LookupTable, FloatingPointFormat, Value

Description:This request will return the type of lookup table and the lookup table entry specified by index. The entry will be obtained from the lookup table specified by lut_id and will be of the format indicated by lut_id’s table type. If the specified entry in the lookup table is not defined, the values for the default entry for that table type will be returned in entry and status will be set to Default. If the specified entry is defined, its contents will be returned in entry and status will be set to Defined. If value_typeis Set,the values returned will be those originally specified by the client. If value_typeis Realized,the values returned will be the values that are actually used during rendering (i.e., the default values, which are used if the specified value is not supported on the drawable). Floating point values in entry will be returned in the floating point format specified in fp_format.

4.2.5. Get Table Entries

Name: PEXGetTableEntries start : TABLE_INDEX count : CARD16

Reply: table_type : TABLE_TYPE entries : LISTofTABLE_ENTRY

Errors: LookupTable, Value, FloatingPointFormat

Description:This request will return the type of table and count table entries from the lookup table specified by lut_id, starting at the entry specified by start. The default entry will be returned for any entry in the requested

PEX Version 5.1, 31-August-1992 range that is not defined. If value_typeis Set,the values returned will be those originally specified by the client. If value_typeis Realized,the values returned will be the values that are actually used during rendering (i.e., the default values, which are used if the specified value is not supported on the drawable).

Floating point values in entries will be returned in the floating point format specified in fp_format.

PEX Version 5.1, 31-August-1992

4.3. Lookup Table Modification

This section contains requests that modify lookup table resources.

4.3.1. Set Table Entries

Name: PEXSetTableEntries

Request:fp_format : FLOAT_FORMAT lut_id : LOOKUP_TABLE_ID start : TABLE_INDEX count : CARD16 entries : LISTofTABLE_ENTRY

Errors: LookupTable, Value, FloatingPointFormat, ColorType, Alloc

Description:This request will set count lookup table entries in the lookup table resource specified by lut_id, starting at the entry indicated by start. The values to use when setting the entries in the lookup table are provided in entries, and are in the format specified for a lookup table of lut_id’s type. Floating point values in entries will be in the floating point format specified in fp_format.

4.3.2. Delete Table Entries

Name: PEXDeleteTableEntries

Request:lut_id : LOOKUP_TABLE_ID

Errors: LookupTable, Value

Description:This request will delete the defined table entries in the lookup table resource specified by lut_id, between and including the entry specified by start and the entry specified by start+count-1.

PEX Version 5.1, 31-August-1992

5. Pipeline Contexts

______________________________________________________________________________________________ A pipeline contextis a PEX resource that contains an instance of the attributes that describe a rendering pipeline.

The attributes in a pipeline context are copied to a renderer resource whenever a PEXBeginRendering request is executed. This section describes pipeline context attributes and the operations that can be performed on pipeline context resources.

Some of the requests in this section affect attributes of a pipeline context. The item_maskand item_listparameters specify which components are to be affected. Each bit in the item_maskindicates whether or not the corresponding attribute is affected. In the cases where pipeline context attributes are being set or queried, there is a corresponding entry in the item_listfor each set bit in item_mask. It is therefore possible to affect one or many pipeline context attributes with a single request.

A name set resource ID is one of the attributes of a pipeline context. If a name set is created, bound to a pipeline context, and then freed, the contents of the name set will remain, since the contents are still being referenced by the pipeline context. However, when a pipeline context’s attributes are queried, the value AlreadyFreed will be returned for the name set ID, since it no longer has a valid resource ID by which it can be referenced.

The pipeline context components are listed in the following table.

Attribute Name Data Type Default Value

Marker attributes marker_type MARKER_TYPE MarkerAsterisk marker_scale FLOAT 1.0 marker_color COLOR_SPECIFIER {Indexed,1} marker_bundle_index TABLE_INDEX 1

Textattributes text_font_index TABLE_INDEX 1 text_precision TEXT_PRECISION String char_expansion FLOAT 1.0 char_spacing FLOAT 0.0 text_color COLOR_SPECIFIER {Indexed,1} char_height FLOAT 0.01 char_up_vector VECTOR_2D <0.0, 1.0> text_path TEXT_PATH PathRight text_alignment TEXT_ALIGNMENT {HalignNormal, ValignNormal} atext_height FLOAT 0.01 atext_up_vector VECTOR_2D <0.0, 1.0> atext_path TEXT_PATH PathRight atext_alignment TEXT_ALIGNMENT {HalignNormal, ValignNormal} atext_style ATEXT_STYLE ATextNotConnected text_bundle_index TABLE_INDEX 1

Lineand curve attributes line_type LINE_TYPE LineTypeSolid line_width FLOAT 1.0 line_color COLOR_SPECIFIER {Indexed,1} curve_approx CURVE_APPROX {1, 1.0} polyline_interp POLYLINE_INTERP PolylineInterpNone line_bundle_index TABLE_INDEX 1

Surface attributes interior_style INTERIOR_STYLE InteriorStyleHollow interior_style_index TYPE_OR_TABLE_INDEX 1

PEX Version 5.1, 31-August-1992 surface_color COLOR_SPECIFIER {Indexed,1} reflection_attr REFLECTION_ATTR {1.0, 1.0, 1.0, 0.0, 0.0, {Indexed,1}} reflection_model REFLECTION_MODEL ReflectionNoShading surface_interp SURFACE_INTERP SurfaceInterpNone bf_interior_style INTERIOR_STYLE InteriorStyleHollow bf_interior_style_index TYPE_OR_TABLE_INDEX 1 bf_surface_color COLOR_SPECIFIER {Indexed,1} bf_reflection_attr REFLECTION_ATTR {1.0, 1.0, 1.0, 0.0, 0.0, {Indexed,1}} bf_reflection_model REFLECTION_MODEL ReflectionNoShading bf_surface_interp SURFACE_INTERP SurfaceInterpNone surface_approx SURFACE_APPROX {1, 1.0, 1.0} culling_mode CULL_MODE None distinguish BOOLEAN False pattern_size VECTOR_2D {1.0, 1.0} pattern_ref_pt COORD_3D {0.0, 0.0, 0.0} pattern_ref_vec1 VECTOR_3D <1.0, 0.0, 0.0> pattern_ref_vec2 VECTOR_3D <0.0, 1.0, 0.0> interior_bundle_index TABLE_INDEX 1

Surface edge attributes surface_edges SWITCH Off surface_edge_type SURFACE_EDGE_TYPE SurfaceEdgeSolid surface_edge_width FLOAT 1.0 surface_edge_color COLOR_SPECIFIER {Indexed,1} edge_bundle_index TABLE_INDEX 1

Geometrytransformation attributes local_transform MATRIX identity global_transform MATRIX identity model_clip CLIP_INDICATOR NoClip model_clip_volume LISTofHALF_SPACE Null view_index TABLE_INDEX 0

Color transformation attributes light_state LISTofTABLE_INDEX Null depth_cue_index TABLE_INDEX 0 color_approx_index TABLE_INDEX 0 rdr_color_model COLOR_MODEL 0 psurf_char PSURF_CHAR {1, NULL}

ASFattributes asfs ASF_SPECIFIER {0, all Individual}

Miscellaneous attributes pick_id CARD32 0

HLHSR_identifier CARD32 0 name_set † NAME_SET_ID None

The bits in the asfs field of an ASF_SPECIFIER are defined as:

marker_type_asf ASF_VALUE Individual marker_scale_asf ASF_VALUE Individual marker_color_asf ASF_VALUE Individual text_font_index_asf ASF_VALUE Individual text_precision_asf ASF_VALUE Individual

__________________ † When pipeline context attributes are copied to a renderer (e.g., whenever a PEXBeginRendering request occurs), the actual contents of the name set resource is copied, and not the resource ID of the name set.

PEX Version 5.1, 31-August-1992 char_expansion_asf ASF_VALUE Individual char_spacing_asf ASF_VALUE Individual text_color_asf ASF_VALUE Individual line_type_asf ASF_VALUE Individual line_width_asf ASF_VALUE Individual line_color_asf ASF_VALUE Individual curve_approx_asf ASF_VALUE Individual polyline_interp_asf ASF_VALUE Individual interior_style_asf ASF_VALUE Individual interior_style_index_asf ASF_VALUE Individual surface_color_asf ASF_VALUE Individual reflection_model_asf ASF_VALUE Individual surface_interp_asf ASF_VALUE Individual reflection_attr_asf ASF_VALUE Individual bf_interior_style_asf ASF_VALUE Individual bf_interior_style_index_asf ASF_VALUE Individual bf_surface_color_asf ASF_VALUE Individual bf_reflection_model_asf ASF_VALUE Individual bf_surface_interp_asf ASF_VALUE Individual bf_reflection_attr_asf ASF_VALUE Individual surface_approx_asf ASF_VALUE Individual surface_edges_asf ASF_VALUE Individual surface_edge_type_asf ASF_VALUE Individual surface_edge_width_asf ASF_VALUE Individual surface_edge_color_asf ASF_VALUE Individual

The attributes of the pipeline context resource are defined as follows:

marker_type

This attribute contains the marker type to use when drawing marker primitives. See the "Extension

Information" section for descriptions of the registered marker types.

marker_scale

This attribute contains the marker scale factor to use when drawing marker primitives.

marker_color

This attribute contains the color value to use when drawing marker primitives.

marker_bundle_index

This attribute contains the lookup table index to be used to obtain bundled marker attributes from the marker bundle table.

text_font_index

This attribute contains the lookup table index to be used to obtain the font ID for drawing text and annotation text primitives.

text_precision

This attribute contains the text precision to use when drawing text and annotation text primitives.

char_expansion

This attribute contains the character expansion to use when drawing text primitives. The character expansion factor is the deviation of the width to height ratio of the characters from the ratio indicated by the font designer. PEX Version 5.1, 31-August-1992 char_spacing

This attribute contains the character spacing to use when drawing text primitives. Character spacing specifies how much additional space is to be inserted between two adjacent character bodies and is specified as a fraction of the font-nominal character height.

text_colorThis attribute contains the color value to use when drawing text and annotation text primitives.

char_heightThis attribute contains the character height to use when drawing text primitives. The character height is specified in modeling coordinates.

char_up_vector

This attribute contains the character up vector to use when drawing text primitives. The up vector is specified in the text local coordinate system. The axes of this coordinate system are determined by the direction vectors specified with the text primitive.

text_pathThis attribute contains the text path to use when drawing text primitives (i.e., the writing path of the text string).

text_alignment

This attribute contains the horizontal and vertical alignment to use when drawing text primitives.

atext_height

This attribute contains the character height to use when drawing annotation text primitives. The character height is specified in normalized projection coordinates.

atext_up_vector

This attribute contains the character up vector to use when drawing annotation text primitives. The up vector is specified in the annotation text local coordinate system, which is parallel to the display surface.

atext_pathThis attribute contains the text path to use when drawing annotation text primitives (i.e. the writing path of the annotation text string).

atext_alignment

This attribute contains the horizontal and vertical alignment to use when drawing annotation text primitives.

atext_styleThis attribute contains the annotation text style to use when drawing annotation text primitives. See the

"Extension Information" section for descriptions of the registered annotation text styles.

text_bundle_index

This attribute contains the lookup table index to be used to obtain bundled text attributes from the text bundle table.

line_typeThis attribute contains the type to use when drawing polyline and curve primitives. See the "Extension

Information" section for descriptions of the registered line types.

line_widthThis attribute contains the width to use when drawing polyline or curve primitives. This is the scale factor applied to the width of the polyline or curve primitive when it is to be rendered. Line width is applied in 2D raster coordinates after the primitive has been transformed from 3D space to 2D raster space.

line_colorThis attribute contains the color value to use when drawing polyline and curve primitives.

PEX Version 5.1, 31-August-1992 curve_approx

This attribute contains the curve approximation to use when drawing curve primitives. It sets the curve approximation method and the tolerance value for drawing curves. See the "Extension Information" section for descriptions of the registered curve approximation methods and how the curve tolerance is used with each type.

polyline_interp

This attribute contains the polyline interpolation method to use when drawing polyline primitives. See the

"Extension Information" section for descriptions of the registered polyline interpolation methods.

line_bundle_index

This attribute contains the lookup table index to be used to obtain bundled polyline and curve attributes from the line bundle table.

interior_style

This attribute contains the interior style to use when drawing surface primitives. See the "Extension

Information" section for descriptions of the registered interior styles.

interior_style_index

This attribute contains the index to use if the interior style is of type Pattern or Hatch. The interior style index contains the table index of the pattern table entry to be used when the interior style is Pattern, and the hatch table enumerated type index to be used when the interior style is Hatch.

surface_color

This attribute contains the color value to use when drawing surface primitives.

reflection_attr

This attribute contains the ambient coefficient; the diffuse coefficient; the specular coefficient, concentration, and color; and the transmission coefficient that are to be used in the light source shading computations when rendering surfaces (area-defining primitives). The specular color attribute provides an additional coefficient per primary for use in the specular reflection computation. This allows highlights to be computed that are some color other than that of the light source. The specular concentration defines the sharpness of the specular highlights or the "shininess" of a surface. This value is typically used as the exponent in the specular reflection term of lighting equations and it ranges from zero to the maximum floating point value. If specular_conc is zero, specular highlights are very broad. If specular_conc is much greater than zero, the highlights are very small and sharp, as if the surface was very shiny. The transmission coefficient indicates the amount of light that passes through a surface. A transmission coefficient of zero indicates that the surface is opaque (lets no light through). A transmission coefficient of 1.0 indicates that the surface is totally invisible

(lets all light through).

reflection_model

This attribute contains the reflection model to use when drawing surface primitives. See the "Extension

Information" section for descriptions of the registered reflection models.

surface_interp

This attribute contains the surface interpolation method to use when drawing surface primitives. See the

"Extension Information" section for descriptions of the registered surface interpolation methods.

bf_interior_style

This attribute contains the interior style to use when drawing backfacing surface primitives. See the

"Extension Information" section for descriptions of the registered interior styles.

bf_interior_style_index

This attribute contains the index to use for backfacing surface primitives if the interior style is of type Pattern or Hatch. The interior style index contains the table index of the pattern table entry to be used when the interior style is Pattern, and the hatch table enumerated type index to be used when the interior style is Hatch.

PEX Version 5.1, 31-August-1992 bf_surface_color

This attribute contains the color value to use when rendering backfacing surface primitives.

bf_reflection_attr

This attribute contains the reflection values to be used when rendering backfacing surfaces.

bf_reflection_model

This attribute contains the reflection model to use when drawing backfacing surface primitives. See the

"Extension Information" section for descriptions of the registered reflection models.

bf_surface_interp

This attribute contains the surface interpolation method to use when drawing backfacing surface primitives.

See the "Extension Information" section for descriptions of the registered surface interpolation methods.

surface_approx

This attribute contains the surface approximation and the tolerance to use when drawing surface primitives.

See the "Extension Information" section for descriptions of the registered surface approximation methods and of how the surface tolerance is used with each of them.

culling_mode

This attribute contains the culling mode that is used in processing backfacing surfaces. If the culling mode is

BackFaces, all back-facing surfaces will be culled and only front-facing surfaces will be rendered. If the culling mode is FrontFaces, all front-facing surfaces will be culled and only back-facing surfaces will be rendered. If the culling mode is None,both front- and back-facing polygons will be rendered.

distinguishThis attribute contains the distinguish mode that is used in processing backfacing surfaces. This flag selects whether back-facing surfaces are rendered with the back-face surface attributes or the front-face surface attributes. If distinguish is True, then back-face attributes are used to render the surface. If distinguish is

False, then front-face attributes are used to render the surface.

pattern_size

This attribute contains the pattern size to use when drawing surface primitives. It is specified in modeling coordinates. The value <x,0>will be used as the pattern width vector and the value <0,y>will be used as the pattern height vector. If the interior style is Pattern, the renderer attempts to use these values, plus the pattern reference point and the pattern reference vectors, to position, scale, and rotate the pattern on the surface.

pattern_ref_pt

This attribute contains the pattern reference point to use when drawing surface primitives. It is specified in modeling coordinates. When the interior style is Pattern, the renderer attempts to use the pattern reference point, reference vectors, and the pattern size to position and scale the pattern on the surface.

pattern_ref_vec1

This attribute contains the first of two pattern reference vectors to be used when interior style is Pattern. It is specified in modeling coordinates. When the interior style is Pattern, the renderer attempts to use the two pattern reference vectors, the pattern reference point, and the pattern size to position, scale, and rotate the pattern on the surface.

pattern_ref_vec2

This attribute contains the second of two pattern reference vectors to be used when interior style is Pattern. It is specified in modeling coordinates. When the interior style is Pattern, the renderer attempts to use the two interior_bundle_index

This attribute contains the lookup table index to be used to obtain bundled interior attributes from the interior

PEX Version 5.1, 31-August-1992 bundle table.

surface_edges

This attribute contains the surface edge flag attribute, which is used to enable or disable surface edge drawing.

If surface_edges is Off,surface edge drawing is disabled. If surface_edges is On, surface edge drawing is enabled. Surface edges are drawn using the surface edge color, surface edge type, and surface edge width.

surface_edge_type

This attribute contains the edge type to use when drawing surface edges. See the "Extension Information" section for descriptions of the registered surface edge types.

surface_edge_width

This attribute contains the edge width to use when drawing surface edges. This is the scale factor applied to the width of a surface edge when a surface edge is to be rendered. It is applied in 2D raster coordinates after a surface edge primitive has been transformed from 3D space to 2D raster space.

surface_edge_color

This attribute contains the color value to use when drawing surface edges.

edge_bundle_index

This attribute contains the lookup table index to be used to obtain bundled surface edge attributes from the surface edge bundle table.

local_transform

This attribute contains the local modeling transformation matrix that is used when drawing output primitives.

global_transform

This attribute contains the global modeling transformation matrix that is used when drawing output primitives.

model_clipThis attribute contains the model clipping flag that indicates whether or not to perform modeling clipping when drawing output primitives.

model_clip_volume

This attribute contains the model clipping volume that is used whenever modeling clipping is enabled.

view_indexThis attribute contains the lookup table index to be used to obtain viewing attributes from the view table.

light_stateThis attribute contains a list of table indices that specify those light sources that are enabled ("turned on").

Any light whose table index is not in this list is considered disabled ("turned off").

depth_cue_index

This attribute contains the lookup table index to be used to obtain bundled depth-cue attributes from the depth-cue bundle table.

color_approx_index

This attribute contains the lookup table index to be used to obtain the color approximation parameters from the color approximation table.

rdr_color_model

This attribute contains the rendering color model that is to be used during the interpolation of shaded primitives. See the "Extension Information" section for descriptions of the registered rendering color models.

psurf_charThis attribute contains the parametric surface characteristics that are to be used when rendering surfaces. The psc_typefield specifies the parametric surface characteristics type to be used when rendering surfaces. The psc_data field supplies additional data that may be used. See the "Extension Information" section for

PEX Version 5.1, 31-August-1992 descriptions of the registered parametric surface characteristics types.

asfs This attribute contains an aspect source flag (asf) for each attribute that can be obtained from a bundle lookup table. When rendering, if the value for an asf is set to Individual, the value for the corresponding attribute will be obtained directly from the current value within the renderer. If the value for the asf is set to Bundled,the value for the attribute will be obtained from the bundle lookup table. When setting asfs, a separate mask

(enables) is used to indicate which asfs are actually to be modified. The value to which an asf is to be modified will then be taken from the corresponding bit in the asfs bitmask. The enables field of the

ASF_SPECIFIER is meaningful only when creating or changing attributes of a pipeline context. During copying, all asf values are copied, and when queried, all asf values are returned and a value with all defined asfs set is returned for the enables bitmask. (This implies that it is not necessary to consider the enables field to be part of the state that is saved and restored while rendering.)

pick_idThis attribute contains the pick ID, which is used in conjunction with picking operations.

HLHSR_identifier

This attribute contains an HLHSR identifier. It is a noop for all registered HLHSR modes except ZBufferId.

When the renderer’s HLHSR_modeis set to ZBufferIdthen a zero value will disable z-buffering and a value of one will enable z-buffering. For non-registered HLHSR modes the meaning is implementation dependent.

Conceptually, this attribute is bound to all output primitives as they enter the rendering pipeline.

name_setThis attribute contains a reference to a name set resource. When attributes of a pipeline context are copied to a renderer, the contents of this name set are copied to the renderer.

PEX Version 5.1, 31-August-1992

5.1. Pipeline Context Resource Management

The pipeline context is an X11 resource and carries all of the responsibilities and access rights of X11 resources.

These requests manage the creation, freeing, and copying of pipeline contexts.

5.1.1. Create Pipeline Context

Name: PEXCreatePipelineContext

Request:fp_format : FLOAT_FORMAT pc_id : PIPELINE_CONTEXT_ID item_mask: PC_BITMASK item_list: LISTofVALUE

Errors: IDChoice, Value, FloatingPointFormat, ColorType, Alloc, NameSet

Description:This request creates a pipeline context resource for the specified pc_id. The item_maskdefines those pipeline context attributes that are to be explicitly set at the time the resource is created. The item_list contains the corresponding list of values used to modify the newly-created pipeline context. Floating point values in item_listwill be in the floating point format specified in fp_format. Similarly, color values in item_listwill be the color type specified by color_type.

5.1.2. Copy Pipeline Context

Name: PEXCopyPipelineContext

Request:src_pc_id : PIPELINE_CONTEXT_ID dest_pc_id : PIPELINE_CONTEXT_ID

Errors: PipelineContext, Value

Description:This request copies the source pipeline context src_pc_id to a destination pipeline context dest_pc_id. The dest_pc_id must already exist as a valid resource. The item_maskindicates which values in the pipeline context will be copied. PEX Version 5.1, 31-August-1992

5.1.3. Free Pipeline Context

Name: PEXFreePipelineContext

Request:pc_id : PIPELINE_CONTEXT_ID

Errors: PipelineContext

Description:This request deletes the association between the resource ID and the pipeline context. The pipeline context storage will be freed when no other resource references it.

PEX Version 5.1, 31-August-1992

5.2. Pipeline Context Inquiry

This section defines the requests that can be used to inquire pipeline context attributes.

5.2.1. Get Pipeline Context

Name: PEXGetPipelineContext

Request:fp_format : FLOAT_FORMAT pc_id : PIPELINE_CONTEXT_ID item_mask: PC_BITMASK

Reply: item_list: LISTofVALUE

Errors: PipelineContext, FloatingPointFormat, Value

Description:This request will return components of the pipeline context specified by pc_id. The item_maskspecifies which components are to be inquired and returned. The specified attributes of the pipeline context will be returned in item_list. Floating point values in item_listwill be returned in the floating point format specified in fp_format.

5.3. Pipeline Context Modification

This section defines the requests that can be used to modify attributes of pipeline context resources.

5.3.1. Change Pipeline Context

Name: PEXChangePipelineContext item_list: LISTofVALUE

Errors: PipelineContext, Value, FloatingPointFormat, ColorType, NameSet

Description:This request will modify components of the pipeline context specified by pc_id. The item_maskspecifies which components are to be modified. The values for the attributes that are to be modified are contained in item_list. Floating point values in item_listwill be in the floating point format specified in fp_format.

Similarly, color values in item_listwill be the color type specified by color_type.

PEX Version 5.1, 31-August-1992

6. Renderers

______________________________________________________________________________________________ A renderer is a PEX resource that can be created for the purpose of doing 3D rendering. A renderer consists of resource IDs for various tables and name sets, the resource ID of a pipeline context from which the initial rendering pipeline attributes will be copied, and other attributes. A renderer also manages the HLHSR buffer needed for some hidden line/hidden surface algorithms. A renderer is made ready for rendering by the PEXBeginRendering request

(a PEXBeginRendering is also performed implicitly as part of the PEXRenderNetwork request). A PEX implementation may choose to allow certain renderer attributes to be bound only at the time of a

PEXBeginRendering request or at anytime during the lifetime of the renderer. To obtain information about how renderer attributes are bound for a particular PEX implementation, the PEXGetRendererDynamics request should be used.

Some renderer resource requests require an item_maskparameter. Each bit in the item_maskindicates whether or not the corresponding attribute is to be set/queried. There is a corresponding entry in the item_listfor each set bit in item_mask. It is therefore possible to set/query one or many renderer attributes with a single request.

Any of a renderer’s attributes that are resource IDs that are not explicitly specified will be set to the default value of

Null when the renderer is created. During rendering operations, if a renderer makes an attempt to access an attribute from a lookup table whose resource ID is Null, the default attributes for the lookup table (as listed in Appendix D) will be used. If a renderer makes an attempt to read from a name set whose resource ID is Null, the result will be as if the name set was empty. If the renderer’s pipeline context attribute contains the resource ID Null, the default values for pipeline context attributes will be copied into the renderer whenever a PEXBeginRendering request is performed.

Pipeline context, lookup table, and name set resources can be bound to a renderer and then freed. When this happens, the contents of these resources will remain, since they are still being referenced by the renderer. However, when that renderer’s attributes are queried, the value AlreadyFreed will be returned for those resources that have been freed and thus no longer have a valid resource ID by which they can be referenced.

If a window that is associated with a renderer is destroyed or resized while the renderer is in the Rendering state, an implicit PEXEndRendering is performed by the server with flush equal to False in order to return the renderer to the Idle state. All subsequent output and traversal commands (e.g., PEXRenderOutputCommands,

PEXBeginStructure, PEXEndStructure, PEXRenderElements, and PEXAccumulateState) are ignored, up to and including the final PEXEndRendering. No errors are generated; however, at a subsequent

PEXBeginRendering, an Allocerror may be generated if an attempt to reallocate the z-buffer fails.

If a window that is associated with a renderer is moved, exposed, or occluded while the renderer is in the Rendering state, the server must continue to process output commands using the newly-modified window hierarchy until the next explicit or implicit PEXEndRendering occurs.

Whenever an implicit or explicit PEXBeginRendering occurs and the HLHSR_modeindicates z-buffering should be performed, a z-buffer suitable for use with the specified drawable will be allocated, if necessary, and bound to the renderer. (A new z-buffer is only allocated if a z-buffer does not exist for the renderer or, if the z-buffer which is bound to the renderer is not suitable for the current drawable.) If the z-buffer could not be allocated, an Allocerror is generated and the rendering is aborted. If clear_Z is enabled or, if a new z-buffer was allocated, then the z-buffer will be cleared to infinity in the region specified by the renderer’s current clip list. The value of infinity is implementation-dependent.

During rendering, primitives will be clipped by the renderer’s clip list. If z-buffering is enabled, primitives closer to the eye will be drawn over primitives that are further away. When primitives have the same z values, it is implementation-dependent which primitive will get drawn.

The z-buffer will not be deallocated when an explicit or implicit PEXEndRendering occurs. It remains bound to the renderer until the renderer is freed. When the next PEXBeginRendering occurs, an attempt will be made to

PEX Version 5.1, 31-August-1992 reuse the z-buffer. If it cannot be reused (for instance, if the previous and current drawable are a different size), it will be deallocated and a z-buffer suitable for the new drawable will be allocated.

The renderer components are listed in the following table. The abbreviation "imp. dep." means that the default value is implementation-dependent.

Attribute Name Data Type Default Value pipeline_context PIPELINE_CONTEXT_ID Null current_path LISTofELEMENT_REF Null renderer_state RENDERER_STATE Idle marker_bundle LOOKUP_TABLE_ID Null text_bundle LOOKUP_TABLE_ID Null line_bundle LOOKUP_TABLE_ID Null interior_bundle LOOKUP_TABLE_ID Null edge_bundle LOOKUP_TABLE_ID Null view_table LOOKUP_TABLE_ID Null color_table LOOKUP_TABLE_ID Null depth_cue_table LOOKUP_TABLE_ID Null light_table LOOKUP_TABLE_ID Null color_approx_table LOOKUP_TABLE_ID Null pattern_table LOOKUP_TABLE_ID Null text_font_table LOOKUP_TABLE_ID Null highlight_inclusion NAME_SET_ID Null highlight_exclusion NAME_SET_ID Null invisibility_inclusion NAME_SET_ID Null invisibility_exclusion NAME_SET_ID Null pick_inclusion NAME_SET_ID Null pick_exclusion NAME_SET_ID Null pick_start_path LISTofELEMENT_REF Null background_color COLOR_SPECIFIER {Indexed, 0} clear_I BOOLEAN False clear_Z BOOLEAN True echo_mode ECHO_MODE NoEcho

HLHSR_mode HLHSR_MODE 1

NPC_subvolume NPC_SUBVOLUME {(0.0,0.0,0.0),(1.0,1.0,1.0)} viewport VIEWPORT {imp. dep., imp. dep., True} clip_list LISTofDEVICE_RECT Null

The attributes of the renderer resource are defined as follows:

pipeline_context

This attribute specifies the resource ID of the pipeline context from which initial rendering pipeline attribute values will be copied whenever an explicit or implicit PEXBeginRendering request is executed.

current_path

This attribute contains a list of element references for keeping track of paths for client-side traversal.

renderer_state

This attribute contains the current state of the renderer. The renderer_state is set to Rendering whenever an explicit or implicit PEXBeginRendering request is processed, to Picking whenever an explicit or implicit

PEXBeginPickOne or PEXBeginPickAll request is processed, and to Idle whenever a explicit or implicit

PEXEndRendering, PEXEndPickOne or PEXEndPickAll request is processed.

marker_bundle

This attribute contains the resource ID of the marker bundle lookup table to be used when rendering.

PEX Version 5.1, 31-August-1992 text_bundleThis attribute contains the resource ID of the text bundle lookup table to be used when rendering.

line_bundleThis attribute contains the resource ID of the line bundle lookup table to be used when rendering.

interior_bundle

This attribute contains the resource ID of the interior bundle lookup table to be used when rendering.

edge_bundle

This attribute contains the resource ID of the edge bundle lookup table to be used when rendering.

view_tableThis attribute contains the resource ID of the view lookup table to be used when rendering.

color_tableThis attribute contains the resource ID of the color lookup table to be used to resolve references to indexed colors.

depth_cue_table

This attribute contains the resource ID of the depth-cue lookup table to be used when rendering.

light_tableThis attribute contains the resource ID of the light lookup table to be used when rendering.

color_approx_table

This attribute contains the resource ID of the color approximation lookup table to be used during the color approximation stage of the rendering pipeline.

pattern_table

This attribute contains the resource ID of the lookup table to be used when referencing patterns.

text_font_table

This attribute contains the resource ID of the lookup table to be used when referencing text fonts.

highlight_inclusion

This attribute contains the resource ID of the name set to be used as the highlight inclusion set.

highlight_exclusion

This attribute contains the resource ID of the name set to be used as the highlight exclusion set.

invisibility_inclusion

This attribute contains the resource ID of the name set to be used as the invisibility inclusion set.

invisibility_exclusion

This attribute contains the resource ID of the name set to be used as the invisibility exclusion set.

pick_inclusion

This attribute contains the resource ID of the name set to be used as the pick inclusion filter during picking.

pick_exclusion

This attribute contains the resource ID of the name set to be used as the pick exclusion filter during picking.

pick_start_path

This attribute contains a hierarchical path that indicates where to start the next server side "pick all" traversal.

PEXPickAll starts hit testing at the next element after the one specified by this path. PEXPickAll and

PEXEndPickAll both set this attribute to the path of the last element processed during the "pick all" traversal.

background_color

This attribute contains the color value to use when clearing the image buffer. The image buffer is cleared by

PEX Version 5.1, 31-August-1992

PEXBeginRendering when clear_I is enabled. The color_approx_index in the initial pipeline context is used to map the color to a pixel value.

clear_IThis attribute indicates whether the image buffer should be cleared to the background color at

PEXBeginRendering. Only pixels within the renderer’s clip list are cleared.

clear_ZThis attribute indicates whether the z-buffer should be cleared to infinity (the value used for infinity is platform dependent) at the start of rendering. Only pixels within the renderer’s clip list are cleared. This attribute is ignored if the HLHSR_modedoes not require a z-buffer.

echo_modeThis attribute indicates whether primitives should be echoed, unechoed or drawn normally. The method used for echoing and unechoing primitives is implementation dependent and there is no guarantee that the method employed will preserve temporal priority. Echoing takes precedence over highlighting. It is recommended, but not required, that the echo and highlight methods are visually distinct.

HLHSR_mode

This attribute contains the hidden line/hidden surface method used when resolving visibility of overlapping primitives. The PEXGetRendererDynamics request can be used to determine whether changing the

HLHSR_modewhile the renderer_state attribute is set to Rendering has any effect.

NPC_subvolume

This attribute contains the normalized project coordinates for the sub-volume space that is to be mapped to the viewport.

viewportThis attribute is used to describe the area within a drawable in which 3D graphics primitives may appear. The viewport coordinates are specified in device coordinates, which have an x,y offset (in pixels) from the lower left corner of the drawable. It is permissible to specify a viewport with boundaries outside of the drawable.

Geometry that is mapped to values outside the drawable will be clipped. Viewport z values must be in the range [0-1.0], where z=0 maps to the device-coordinate z value representing objects that are furthest from the viewing position, and z=1 maps to the device-coordinate value representing objects that are closest to the viewing position. Depending on the dynamics of the viewportattribute (see PEXGetRendererDynamics), the values that define a viewport may be bound at any time, or they may take effect only at the time of a

PEXBeginRendering. Whenever the viewport values are bound, the viewport’s use_drawable flag is examined first. If it is set to True, the viewport width and height are obtained from the drawable’s current width and height and the viewport z values are obtained from the values specified in the viewport structure. If the use_drawable flag is False, the viewport width, height and z values are all set to the values in the viewport structure. The viewport is then set to the largest rectangle, anchored at the lower left corner, that achieves an isotropic mapping to the renderer’s NPC_subvolume. The viewport will remain in the same position relative to the lower left hand corner of the drawable after a resize event has occurred.

clip_listThis attribute contains a list of rectangles in device coordinates that define the portions of the drawable in which rendering is enabled. If the list is Null, then all of the pixels on the drawable may be overwritten during rendering. If the list is not Null, the renderer may only render on those pixels that are within the rectangles in the list. The rectangles should be non-overlapping, or the graphics results will be undefined. Pixels that are outside of all of the rectangles in clip_list are effectively "write-protected". The rectangles in the clip list are defined by xmin,ymin,xmax,and ymaxwhich are in device coordinates. (0,0) is at the lower left hand corner of the window and the xmaxand ymaxvalues are inclusive. These rectangles will remain in the same position relative to the lower left hand corner of the drawable after a resize has occurred. (Note: If a z-buffering algorithm is used, only those pixels under the rectangles in the clip list will have their z values initialized when a PEXBeginRendering or a PEXRenderNetwork request is issued.)

PEX Version 5.1, 31-August-1992

6.1. Renderer Resource Management

The renderer is an X11 resource and carries all of the responsibilities and access rights of X11 resources. These requests manage the creation and freeing of renderer resources.

6.1.1. Create Renderer

Name: PEXCreateRenderer

Request:fp_format : FLOAT_FORMAT rdr_id : RENDERER_ID drawable_example : DRAWABLE_ID item_mask: BITMASK item_list: LISTofVALUE

Errors: IDChoice, Drawable, PipelineContext, NameSet, LookupTable, FloatingPointFormat, Value, Alloc, Match

Description:This request creates a renderer resource for the specified rdr_id. It can be used to render onto drawables with the same root window and depth as the example drawable specified by drawable_example. The item_maskdefines those renderer attributes that are to be explicitly set at the time the resource is created.

The item_listcontains the corresponding list of values used to modify the newly-created renderer. Floating point values in item_listwill be in the floating point format specified in fp_format.

6.1.2. Free Renderer

Name: PEXFreeRenderer

Request:rdr_id : RENDERER_ID

Errors: Renderer

Description:This request deletes the specified renderer resource and frees the storage associated with it. If the renderer’s renderer_state attribute is set to Rendering when this request is processed, an implicit PEXEndRendering request with flush equal to False will be performed before the renderer is freed. If the renderer’s renderer_state attribute is set to Picking when this request is processed, the pick operation will be aborted.

PEX Version 5.1, 31-August-1992

6.2. Renderer Modification

The requests in this section can be used to modify attributes of renderer resources.

6.2.1. Change Renderer

Name: PEXChangeRenderer

Request:fp_format : FLOAT_FORMAT rdr_id : RENDERER_ID item_mask: BITMASK item_list: LISTofVALUE

Errors: Renderer, Match, Value, FloatingPointFormat, NameSet, LookupTable, PipelineContext

Description:This request changes components of a renderer. The item_maskand item_listspecify which components are to be changed. Each bit in the item_maskindicates whether or not there is a corresponding entry in the item_list. It is therefore possible to modify one or many renderer attributes with a PEXChangeRenderer request. A renderer’s current_path and renderer_state attribute are read-only, therefore attempts to modify them will be ignored. Floating point values in item_listwill be in the floating point format specified in fp_format.

6.3. Renderer Inquiry

The requests in this section can be used to inquire renderer attributes.

6.3.1. Get Renderer Attributes

Name: PEXGetRendererAttributes

Reply: item_list: LISTofVALUE

Errors: Renderer, FloatingPointFormat, Value

Description:This request will return components of the renderer specified by rdr_id. The item_maskspecifies which components are to be inquired and returned. The specified attributes of the renderer will be returned in item_list. Floating point values in item_listwill be returned in the floating point format specified in fp_format. (The values returned are those that were last set by the client. Depending on the dynamics of the renderer, these may or may not be the values currently in use. See PEXGetRendererDynamics.)

PEX Version 5.1, 31-August-1992

6.3.2. Get Renderer Dynamics

Name: PEXGetRendererDynamics

Request:rdr_id : RENDERER_ID

Reply: tables : BITMASK namesets : BITMASK attributes : BITMASK

Errors: Renderer

Description:This request will return the dynamics (binding times) for all of the attributes of the specified renderer. The tables bitmask has the following bits defined:

MarkerBundle MarkerBundleContents

TextBundle TextBundleContents

LineBundle LineBundleContents

InteriorBundle InteriorBundleContents

EdgeBundle EdgeBundleContents

ViewTable ViewTableContents

ColorTable ColorTableContents

DepthCueTable DepthCueTableContents

LightTable LightTableContents

ColorApproxTable ColorApproxTableContents

PatternTable PatternTableContents

TextFontTable TextFontTableContents

The namesets bitmask has the following bits defined:

HighlightNameset HighlightNamesetContents

InvisibilityNameset InvisibilityNamesetContents

PickNameset PickNamesetContents

The attributes bitmask has the following bits defined:

HLHSRMode

NPCSubvolume

Viewport

ClipList

EchoMode

For each defined bit, a value of zero indicates that the specified attribute is dynamicand a value of one indicates that it is not. Changes to dynamicattributes take effect immediately. Attributes which are not dynamiccan be modified at any time but the new value will not take effect until the next explicit or implicit

PEXBeginRendering occurs. Implementations that allow attributes such as HLHSRModeto be dynamic must specify the semantics of changing between all possible supported values for that attribute.

PEX Version 5.1, 31-August-1992

6.4. Client-Side Traversal Support

These requests provide support for client-side structure traversal. See section on Renderer Picking for requests to do client side picking. Client-side search traversals are not supported.

6.4.1. Begin Rendering

Name: PEXBeginRendering

Request:rdr_id : RENDERER_ID drawable_id : DRAWABLE_ID

Errors: Renderer, Drawable, Match, Alloc, RendererState

Description:This request causes rendering to begin on the drawable specified by drawable_id. The output of the renderer specified by rdr_id is bound to that drawable until a PEXEndRendering request is processed.

The initial rendering pipeline attributes are copied into the renderer from the pipeline context specified by the renderer’s pipeline_contextattribute. If pipeline_contextis Null, the default values for all of the attributes in a pipeline context are copied into the renderer instead. The renderer’s renderer_state attribute is set to Rendering and its current_path attribute is initialized to structure id zero with an element offset of zero. If clear_I is enabled then the image buffer will be cleared to background_color. If clear_Z is enabled and the HLHSR_modeindicates that z-buffering should be performed, then the z-buffer will be cleared to infinity. The image and z-buffer are cleared only in the region specified by clip_list.

If the specified drawable does not have the same root and depth as the drawable that was passed in to create the renderer, or, if the specified drawable is not one of the supported drawables returned by

PEXMatchRendererTargets, a Match error will be generated.

If renderer_state is currently Rendering or Picking, the operation is aborted, the PEXBeginRendering request is executed, and a RendererState error is returned.

6.4.2. End Rendering

Name: PEXEndRendering flush : BOOLEAN

Errors: Renderer, RendererState

Description:This request terminates the current rendering operation for the renderer specified by rdr_id. If flush is True, all pending output will be rendered onto the drawable. If flush is False, all pending output is discarded. In

PEX Version 5.1, 31-August-1992 either case, the renderer_state attribute of the renderer is set to Idle. If the renderer_state attribute is currently Idle (i.e., no rendering is in progress or the rendering was aborted due to a resize), the request is ignored and no error is generated. If the renderer_state is currently Picking then a RendererState error will be generated.

6.4.3. Begin Structure

Name: PEXBeginStructure

Request:rdr_id : RENDERER_ID s_id : CARD32

Errors: Renderer

Description:If the renderer_state attribute of the renderer specified by rdr_id is set to Rendering or Picking, then this request causes the pipeline attributes of the renderer to be saved. If the renderer_state attribute is set to

Idle, then this request is ignored. The attributes of the renderer resource itself (i.e., the attributes of a renderer that can be set/queried, including table and name set resource IDs) are not saved. The element offset of the last entry in the renderer’s current_path is incremented (to account for the client-side "execute structure" command), then the name specified by s_id together with an element offset of zero (indicating an empty structure) is appended to the current_path attribute. Each subsequent output command will cause the element offset to be incremented by one until the next PEXBeginStructure request or the next

PEXEndStructure request.

After saving the current rendering pipeline attributes, the global_transform attribute is set to the matrix computed by concatenating the current local_transform and the current global_transform matrices. Then the local_transform matrix is set to the identity matrix.

6.4.4. End Structure

Name: PEXEndStructure

Errors: Renderer, RendererState request restores the last-saved pipeline attributes in the renderer. If the renderer_state attribute is set to

Idle, then this request is ignored. In addition, the last element reference in the renderer’s current_path is removed, and subsequent output commands will cause the element offset of the element reference at the end of the list to be incremented. This request itself does not cause an increment to current_path.

PEX Version 5.1, 31-August-1992

6.5. Rendering Commands

These requests cause output commands to be processed by a renderer.

6.5.1. Render Output Commands

Name: PEXRenderOutputCommands

Request:fp_format : FLOAT_FORMAT rdr_id : RENDERER_ID cmds: LISTofOUTPUT_CMD

Errors: Renderer, FloatingPointFormat, OutputCommand

Description:If the renderer_state attribute of the renderer specified by rdr_id is set to Rendering or Picking, the output commands in cmdswill be immediately processed. If the renderer_state attribute is set to Idle, the commands will be ignored. Floating point values in cmdswill be in the floating point format specified in fp_format. The formats for the various types of output commands can be found Section 3 - Output

Commands. Output commands are processed by the server in order until one is found to be in error, or until the entire list has been processed. The erroneous output command and all others following it in the request are ignored, and an OutputCommanderror is returned to the client. The current_path attribute of the renderer is updated to reflect only those output commands actually processed.

6.5.2. Render Elements

Name: PEXRenderElements

Request:rdr_id : RENDERER_ID s_id : STRUCTURE_ID range : ELEMENT_RANGE

Errors: Renderer, Structure, Value

Description:If the renderer_state attribute of the renderer specified by rdr_id is set to Rendering or Picking, then this request causes a range of structure elements in the structure specified by s_id to be processed using the specified renderer. If the renderer_state attribute is set to Idle, then this request is ignored. The semantics of this request are the same as for PEXRenderOutputCommands except that the output commands are taken from the specified structure.

The offsets that define the range of elements to be rendered are computed using the positions in range in the following fashion. If whenceis Beginning,the computed offset is just the value specified by offset. If whenceis Current, the offset is computed by adding offsetto s_id’s element pointer. If whenceis End, the offset is computed by adding offsetto the number of elements in the structure. Offsetcan be a negative number. PEX Version 5.1, 31-August-1992

If either computed offset is less than zero, it will be set to zero before the rendering occurs. If either computed offset is greater than the number of elements in the structure, it will be set to the offset of the last structure element. The structure’s element pointer is not affected by this request.

6.5.3. Accumulate State

Name: PEXAccumulateState

Request:rdr_id : RENDERER_ID path : LISTofELEMENT_REF

Errors: Renderer, Path

Description:If the renderer_state attribute of the renderer specified by rdr_id is set to Rendering or Picking, this request accumulates the state that would be in effect if a traversal were done to the element specified by path. If the renderer_state attribute is set to Idle, then this request is ignored.

Accumulation of state begins with the current pipeline attributes. A linear descent down the specified path is then made and the structure elements that lie along the specified path are examined in order. Any element that contains an output command that would modify pipeline state (such as Set Line Color) is sent to the renderer for processing. All other output commands (such as PolyLine 3D, Execute Structure,

Label, etc) are skipped. The traversal is flat meaning that the current pipeline attributes will not get

"pushed" when a structure in the path is executed. However, the current path offset is bumped for each output command that is encountered during accumulate state.

6.5.4. Render Network

Name: PEXRenderNetwork drawable_id : DRAWABLE_ID s_id : STRUCTURE_ID

Errors: Renderer, Drawable, Structure, Match, Alloc, RendererState

Description:This request causes the structure network rooted at s_id to be traversed and rendered on drawable_id, using the renderer specified by rdr_id.

This functionality is equivalent to the following (pseudo-)requests:

PEXBeginRendering(rdr_id, drawable_id)

PEXRenderElements(rdr_id, s_id, all elements of s_id)

PEXEndRendering(rdr_id, True)

PEX Version 5.1, 31-August-1992

7. Renderer Picking

______________________________________________________________________________________________ The semantics of picking are identical to rendering except that during picking primitives are hit tested instead of converted to pixels. In other words, all primitives which are passed to the rendering pipeline (ie: they do not satisfy the invisibility filter and they are not culled backfaces) are eligible for picking. Picking uses the geometric definition of primitives so it is possible for hollow, empty and transparent polygons to be picked. However it is implementation dependent whether rendering effects which increase the area of the primitive (such as linewidth) are considered.

Two types of hit test traversals are supported: "pick one" and "pick all". A pick one traversal will return at most one primitive which satisfies the pick criteria. A "pick all" traversal will return all primitives which satisfy the pick criteria, up to a user specified maximum number of hits. For both types of traversals the spatial test which is performed on the primitives is controlled by the hit box which is specified in pick_data.

The hit box may be specified in device coordinates (if the server supports DC_HitBoxpick devices) or in NPC space

(if the server supports NPC_HitVolumepick devices). The supported pick device types can be inquired via

PEXGetEnumeratedTypeInfo. A device coordinate hit box is specified by a pick_positionand a pick_distance.

The pick_positionis the device coordinate center for the hit box and the shape of the hit box (ie: square, rectangle, circle) is implementation dependent. pick_distance, also measured in device coordinates, defines the half-width or radius of the hit box. The NPC hit volume is specified by two points in NPC space. Primitives that lie within or intersect the hit box are considered "hit".

The pick_methoddetermines which "hit" primitives will be picked. For pick one, pick_methodcan be set to: Last,

ClosestZ, VisibleAny,or VisibleClosest. For pick all, pick_methodcan be set to: Allor Visible. An error will be returned if the specified pick_methodis not supported on the connection. The supported pick one and pick all methods can be inquired using PEXGetEnumeratedTypeInfo. PEX servers are required to support Last for pick one and Allfor pick all.

The pick_inclusionand pick_exclusionrenderer attributes specify the name sets to be used to filter picked primitives after a pick traversal. The pick requests will only return primitives which are not excluded by the pick filter. If possible, pick one will return a primitive which most closely satisfies the pick criteria and also passes the pick filter test. A flag is returned from pick one requests to indicate whether a primitive which did not satisfy the pick filter was a better candidate with the specified pick_method. The dynamics of pick_inclusionand pick_exclusioncan be determined by calling PEXGetRendererDynamics.

During a pick one traversal at most one primitive is picked. If the pick_methodis Last then the last "hit" primitive which satisfies the pick filter test is returned. If the pick_methodis ClosestZ then the "hit" primitive which has a z value closest to the front clipping plane and satisfies the pick filter is returned. If multiple primitives satisfy this criteria then any of them may be returned. If the pick_methodis VisibleAnythen any "hit" primitive which is visible

(taking the current HLHSR mode into account) and satisfies the pick filter may be returned. If the pick_methodis

VisibleClosestthen all "hit" primitives which are visible are first selected. Of the selected primitives, the one which is closest to the pick_positionand satisfies the pick filter is returned. If an NPC hit volume was specified then the pick_positionis the center of the volume. The z buffer contents may not be preserved when using the "visible" pick methods.

The "visible" pick methods only return primitives which would be visible in the pick aperature if they were rendered using the renderer’s current HLHSR mode. For example, if the HLHSR mode is set to ZBuffer,the pick one method

ClosestZ may return a primitive which is occluded by another primitive which does not satisfy the pick filter test.

However, pick one method VisibleAnyguarantees that the picked primitive is not occluded.

During a "pick all" traversal multiple primitives may be picked. If the pick_methodis Allthen the first max_hits primitives, which lie within or intersect the hit box, are returned. If the pick_methodis Visiblethen the first max_hitsprimitives which are visible (taking the current HLHSR mode into account) and lie within or intersect the hit box, are returned. Pick first can be accomplished by setting max_hitsequal to one.

PEX Version 5.1, 31-August-1992

PickAllis further controlled by the pick_start_path renderer attribute. pick_start_path indicates where to begin the next PickAlltraversal and it is bound at the start of a PickAlltraversal.

If the drawable that is associated with a renderer is destroyed or resized while the renderer is performing a pick one or pick all hit test, the pick operation is terminated and the renderer is returned to the Idle state. All subsequent output and traversal commands (e.g., PEXRenderOutputCommands, PEXBeginStructure, PEXEndStructure,

PEXRenderElements, and PEXAccumulateState) are ignored until the final PEXEndPickOne or

PEXEndPickAll request is received. No errors are generated but pick_status will be set to Abortedin the pick reply.

If the drawable that is associated with a renderer is moved, exposed, or occluded while the renderer is performing a pick one or pick all hit test, the server must continue to process output commands using the newly-modified window hierarchy until the pick operation is explicitly or implicitly terminated.

PEX Version 5.1, 31-August-1992

7.1. Pick One

7.1.1. Begin Pick One

Name: PEXBeginPickOne

Request:fp_format : FLOAT_FORMAT pick_method: PICK_ONE_METHOD rdr_id : RENDERER_ID drawable_id : DRAWABLE_ID s_id : INT32 pick_data : PICK_RECORD

Errors: Renderer, Drawable, Match, Alloc, RendererState, Value

Description:This request starts a client side pick one traversal. When a renderer is in "pick one" mode, primitives will be hit tested instead of converted to pixels and, a hierarchical path to the picked primitive will be maintained. pick_methodspecifies the pick criteria to use so that only one primitive will be selected. It may be set to Last, ClosestZ, VisibleAny,or VisibleClosest. (PEXBeginPickAll will return the First picked primitive when max_hitsis set to one.) If the specified pick_methodis not supported then a Valueerror will be returned.

The pick aperature is defined by pick_data. Either a DC_HitBoxor NPC_HitVolumecan be specified.

s_id is the root of the client structure network. The current path is initialized to structure s_id and element offset zero before the pick traversal begins. The pick path which is returned from a pick one traversal is equivalent to the renderer’s current path at the time the picked primitive was processed.

If the specified drawable does not have the same root and depth as the drawable that was passed in to create the renderer, or, if the specified drawable is not one of the supported drawables returned by

PEXMatchRendererTargets, a Match error will be generated. If the renderer_state is set to Rendering or

Picking, then the operation will be aborted, the PEXBeginPickOne request will be executed, and a

RendererState error returned.

The existing PEX requests that process output commands or manipulate the current attributes (ie:

PEXRenderOutputCommands, PEXBeginStructure, PEXEndStructure, PEXRenderElements, and

PEXAccumulateState) can be issued when the renderer is in Picking mode. They will have the same semantics except that primitives are hit tested instead of converted to pixels.

PEX Version 5.1, 31-August-1992

7.1.2. End Pick One

Name: PEXEndPickOne

Request:rdr_id : RENDERER_ID

Reply: pick_status : PICK_STATUS better_pick : BOOLEAN pick_path : LISTofPICK_ELEMENT_REF

Errors: Renderer, RendererState

Description:This request places the renderer in Idle mode and returns the pick status along with the hierarchical pick path. If a primitive was picked, then pick_status will be set to Okand pick_path will contain the renderer’s current path at the time the picked primitive was processed. If no primitive was picked then pick_status will be set to NoPickand pick_path will be empty. If the renderer’s drawable was destroyed or resized during the pick operation then pick_status will be set to Abortedand pick_path will be empty.

If there was a primitive which more closely satisfied the pick criteria but did not pass the pick filter test then better_pick will be set to True. Otherwise better_pick will be set to False.

If the renderer_state is Idle when this request is received (i.e., no picking is in progress or picking was aborted due to a resize), then this request is ignored but no error is generated. If the renderer_state is

Rendering or a "pick all" is in progress then a RendererState error will be generated.

7.1.3. Pick One

Name: PEXPickOne

Request:fp_format : FLOAT_FORMAT pick_method: PICK_ONE_METHOD rdr_id : RENDERER_ID drawable_id : DRAWABLE_ID s_id : STRUCTURE_ID pick_data : PICK_RECORD

Errors: Renderer, Drawable, Structure, Match, Alloc, RendererState, Value

Description:This request causes a pick one traversal to be performed on the structure network rooted at s_id. It returns the pick status along with the hierarchical pick path.

PEX Version 5.1, 31-August-1992

This request is equivalent to the following (pseudo-)requests:

PEXBeginPickOne(pick_method, rdr_id, drawable_id, s_id, pick_data)

PEXRenderElements(rdr_id, s_id, all elements of s_id)

PEXEndPickOne(rdr_id)

7.2. Pick All

7.2.1. Begin Pick All

Name: PEXBeginPickAll

Request:fp_format : FLOAT_FORMAT pick_method: PICK_ALL_METHOD send_event: BOOLEAN rdr_id : RENDERER_ID drawable_id : DRAWABLE_ID s_id : INT32 pick_max_hits: CARD32 pick_data : PICK_RECORD

Errors: Renderer, Drawable, Match, Alloc, RendererState, Value

Description:This request starts a client side "pick all" traversal. When the renderer is in "pick all" mode, primitives are hit tested instead of converted to pixels. All picked primitives are recorded until pick_max_hitsis reached.

Additional primitives will not be recorded. Once the the maximum number of hits is reached, the server may choose to ignore all subsequent primitives. When max_hitsis set to one this request will return the

First picked primitive.

pick_methodspecifies the pick criteria to use during the "pick all" traversal. It may be set to Allor Visible.

If the specified pick_methodis not supported then a Valueerror will be returned.

The pick aperature is defined by pick_data. Either a DC_HitBoxor NPC_HitVolumecan be specified.

s_id is the root of the client structure network. The current path is initialized to structure s_id and element offset zero before the pick traversal begins. All pick paths which are returned from a "pick all" traversal are equivalent to the renderer’s current path at the time the picked primitive was processed.

If send_eventis True and pick_methodis All,then a MaxHitsReached event will be sent to the client whenever the maximum number of hits is reached by the server. (If the pick_methodis Visiblethen a complete traversal must be performed before any primitives can be picked.) Upon receiving the event, the client should end the traversal and see if the recorded hits are sufficient. PEXGetImpDepConstants returns a flag indicating whether this event is supported by the server.

If the specified drawable does not have the same root and depth as the drawable that was passed in to create the renderer, or, if the specified drawable is not one of the supported drawables returned by

PEXMatchRendererTargets, a Match error will be generated. If the renderer_state is Rendering or

Picking, then the operation will be aborted, the PEXBeginPickAll request will be executed, and a

RendererState error returned.PEX Version 5.1, 31-August-1992

7.2.2. End Pick All

Name: PEXEndPickAll

Request:rdr_id : RENDERER_ID

Reply: pick_status : PICK_STATUS more_picks: PICK_ALL_STATE pick_paths : LISTofLISTofPICK_ELEMENT_REF

Errors: Renderer, RendererState

Description:This request terminates the current client side "pick all" traversal, places the renderer in Idle mode, and returns the pick status along with the pick paths of any picked primitives. If one or more primitives were picked, then pick_status will be set to Okand pick_paths will contain a hierarchical path for each picked primitive, stored in traversal order. The hierarchical pick path is equivalent to the renderer’s current path at the time the picked primitive was processed. If no primitives were picked then pick_status will be set to

NoPickand pick_paths will be empty. If the renderer’s drawable was destroyed or resized during the pick operation then pick_status will be set to Abortedand pick_paths will be empty.

If all picks were recorded then more_pickswill be set to NoMoreHitsand the renderer’s pick_start_path attribute will be empty. If the maximum number of hits was reached and additional picks were detected, then more_pickswill be set to MoreHits and pick_start_path will be set to the last picked primitive which was recorded. If the server, after reaching the maximum number of hits, started ignoring all subsequent output commands, then more_pickswill be set to MayBeMoreHitsand pick_start_path will be set to the last element processed by the renderer before it started ignoring primitives.

If the renderer_state is Idle when this request is received (i.e., no picking is in progress or picking was aborted due to a resize), then this request is ignored but no error is generated. If the renderer_state is

Rendering or a "pick one" is in progress then a RendererState error will be generated.

7.2.3. Pick All

Name: PEXPickAll

Request:fp_format : FLOAT_FORMAT pick_method: PICK_ALL_METHOD rdr_id : RENDERER_ID drawable_id : DRAWABLE_ID pick_max_hits: CARD32 pick_data : PICK_RECORD

PEX Version 5.1, 31-August-1992

Errors: Renderer, Drawable, Match, Alloc, RendererState, Value, Path

Description:This request traverses the structure network specified in the renderer’s pick_start_path attribute. Hit testing begins after the last element specified in pick_start_path and continues until one of two conditions is met:

pick_max_hitsprimitives are picked or the last element of the first structure in pick_start_path is processed.

If the start path does not define a valid hierarchical path, a Path error is generated and no results are returned.

The pick aperature is defined by pick_data. Either a DC_HitBoxor NPC_HitVolumecan be specified.

The paths of all hit primitives are recorded until pick_max_hitsis reached. These paths are returned in traversal order in pick_paths. Once the maximum number of paths is recorded, the server may choose to ignore subsequent primitives and return the results found. When max_hitsis set to one this request will return the First picked primitive.

If all possible hits were recorded then more_pickswill be set to NoMoreHitsand the renderer’s pick_start_path attribute will be empty. If the maximum number of hits was reached and additional hits were detected, then more_pickswill be set to MoreHits and pick_start_path will be set to the last picked primitive which was recorded. If the server, after reaching the maximum number of hits, started ignoring all subsequent output commands, then more_pickswill be set to MayBeMoreHitsand pick_start_path will be set to the last element processed by the renderer before it started ignoring primitives.

PEX Version 5.1, 31-August-1992

8. Structures

______________________________________________________________________________________________ This section details the usage and management of structure resources. A structure is a resource which stores output commands for later execution. Structures have two settable attributes and a number of attributes that can only be inquired. The modifiable attributes are:

element_ptrThis attribute contains the offset of an element in the structure. Elements are numbered consecutively, starting at offset one. The element pointer determines the position in the structure at which the next editing or element query operation will occur. Whenever a structure is used as a destination in a structure editing request, its element pointer attribute will be updated as a side effect of the operation. When a structure is created, its element pointer is set to zero.

editing_mode

The editing mode attribute specifies how editing operations will affect the structure. If the mode is

StructureInsert, subsequent requests to create structure elements will cause elements to be inserted into the structure. Elements will be inserted into the structure after the structure element specified by the element pointer. The element pointer will then be incremented by the number of elements inserted. If the mode is

StructureReplace, output requests used to create structure elements will cause structure elements to replace elements starting at the location specified by the element pointer. When a structure is created, its editing mode is set to StructureInsert.

A structure’s non-modifiable attributes include its size (number of elements and length in four byte units if it were to be returned to the client) and the number of times it is referenced by other structures. Additional information about structures (ancestors, descendants, etc.) is also available and can be inquired separately.

8.1. Structure Resource Management

A structure is an X11 resource and carries all of the responsibilities and access rights of X11 resources. These requests manage the creation, deletion, and general manipulation of structures.

8.1.1. Create Structure

Name: PEXCreateStructure

Request:s_id : STRUCTURE_ID

Errors: IDChoice, Alloc

Description:This request creates a structure resource with the specified s_id.

PEX Version 5.1, 31-August-1992

8.1.2. Copy Structure

Name: PEXCopyStructure

Request:src_s_id : STRUCTURE_ID dest_s_id : STRUCTURE_ID

Errors: Structure

Description:The structure elements in src_s_id are copied to dest_s_id. Any structure elements in dest_s_id are deleted prior to the copy operation. The destination structure must already exist as a valid resource. Src_s_id’s element pointer and editing mode are also copied to dest_s_id.

8.1.3. Destroy Structures

Name: PEXDestroyStructures

Request:list : LISTofSTRUCTURE_ID

Description:This request destroys each of the structure resources that is specified in list and removes all references to it in the server. Any structure elements that reference a structure in list will be destroyed, and any structure in list that is posted to a PHIGS workstation resource will be unposted. Any paths in search contexts or pick measures that contain the resource ID of any structure in list may still be queried. Such paths may still contain the resource ID of a structure after it has been destroyed. However, any attempts to perform a

PEXSearchNetwork or a PEXUpdatePickMeasure using such a path will result in a Path error being generated.

Any structure that had structure elements removed due to a PEXDestroyStructures request will have their element pointer modified in the following way. If the element pointer is at a position before any of the elements that were deleted, the element pointer remains unchanged. If the element pointer was at the position of an element that was deleted, it will be set to the previous element. If the element pointer was after elements that were deleted, it will be updated so as to point at the same element it pointed to prior to the PEXDestroyStructures request.

PEX Version 5.1, 31-August-1992

8.2. Structure Inquiry

These requests inquire attributes and other information about structures.

8.2.1. Get Structure Info

Name: PEXGetStructureInfo

Request:fp_format : FLOAT_FORMAT s_id : STRUCTURE_ID item_mask: BITMASK_SHORT

Reply: editing_mode: EDIT_MODE element_ptr : CARD32 num_elements: CARD32 total_length : CARD32 has_refs : BOOLEAN

Errors: Structure, FloatingPointFormat, Value

Description:This request returns information about the structure specified by s_id. Item_maskindicates which fields in the reply are required by the client. Items indicated by item_maskwill have valid values returned, and the remaining values will be returned as undefined values. The current value of the structure’s editing mode attribute will be returned in editing_mode.The current value of the structure’s element pointer attribute will be returned in element_ptr. The number of structure elements in the specified structure will be returned in num_elements. If the structure is empty, num_elementswill be zero. The total number of four-byte units necessary to store all elements of the structure (on the client side) will be returned in total_length. (This provides the client the information needed to allocate memory prior to doing a PEXFetchElements request.) If there are any "execute structure" elements in other structure resources that reference s_id, has_refs will be returned as True, otherwise it will be returned as False. The information returned will be computed as if the floating point type in fp_format were being used to return the data.

PEX Version 5.1, 31-August-1992

8.2.2. Get Element Info

Name: PEXGetElementInfo

Request:fp_format : FLOAT_FORMAT s_id : STRUCTURE_ID range : ELEMENT_RANGE

Reply: info: LISTofELEMENT_INFO

Errors: Structure, Value, FloatingPointFormat

Description:This request returns information about elements in the structure specified by s_id. The offsets that define the range of elements about which information is to be obtained are computed using the positions in range in the following fashion. If whenceis Beginning,the computed offset is just the value specified by offset.

If whenceis Current, the offset is computed by adding offsetto s_id’s element pointer. If whenceis End, the offset is computed by adding offsetto the number of elements in the structure. Offsetcan be a negative number.

If either computed offset is less than zero, it will be set to zero before obtaining the element information. If either computed offset is greater than the number of elements in the structure, it will be set to the offset of the last structure element in the structure. The request returns each element’s ELEMENT_TYPE field, and the length of the element in units of four bytes. The sum of the lengths of all elements in the structure will be equal to the length that can be inquired with the PEXGetStructureInfo request. The information returned will be computed as if the floating point type in fp_format were being used to return the data. No information will be returned for inquiries on element offset zero. The element pointer attribute of s_id is not affected by this request.

8.2.3. Get Structures In Network

Name: PEXGetStructuresInNetwork

Request:s_id : STRUCTURE_ID which: {All,NoCrossRefs}

Reply: structures : LISTofSTRUCTURE_ID

Errors: Structure, Value

Description:This request returns a list of unique structure resource IDs that are referenced in the structure network rooted at s_id. If whichis All,all of the structure resources referenced in the structure network rooted at s_id will be returned in the list structures. If whichis NoCrossRefs,only the IDs of structures in the network that aren’t referenced outside the specified structure network are returned. S_idwill always be

PEX Version 5.1, 31-August-1992 returned in the list, unless s_id is an invalid structure ID, in which case the returned list will be empty.

8.2.4. Get Ancestors

Name: PEXGetAncestors

Request:s_id : STRUCTURE_ID path_part : {TopPart, BottomPart} path_depth : CARD32

Reply: paths : LISTofLISTofELEMENT_REF

Errors: Structure, Value

Description:This request returns unique paths in the structure hierarchy that lead to s_id. Paths are returned as a list of structure id/element offset pairs that are in the order from the root structure down to s_id. For full paths, the last entry in each path would have the structure ID equal to s_id and the offset equal to zero. The path_depth indicates the maximum length (number of structure id/element offset pairs) of each path, except that path_depth = 0 means that the full path is to be returned. The path_part indicates whether the head or the tail of each path is to be returned. If path_part = TopPart, only the first path_depth structure id/element offset pairs in each path will be returned. If path_part = BottomPart, only the last path_depth structure id/element offset pairs in each path will be returned. Only unique paths will be returned (i.e., there will be no duplicates in the list of returned paths).

For instance, specifying path_depth = 0 and path_part = TopPart would cause all paths leading to s_id to be returned. Specifying path_depth = 1 and path_part = TopPart would cause all the structures at the top of each structure network containing s_id to be returned. Specifying path_depth = 1 and path_part =

BottomPart would allow you to determine whether or not s_id is referenced. Specifying path_depth = 2 and path_part = BottomPart would allow you to determine the number of immediate ancestors for s_id as well as returning their resource IDs.PEX Version 5.1, 31-August-1992

8.2.5. Get Descendants

Name: PEXGetDescendants

Request:s_id : STRUCTURE_ID path_part : {TopPart, BottomPart} path_depth : CARD32

Reply: paths : LISTofLISTofELEMENT_REF

Errors: Structure, Value

Description:This request returns unique paths in the structure hierarchy from s_id to leaf nodes in the hierarchy. Paths are returned as a list of structure id/element offset pairs that are in the order from s_id down to the leaf nodes. For full paths, the first entry in each path would have the structure ID equal to s_id and the offset equal to the offset of the element that references a descendant in the hierarchy, and the last entry would have the structure ID of a leaf node in the structure hierarchy and an offset of zero. The path_depth indicates the maximum length (number of structure id/element offset pairs) of each path, except that path_depth = 0 means that the full path is to be returned. The path_part indicates whether the head or the tail of each path is to be returned. If path_part = TopPart, only the first path_depth structure id/element offset pairs in each path will be returned. If path_part = BottomPart, only the last path_depth structure id/element offset pairs in each path will be returned. Only unique paths will be returned (i.e., there will be no duplicates in the list of returned paths).

For instance, specifying path_depth = 0 and path_part = TopPart would cause all paths leading from s_id to leaf nodes to be returned. Specifying path_depth = 1 and path_part = TopPart would cause all the direct references to other structures in s_id to be returned. Specifying path_depth = 1 and path_part =

BottomPart could be used to determine the leaf nodes for the structure hierarchy rooted at s_id.

PEX Version 5.1, 31-August-1992

8.2.6. Fetch Elements

Name: PEXFetchElements

Request:fp_format : FLOAT_FORMAT s_id : STRUCTURE_ID range : ELEMENT_RANGE

Reply: elements: LISTofOUTPUT_CMD

Errors: Structure, FloatingPointFormat, Value

Description:This request returns a range of structure elements in the structure specified by s_id. The offsets that define the range of elements to be fetched are computed using the positions in range in the following fashion. If whenceis Beginning,the computed offset is just the value specified by offset. If whenceis Current, the offset is computed by adding offsetto s_id’s element pointer. If whenceis End, the offset is computed by adding offsetto the number of elements in the structure. Offsetcan be a negative number.

If either computed offset is less than zero, it will be set to zero before the fetch occurs. If either computed offset is greater than the number of elements in the source structure, it will be set to the offset of the last structure element in the source structure. The element pointer attribute of s_id is not affected by the fetch operation. The data for each structure element will be returned in the same format as described Section 3 -

Output Commandssection.

Floating point values in elementswill be returned in the floating point format specified in fp_format (if it is supported by the PEX implementation).

No information will be returned for inquiries on element offset zero.

PEX Version 5.1, 31-August-1992

8.3. Structure Resource Attribute Modification

This section contains requests that can be used to modify structure resource attributes.

8.3.1. Set Editing Mode

Name: PEXSetEditingMode

Request:s_id : STRUCTURE_ID mode: EDIT_MODE

Errors: Structure, Value

Description:This request modifies s_id’s editing mode attribute. The editing mode attribute specifies how editing operations will affect the structure. If the editing mode is set to StructureInsert, subsequent requests to create structure elements will cause elements to be inserted into the structure. Elements will be inserted into the structure after the structure element specified by the element pointer. The element pointer will then be incremented by the number of elements inserted. If the mode is StructureReplace, output requests used to create structure elements will cause structure elements to replace elements starting at the location specified by the element pointer.

8.3.2. Set Element Pointer

Name: PEXSetElementPointer position : ELEMENT_POS

Description:This request sets the element pointer attribute of the structure specified by s_id. The element pointer attribute of the structure will be set to the position specified by position, which contains a whenceand offset pair. If whenceis Beginning,the element pointer is set to the specified offset. If whenceis Current, the new element pointer value is computed by adding offsetto the current value of the element pointer. If whenceis End, the new element pointer value is computed by adding the specified offsetto the offset of the last element in the structure. Offsetcan be a negative number.

If the resultant value of the element pointer is less than zero, the element pointer is set to zero. If the resultant value of the element pointer is greater than the number of elements in the structure, then the element pointer is set to the offset of the last element in the structure.

PEX Version 5.1, 31-August-1992

8.3.3. Set Element Pointer At Label

Name: PEXSetElementPointerAtLabel

Request:s_id : STRUCTURE_ID label : INT32 offset: INT32

Errors: Structure, Label

Description:This request sets the element pointer attribute of the structure specified by s_id. A search is conducted for the next occurrence of a "label" structure element containing label. The search for the label starts at the current element pointer plus one, and proceeds in the forward direction. If a "label" structure element containing label is found, the element pointer for the structure is set to the offset of the located label plus offset.

If the resultant value of the element pointer is less than zero, the element pointer is set to zero. If the resultant value of the element pointer is greater than the number of elements in the structure, then the element pointer is set to the offset of the last element in the structure. This is a non-descending search (i.e., the search does not include any structures referenced by "execute structure" elements). If no occurrence of the specified label is found, an error is generated and the structure’s element pointer is left unchanged.

PEX Version 5.1, 31-August-1992

8.3.4. Element Search

Name: PEXElementSearch

Request:s_id : STRUCTURE_ID position : ELEMENT_POS direction : {Forward, Backward} incl : LISTofELEMENT_TYPE excl: LISTofELEMENT_TYPE

Reply: status : {Found, NotFound} found_offset: CARD32

Errors: Structure, Value

Description:This request conducts a search for the first occurrence of the specified element type in the structure specified by s_id. The offset at which to begin searching is computed using the whenceand offsetfound in position. If whenceis Beginning,the search will begin at the element specified by offset. If whenceis

Current, the specified offsetis added to the current value of s_id’s element pointer to determine the element at which to begin the search. If whenceis End, the element at which to begin the search is computed by adding the specified offsetto the offset of the last element in the structure. Offsetcan be a negative number.

If the computed offset is less than zero, the search will begin at the position preceding the first element in the structure. If the computed offset is greater than the number of elements in the structure, then the search will begin at the last element in the structure. The search always includes the starting element.

An element will be selected if its element type is not contained in excland its element type is included in incl. An element type of Allcauses all element types to match. If a structure element type is in both the inclusion and exclusion sets, it will be excluded.

The search terminates if a match is found or if the limits of the structure are reached. The search progresses from the start point and proceeds either forward in the structure or backward, depending on direction. This is a non-descending search (i.e., the search does not include any structures referenced by "execute structure" elements). If the search succeeds in finding a match, a status of Found is returned, and the offset of the matching element is returned in found_offset. If the search is unsuccessful, a status of NotFound is returned, and a value of zero is returned in found_offset.

The element pointer attribute of s_id is not modified as a result of this request.

PEX Version 5.1, 31-August-1992

8.4. Structure Editing

This section contains requests that can be used to modify structure resources.

8.4.1. Store Elements

Name: PEXStoreElements

Request:fp_format : FLOAT_FORMAT s_id : STRUCTURE_ID elements: LISTofOUTPUT_CMD

Errors: Structure, FloatingPointFormat, OutputCommand

Description:This request causes elements to be stored in the structure whose resource ID is specified by s_id. If the editing_modeattribute of the structure is set to StructureInsert, each entry in elementsis used to create a structure element in the structure after the element specified by the structure’s element_ptr attribute. Output commands in the request are processed until one is found to be in error, or until the entire list has been processed. The erroneous output command and all others following it in the request are ignored (they will not be added to the structure), and an OutputCommanderror is returned to the client. The element pointer is incremented by one for each such insertion. Therefore, at the conclusion of the request, the element pointer is left pointing at the last inserted element.

If the editing_modeattribute is set to StructureReplace, a range of elements is first deleted from the structure as if PEXDeleteElements were called with a position1 whence/offset of {Current, 0} and a position2 whence/offset of {Current, n-1} where n is the number of elements to be deleted. (If element zero is included as part of the range to be deleted, all elements in the range except for element zero will be deleted.) If there are fewer elements between the structure’s element pointer and the end of the structure than there are output commands in elements,then only the elements between the element pointer and the end of the structure will be deleted. The element pointer will be left pointing at the element preceding the deleted range. After the deletion, the output commands specified in elementsare inserted at the element pointer position as described above.

Floating point values in elementswill be in the floating point format specified in fp_format. The formats for the various types of output commands can be found in the "Output Commands" section.

PEX Version 5.1, 31-August-1992

8.4.2. Delete Elements

Name: PEXDeleteElements

Request:s_id : STRUCTURE_ID range : ELEMENT_RANGE

Errors: Structure, Value

Description:This request deletes elements in range from the structure whose ID is specified in s_id. The range of elements to be deleted is computed using the whenceand offsetvalues of position1 and position2.

The offsets that define the range of elements to be deleted are each computed using the positions in range in the following fashion. If whenceis Beginning,the computed offset is just the value specified by offset. If whenceis Current, the offset is computed by adding offsetto s_id’s element pointer. If whenceis End, the offset is computed by adding offsetto the number of elements in the structure. Offsetcan be a negative number.

If either computed offset is less than zero, it will be set to zero before the deletion occurs. If either computed offset is greater than the number of elements in the structure, it will be set to the offset of the last structure element. It is not necessary for the first offset to be less than the second. The deletion is inclusive, meaning that the elements at the boundary of the deletion range are also deleted. It does not matter which of the two offsets determines the lower end of the range to be deleted and which determines the higher end of the range. Deleting element zero is effectively a noop. After the deletion operation, the structure’s element pointer will be set to the element preceding the range of deleted elements.

PEX Version 5.1, 31-August-1992

8.4.3. Delete Elements To Label

Name: PEXDeleteElementsToLabel

Request:s_id : STRUCTURE_ID position : ELEMENT_POS label : INT32

Errors: Structure, Label, Value

Description:This request deletes all elements between a computed offset and a specified label in the structure whose ID is specified in s_id. The offset is computed using position in the following fashion. If whenceis

Beginning,the computed offset is just the value specified by offset. If whenceis Current, the offset is computed by adding offsetto s_id’s element pointer. If whenceis End, the offset is computed by adding offsetto the number of elements in the structure. Offsetcan be a negative number.

If the computed offset is less than zero, it will be set to zero before the deletion occurs. If the computed offset is greater than the number of elements in the structure, it will be set to the offset of the last structure element. Elements are deleted starting at the element immediately after the computed offset up to the next occurrence of the label. The label itself is not deleted. The structure’s element pointer is set to point at the element immediately preceding the range of deleted elements. If the specified label is not found, no deletion occurs and the structure’s element pointer is left unchanged.

8.4.4. Delete Elements Between Labels

Name: PEXDeleteElementsBetweenLabels label1 : INT32 label2 : INT32

Errors: Structure, Label

Description:This request deletes all elements between label1 and label2 in the structure whose ID is specified in s_id.

A search for label1 is first performed starting at the current element pointer position plus one. A search for label2 is then performed, starting at the element after label1. The range of elements between the two labels is then deleted. The two label elements themselves are not deleted. The structure’s element pointer is set to point at the element immediately preceding the range of deleted elements (the element containing label1).

If either of the two specified labels is not found between starting point of the search and the end of the structure, no deletion occurs and the structure’s element pointer is left unchanged.

PEX Version 5.1, 31-August-1992

8.4.5. Copy Elements

Name: PEXCopyElements

Request:src_s_id : STRUCTURE_ID src_range : ELEMENT_RANGE dest_s_id : STRUCTURE_ID dest_position : ELEMENT_POS

Errors: Structure, Value

Description:This request copies elements in src_range from the structure specified in src_s_id to the dest_position in the structure specified in dest_s_id. The range of elements to be copied is computed using the whenceand offsetvalues of position1 and position2 in src_range.

The offsets that define the range of elements to be copied are each computed using the positions in src_range in the following fashion. If whenceis Beginning,the computed offset is just the value specified by offset. If whenceis Current, the offset is computed by adding offsetto src_s_id’s element pointer. If whenceis End, the offset is computed by adding offsetto the number of elements in the structure. Offset can be a negative number.

If either computed offset is less than zero, it will be set to zero before the copy occurs. If either computed offset is greater than the number of elements in the source structure, it will be set to the offset of the last structure element in the source structure. It does not matter which of the two offsets determines the lower end of the range to be copied and which determines the higher end of the range (i.e., the element order will not be reversed if offset1is greater than offset2).

The position to which the elements will be copied is computed using dest_position in the following fashion.

If whenceis Beginning,the computed destination offset is just the value specified by offset. If whenceis

Current, the offset is computed by adding offsetto dest_s_id’s element pointer. If whenceis End, the offset is computed by adding offsetto the number of elements in the destination structure. Offsetcan be a negative number.

It is permissible for src_s_id and dest_s_id to be the same. If this is the case, the copy operation performs as if the indicated range is copied to a temporary location, and then inserted relative to the destination position.

After the copy operation, the destination structure’s element pointer is updated to point at the last element inserted in the destination structure. The editing mode attribute of dest_s_id is ignored during this request;

copied elements are always inserted into the destination structure, never used to replace existing structure elements. PEX Version 5.1, 31-August-1992

8.4.6. Change Structure References

Name: PEXChangeStructureReferences

Request:old_s_id : STRUCTURE_ID new_s_id: STRUCTURE_ID

Errors: Structure

Description:This request changes any "execute structure" elements in the server that reference the structure specified by old_s_id into "execute structure" elements that reference the structure specified by new_s_id.

Any references to the structure new_s_idthat existed before this request are not affected. On all PHIGS workstation resources where new_s_idis already posted, it remains posted and old_s_id, if posted there, is unposted. On all PHIGS workstation resources where new_s_idis not already posted and old_s_id is posted, new_s_idis posted with the same priority as old_s_id and old_s_id is unposted. If there were references to the structure resource specified by old_s_id and the structure resource specified by new_s_id does not exist, an error is returned and no action is taken.

PEX Version 5.1, 31-August-1992

9. Name Sets

______________________________________________________________________________________________ A name set is a PEX resource that is used to filter output commands during rendering, picking, and searching operations. Name sets typically make fairly small demand on server memory resources, but they are of variable size so this can vary depending on their contents.

9.1. Name Set Resource Management

The name set is an X11 resource and carries all of the responsibilities and access rights of X11 resources. These requests manage the creation, freeing, and copying of name set resources.

9.1.1. Create Name Set

Name: PEXCreateNameSet

Request:ns_id : NAME_SET_ID

Errors: IDChoice, Alloc

Description:This request creates a name set resource for the specified ns_id. The name set is initialized to an empty list when the resource is created.

9.1.2. Copy Name Set

Name: PEXCopyNameSet

Request:src_ns_id : NAME_SET_ID dest_ns_id : NAME_SET_ID

Errors: NameSet

Description:This request copies the source name set src_ns_id to a destination name set dest_ns_id after first emptying the contents of dest_ns_id. The dest_ns_id must already exist as a valid resource.

PEX Version 5.1, 31-August-1992

9.1.3. Free Name Set

Name: PEXFreeNameSet

Request:ns_id : NAME_SET_ID

Errors: NameSet

Description:This request deletes the association between the resource ID and the name set. The name set storage will be freed when no other resource references it.

PEX Version 5.1, 31-August-1992

9.2. Name Set Inquiry

These requests inquire the contents of name set resources.

9.2.1. Get Name Set

Name: PEXGetNameSet

Request:ns_id : NAME_SET_ID

Reply: names : LISTofNAME

Errors: NameSet

Description:This request will return the contents of the name set specified by ns_id.

9.3. Name Set Modification

These requests can be used to modify the contents of name set resources.

9.3.1. Change Name Set

Name: PEXChangeNameSet action : {Replace, Add,Remove} names : LISTofNAME

Errors: NameSet, Value

Description:This request changes the contents of a name set resource. If action is Add,the specified list of names is added to the name set. If action is Remove,the specified list of names is removed from the name set. If action is Replace, all the names in the name set are removed, then the specified list of names is added to the name set. If an attempt is made to remove a name which is not in the nameset, then the name will be ignored and no error will be generated.

PEX Version 5.1, 31-August-1992

10. Search Contexts

______________________________________________________________________________________________ A search contextis a PEX resource that allows clients to perform searching operations on structure networks. This section describes the operations that can be performed on search context resources and the operations that can be performed using search context resources. PEX currently provides no support for searching of client-side structure networks.

Some of the requests in this section affect attributes of a search context. The item_maskand item_listparameters specify which components are to be affected. Each bit in the item_maskindicates whether or not the corresponding attribute is affected. In the cases where search context attributes are being set or queried, there is a corresponding entry in the item_listfor each set bit in item_mask. It is therefore possible to affect one or many search context attributes with a single request.

Two of the search context attributes contain name set resource IDs. If a name set is created, bound to a search context, and then freed, the contents of the name set will remain, since it is still being referenced by the search context. However, when a search context is queried, the value AlreadyFreed will be returned for the name set ID, since it no longer has a valid resource ID by which it can be referenced.

When a text primitive or annotation text primitive is encountered during a search operation, only the origin of the text string is used to determine if the search was successful.†

The search context components, in order, are listed in the following table.

Attribute Name Data Type Default Value search_pos COORD_3D (0.0,0.0,0.0) search_dist FLOAT 0.0 search_ceiling CARD16 1 model_clip_flag BOOLEAN False start_path LISTofELEMENT_REF Null normal_list LISTofNAME_SET_PAIR Null inverted_list LISTofNAME_SET_PAIR Null

The attributes of the search context resource are defined as follows:

search_posThis attribute specifies the search reference position in world coordinates.

search_distThis attribute specifies a distance from the search reference position in world coordinates. A successful search occurs only when an output primitive element is found that satisfies the search filter criteria and is within the specified distance from the search reference point. In order to satisfy the search criteria if search_dist is less than or equal to zero, the primitive must intersect the search_pos.

search_ceiling

This attribute defines the ceiling of the search operation. The search ceiling is an index into the list contained in start_path and searching stops when the end of the structure specified by search_ceiling is reached. For example, if there are n items in start_path, and search_ceiling is set to n, the search traversal will terminate at the end of the last structure in the list. On the other hand, if search_ceiling is equal to one, then the search

__________________ † The criteria of closeness to the origin matches PHIGS semantics for incremental spatial search on annotation text. However, PHIGS specifies that the enclosing rectangle of text primitives be used when searching. The traversal-time values of the geometric text attributes, together with text font 1, text precision Stroke,characterexpansion factor 1 and character spacing 0, determine the spatial extent of the enclosing rectangle. At this time, PEX does not follow the PHIGS semantics for searching on text primitives. In order to release the current PEX documents in a timely manner, this issue has been deferred until a future version of PEX. PEX Version 5.1, 31-August-1992

will effectively operate without a ceiling, terminating at the end of the first structure in start_path.

model_clip_flag

This attribute specifies whether modeling clipping must be performed during the search operation. If True, modeling clipping is performed using the modeling clipping attributes as they are encountered during the traversal. If False, no modeling clipping is performed and modeling clipping attributes that are encountered during the traversal are effectively ignored.

start_pathThis attribute defines the structure network path that is to be used as the starting point for the search.

Searching begins at the element followingthe one indicated by the start path.

normal_listThis attribute contains the list of name set resource ID pairs to be used as filters in the search operation. If the normal_list is Null, all name sets are considered accepted by the normal filter list.

inverted_list

This attribute contains the list of name set resource ID pairs to be inverted and used as filters in the search operation. If the inverted_list is Null, all name sets are considered accepted by the inverted filter list.

PEX Version 5.1, 31-August-1992

10.1. Search Context Resource Management

The search context is an X11 resource and carries all of the responsibilities and access rights of X11 resources.

These requests manage the creation, freeing, and copying of search contexts.

10.1.1. Create Search Context

Name: PEXCreateSearchContext

Request:fp_format : FLOAT_FORMAT sc_id : SEARCH_CONTEXT_ID item_mask: BITMASK item_list: LISTofVALUE

Errors: IDChoice, Value, FloatingPointFormat, Alloc, Path, NameSet

Description:This request creates a search context resource for the specified sc_id. The item_maskdefines those search context attributes that are to be explicitly set at the time the resource is created. The item_listcontains the corresponding list of values used to modify the newly-created search context. Floating point values in item_listwill be in the floating point format specified in fp_format.

10.1.2. Copy Search Context

Name: PEXCopySearchContext

Request:src_sc_id : SEARCH_CONTEXT_ID dest_sc_id : SEARCH_CONTEXT_ID

Errors: SearchContext, Value

Description:This request copies the source search context src_sc_id to a destination search context dest_sc_id. The dest_sc_id must already exist as a valid resource. The item_maskindicates which values in the search context will be copied. PEX Version 5.1, 31-August-1992

10.1.3. Free Search Context

Name: PEXFreeSearchContext

Request:sc_id : SEARCH_CONTEXT_ID

Errors: SearchContext

Description:This request deletes the specified search context resource and frees the storage associated with it.

PEX Version 5.1, 31-August-1992

10.2. Search Context Inquiry

The requests in this section can be used to inquire search context attributes.

10.2.1. Get Search Context

Name: PEXGetSearchContext

Request:fp_format : FLOAT_FORMAT sc_id : SEARCH_CONTEXT_ID item_mask: BITMASK

Reply: item_list: LISTofVALUE

Errors: SearchContext, FloatingPointFormat, Value

Description:This request will return components of the search context specified by sc_id. The item_maskspecifies which components are to be inquired and returned. The specified attributes of the search context will be returned in item_list. Floating point values in item_listwill be returned in the floating point format specified in fp_format.

10.3. Search Context Modification

The requests in this section can be used to modify attributes of search context resources.

10.3.1. Change Search Context

Name: PEXChangeSearchContext item_list: LISTofVALUE

Errors: SearchContext, Value, FloatingPointFormat, Path, NameSet

Description:This request changes components of a search context. The item_maskand item_listspecify which components are to be changed. Each bit in the item_maskindicates whether or not there is a corresponding entry in the item_list. It is therefore possible to modify one or many search context attributes with a

PEXChangeSearchContext request. Floating point values in item_listwill be in the floating point format specified in fp_format. PEX Version 5.1, 31-August-1992

10.4. Structure Network Searching

This section describes requests that use search context resources to perform structure network searching operations.

10.4.1. Search Network

Name: PEXSearchNetwork

Request:sc_id : SEARCH_CONTEXT_ID

Reply: found_path : LISTofELEMENT_REF

Errors: SearchContext, Path

Description:This request causes a spatial search in world coordinates to be performed on a structure network. The parameters of the searching operation are found in the search context sc_id. The search begins at the element followingthe one indicated by the start_path attribute of sc_id. The search is terminated once the end of the structure indicated by search_ceiling has been reached. The first element that meets the search criteria is returned in found_path. If no element is found, found_path will be null. After the search has completed, the start_path attribute of sc_id will be set to the value that is returned in found_path.

For a structure element to be considered a candidate for the search, the current name set has to be accepted by all the name set pairs in the search context’s normal_list, and has to be rejected by all of the name set pairs in the inverted_list. If the normal_list is Null, all possible name sets are accepted by the normal list.

If the inverted_list is Null, all possible name sets are accepted by the inverted list. Therefore the default case is that all output primitives are considered.

PEX Version 5.1, 31-August-1992

11. PHIGS Workstations

______________________________________________________________________________________________ A PHIGS workstation is a PEX resource that combines other resources into a single entity that behaves in a manner similar to the PHIGS abstraction of a "workstation". The PHIGS workstation has built into it all of the capabilities of the renderer resource described earlier. A PHIGS workstation, with its lookup tables and name sets, effectively contains an instance of a renderer, but it also contains functionality above and beyond that found in a renderer resource.

This section describes the operations that can be performed on PHIGS workstation resources and the operations that can be performed using PHIGS workstation resources. In addition to the attributes listed below, the PHIGS workstation resource also contains an implementation-dependent number of pick device descriptors that support picking operations. These can be set and queried with requests found in the next section, "Picking".

There are several differences between PHIGS workstations and renderers. Due to the desire to match PHIGS semantics for dealing with views, a PHIGS workstation resource has a built-in view table that can only be accessed through the defined PHIGS workstation requests. However, this view table is functionally the same as that used by a renderer, and information about it may be obtained by using the lookup table requests to obtain information about tables of type View. A PHIGS workstation resource that has its associated drawable destroyed will be freed implicitly.

Lookup table and name set resources can be bound to a PHIGS workstation resource and then freed. The contents of these resources will remain, since they are still being referenced by the PHIGS workstation. However, when a

PHIGS workstation’s attributes are queried, the value AlreadyFreed will be returned for those resources that have been freed and thus no longer have a valid resource ID by which they can be referenced.

PEX Version 5.1, 31-August-1992

11.1. PHIGS Workstation Resource Management

The PHIGS workstation is an X11 resource and carries all of the responsibilities and access rights of X11 resources.

These requests manage the creation, freeing, and copying of PHIGS workstation resources.

11.1.1. Create PHIGS Workstation

Name: PEXCreatePhigsWKS

Request:wks_id: PHIGS_WKS_ID drawable_id : DRAWABLE_ID marker_bundle : LOOKUP_TABLE_ID text_bundle: LOOKUP_TABLE_ID line_bundle : LOOKUP_TABLE_ID interior_bundle : LOOKUP_TABLE_ID edge_bundle : LOOKUP_TABLE_ID color_table : LOOKUP_TABLE_ID depth_cue_table : LOOKUP_TABLE_ID light_table : LOOKUP_TABLE_ID color_approx_table : LOOKUP_TABLE_ID pattern_table : LOOKUP_TABLE_ID text_font_table: LOOKUP_TABLE_ID highlight_inclusion : NAME_SET_ID highlight_exclusion: NAME_SET_ID invisibility_inclusion: NAME_SET_ID invisibility_exclusion: NAME_SET_ID buffer_mode: BUFFER_MODE

Errors: IDChoice, Drawable, Match, LookupTable, NameSet, Alloc, Value

Description:This request creates a PHIGS workstation resource for the specified wks_id.The window or pixmap specified by drawable_id is associated with the newly-created PHIGS workstation resource. The named tables and name sets are also bound to the PHIGS workstation resource for use during rendering. A view table that supports current and requested view table entries is allocated for the PHIGS workstation automatically at creation time. The requests PEXSetViewRep and PEXGetViewRep can be used to modify and query the PHIGS workstation view table. The buffer_modeattribute is used to specify whether the workstation will operate in single-buffered or double-buffered mode. If double-buffered, an additional image buffer will be created for the drawable in an implementation-dependent fashion in order to support double-buffering. If drawable_id is a pixmap, then no double buffering will be performed.

PEX Version 5.1, 31-August-1992

11.1.2. Free PHIGS Workstation

Name: PEXFreePhigsWKS

Request:wks_id: PHIGS_WKS_ID

Errors: PhigsWKS

Description:This request deletes the PHIGS workstation resource and any image buffers that were created by the PEX extension in order to support double-buffering. The storage associated with the resource is then freed as well. PEX Version 5.1, 31-August-1992

11.2. PHIGS Workstation Inquiry

This section defines requests that can be used to get information about a PHIGS workstation resource.

11.2.1. Get PHIGS Workstation Info

Name: PEXGetWKSInfo

Request:fp_format : FLOAT_FORMAT wks_id: PHIGS_WKS_ID item_mask: WKS_BITMASK

Reply: item_list: LISTofVALUE

Errors: PhigsWKS, FloatingPointFormat, Value

Description:This request returns attributes of the PHIGS workstation resource indicated by wks_id. Floating point values will be returned in the floating point format specified by fp_format. The parameter item_mask indicates which attributes are to be returned. For each bit that is set in item_mask,a corresponding value is returned in item_list.

In the table below, the abbreviation "create wks req." indicates that the parameter is set by the

PEXCreatePhigsWKS request. The abbreviation "imp. dep." means that the default value is implementation-dependent. The attributes that may be returned, in order, are:

Attribute Name Data Type Default display_update DISPLAY_UPDATE VisualizeEach visual_state VISUAL_STATE Correct display_surface DISPLAY_STATE Empty view_update UPDATE_STATE NotPending defined_views LISTofTABLE_INDEX View 0 defined wks_update UPDATE_STATE NotPending req_NPC_subvolume NPC_SUBVOLUME (0.0,0.0,0.0),(1.0,1.0,1.0) cur_NPC_subvolume NPC_SUBVOLUME (0.0,0.0,0.0),(1.0,1.0,1.0) req_wks_viewpt VIEWPORT {imp. dep., imp. dep., True} cur_wks_viewpt VIEWPORT {imp. dep., imp. dep., True}

HLHSR_update UPDATE_STATE NotPending req_HLHSR_mode HLHSR_MODE 1 cur_HLHSR_mode HLHSR_MODE 1 drawable_id DRAWABLE_ID create wks req.

marker_bundle LOOKUP_TABLE_ID create wks req.

text_bundle LOOKUP_TABLE_ID create wks req.

line_bundle LOOKUP_TABLE_ID create wks req.

interior_bundle LOOKUP_TABLE_ID create wks req.

edge_bundle LOOKUP_TABLE_ID create wks req.

color_table LOOKUP_TABLE_ID create wks req.

depth_cue_table LOOKUP_TABLE_ID create wks req.

light_table LOOKUP_TABLE_ID create wks req.

color_approx_table LOOKUP_TABLE_ID create wks req.

PEX Version 5.1, 31-August-1992 pattern_table LOOKUP_TABLE_ID create wks req.

text_font_table LOOKUP_TABLE_ID create wks req.

highlight_inclusion NAME_SET_ID create wks req.

highlight_exclusion NAME_SET_ID create wks req.

invisibility_inclusion NAME_SET_ID create wks req.

invisibility_exclusion NAME_SET_ID create wks req.

posted_structs LISTofSTRUCTURE_INFO Null num_priorities CARD32 imp. dep.

buffer_update UPDATE_STATE NotPending req_buffer_mode BUFFER_MODE create wks req.

cur_buffer_mode BUFFER_MODE create wks req.

display_update

Returns the PHIGS workstation’s current display update mode. This mode specifies how the PHIGS workstation attempts to visualize changes, and can be set with the PEXSetDisplayUpdateMode request.

visual_stateReturns the PHIGS workstation’s current visual state. The visual state will be Correct if there are no deferred actions and no changes have been simulated on the display surface. The visual state will be

Deferred if there are deferred actions, or if there are deferred actions and some changes have been simulated on the display surface. The visual state will be Simulatedif there are no deferred actions, but some changes have been simulated on the display surface.

display_surface

Returns the current status of the PHIGS workstation’s display surface. The display surface will be

Emptyif nothing has been rendered on the drawable, NotEmptyotherwise.

view_update

Returns Pending or NotPending, depending on whether there are view modification requests that have yet to be made current.

defined_views

Returns the list of view table indices that are defined in the PHIGS workstation’s current view table.

The list of defined view indices will be returned in the order of view transformation input priority.

wks_updateReturns Pending or NotPending, depending on whether there are workstation transformation requests that have yet to be made current.

req_NPC_subvolume

Returns the value for the PHIGS workstation’s NPC subvolume specification that has been requested but has not yet been made current.

cur_NPC_subvolume

Returns the current value for the PHIGS workstation’s NPC subvolume specification.

req_wks_viewpt

Returns the value for the PHIGS workstation’s viewport specification that has been requested but has not yet been made current.

cur_wks_viewpt

Returns the current value for the PHIGS workstation’s viewport specification.

HLHSR_update

Returns Pending or NotPending, depending on whether there are HLHSR mode requests that have yet to be made current.PEX Version 5.1, 31-August-1992 req_HLHSR_mode

Returns the value for the PHIGS workstation’s HLHSR mode that has been requested but has not yet been made current.

cur_HLHSR_mode

Returns the current value for the PHIGS workstation’s HLHSR mode.

drawable_id

Returns the resource ID of the drawable that is being used as the display surface.

marker_bundle

Returns the resource ID of the PHIGS workstation’s marker bundle table.

text_bundleReturns the resource ID of the PHIGS workstation’s text bundle table.

line_bundleReturns the resource ID of the PHIGS workstation’s line bundle table.

interior_bundle

Returns the resource ID of the PHIGS workstation’s interior bundle table.

edge_bundle

Returns the resource ID of the PHIGS workstation’s edge bundle table.

color_tableReturns the resource ID of the color lookup table that will be used by the PHIGS workstation to dereference indexed color values.

depth_cue_table

Returns the resource ID of the PHIGS workstation’s depth-cue table.

light_tableReturns the resource ID of the PHIGS workstation’s light table.

color_approx_table

Returns the resource ID of the color approximation table that will be used by the PHIGS workstation.

pattern_table

Returns the resource ID of the PHIGS workstation’s pattern table.

text_font_table

Returns the resource ID of the PHIGS workstation’s text font table.

highlight_inclusion

Returns the resource ID of the PHIGS workstation’s highlight inclusion name set.

highlight_exclusion

Returns the resource ID of the PHIGS workstation’s highlight exclusion name set.

invisibility_inclusion

Returns the resource ID of the PHIGS workstation’s invisibility inclusion name set.

invisibility_exclusion

Returns the resource ID of the PHIGS workstation’s invisibility exclusion name set.

posted_structs

Returns the resource ID and associated priority of each of the structures in the PHIGS workstation’s posted structure list. The list will be returned in structure priority order.

PEX Version 5.1, 31-August-1992 num_priorities

Returns the number of display priorities that are supported. A value of zero indicates that a continuous range of priorities is supported.

buffer_update

Returns Pending or NotPending, depending on whether there are buffer mode requests that have yet to be made current.

req_buffer_mode

Returns the value for the PHIGS workstation’s buffer mode that has been requested but has not yet been made current.

cur_buffer_mode

Returns the value for the PHIGS workstation’s buffer mode, either Singleor Double. If the drawable associated with the PHIGS workstation resource is a pixmap, then no double-buffering will be performed. PEX Version 5.1, 31-August-1992

11.2.2. Get Dynamics

Name: PEXGetDynamics

Request:drawable_id : DRAWABLE_ID

Reply: view_rep: DYNAMIC_TYPE marker_bundle : DYNAMIC_TYPE text_bundle: DYNAMIC_TYPE line_bundle : DYNAMIC_TYPE interior_bundle : DYNAMIC_TYPE edge_bundle : DYNAMIC_TYPE color_table : DYNAMIC_TYPE pattern_table : DYNAMIC_TYPE wks_transform : DYNAMIC_TYPE highlight_filter : DYNAMIC_TYPE invisibility_filter : DYNAMIC_TYPE

HLHSR_mode: DYNAMIC_TYPE structure_modify: DYNAMIC_TYPE post_structure : DYNAMIC_TYPE unpost_structure : DYNAMIC_TYPE delete_structure : DYNAMIC_TYPE reference_modify: DYNAMIC_TYPE buffer_modify: DYNAMIC_TYPE light_table : DYNAMIC_TYPE depth_cue_table : DYNAMIC_TYPE color_approx_table : DYNAMIC_TYPE

Errors: Drawable, Match

Description:This request returns information about the dynamics that are supported by PHIGS workstations associated with drawables of the type specified by drawable_id. The list of dynamics, in order, is as follows:

PEX Version 5.1, 31-August-1992

Attribute Name Description view_rep Changes to view table marker_bundle Changes to marker bundle text_bundle Changes to text bundle line_bundle Changes to line bundle interior_bundle Changes to interior bundle edge_bundle Changes to edge bundle color_table Changes to color table pattern_table Changes to pattern table wks_transform Changes to workstation transformations highlight_filter Changes to highlight name set invisibility_filter Changes to invisibility name set

HLHSR_mode Changes to HLHSR mode structure_modify Structure modifications (edits) post_structure Additions to posted structure list unpost_structure Deletions from posted structure list delete_structure Deletion of structure resources reference_modify Structure reference modifications buffer_modify Changes to buffering mode light_table Changes to light table depth_cue_table Changes to depth cue table color_approx_table Changes to color approximation table

The value returned for each of the items in the list above can be one of IMM,IRG,or CBS,where IMM means that the specified action can be performed and the correct image displayed immediately, IRGmeans that the specified action requires a regeneration of the image, and CBSmeans that the specified action can be simulated immediately if the PHIGS workstation’s display_update mode is set to SimulateSome.

PEX Version 5.1, 31-August-1992

11.2.3. Get View Representation

Name: PEXGetViewRep

Request:fp_format : FLOAT_FORMAT wks_id: PHIGS_WKS_ID index: TABLE_INDEX

Reply: view_update: {Pending, NotPending} requested : VIEW_REP current : VIEW_REP

Errors: PhigsWKS, FloatingPointFormat, Value

Description:This request returns the value of the view update state and the specified entries in the requested and current view tables in the PHIGS workstation specified by wks_id. The view_updatewill be Pending if a view change has been requested but not established. If the specified entry is not defined, an error will be generated and the contents of the reply parameters will be undefined. Floating point values will be returned in the floating point format specified by fp_format.

PEX Version 5.1, 31-August-1992

11.3. PHIGS Workstation Manipulation

This section contains requests that modify PHIGS workstation resources.

11.3.1. Redraw All Structures

Name: PEXRedrawAllStructures

Request:wks_id: PHIGS_WKS_ID

Errors: PhigsWKS

Description:This request redraws all the posted structures contained in the PHIGS workstation resource specified by wks_id. First, if the PHIGS workstation’s display_surface attribute is NotEmpty,its drawable is cleared to the color stored in entry zero of its color lookup table. Then, if any of its view_update,wks_update,

HLHSR_update,or buffer_update attributes is set to Pending, the requested values are made the current values and the attribute is set to NotPending. After this, all the posted structures are traversed and rendered

(in priority order). Finally, the PHIGS workstation’s visual_state attribute is set to Correct.

11.3.2. Update Workstation

Name: PEXUpdateWorkstation

Description:This request will perform actions identical to PEXRedrawAllStructures on the PHIGS workstation specified by wks_idif its visual_state attribute is currently set to Deferred or Simulated.

PEX Version 5.1, 31-August-1992

11.3.3. Redraw Clip Region

Name: PEXRedrawClipRegion

Request:wks_id: PHIGS_WKS_ID clip_list : LISTofDEVICE_RECT

Errors: PhigsWKS

Description:This request will perform actions similar to the PEXRedrawAllStructures request, except that no PHIGS workstation state attributes are modified or updated by this request. Rendering will occur only in the region defined by clip_list. The color stored in entry zero of the wks_id’scolor lookup table is used to clear the region under the rectangles defined by clip_list. The rectangles in clip_list should be non-overlapping, or the graphics results will be undefined. (If a z-buffering algorithm is used, only those pixels under the rectangles in the clip list will have their z values initialized.) All of the posted structures for wks_idare then redrawn, but only pixels under the rectangles in clip_list are affected. Pending changes are not made current by this request, nor is the visual_state attribute modified.

11.3.4. Execute Deferred Actions

Name: PEXExecuteDeferredActions

Description:This request causes all the deferred actions on the PHIGS workstation specified by wks_idto be executed.

PEX Version 5.1, 31-August-1992

11.3.5. Set View Priority

Name: PEXSetViewPriority

Request:wks_id: PHIGS_WKS_ID index1: TABLE_INDEX index2: TABLE_INDEX priority : {Higher, Lower}

Errors: PhigsWKS, Value

Description:This request sets the relative priorities of entries in wks_id’scurrent view table. The priority of view table entry index1with respect to view table entry index2is set to the next Higher or Lowerpriority. These priorities are used to determine the order in which view table entries are tested when selecting the inverse viewing transformation to use for transformation from device coordinates to world coordinates.

11.3.6. Set Display Update Mode

Name: PEXSetDisplayUpdateMode display_update : DISPLAY_UPDATE

Description:This request sets the display_update attribute of the PHIGS workstation resource specified by wks_id. This attribute defines how changes to the display surface will be visualized. The list of permissible display update modes is defined in the "Extension Information" section that describes enumerated types.

If double buffering is enabled (see PEXSetWKSBufferMode), the display update mode affects which buffer is rendered into. If the display update mode is VisualizeNone,VisualizeEachor VisualizeWhenever, output primitives are rendered into the back (undisplayed) buffer while the structure network is being traversed. When the traversal is complete, the front and back buffers are swapped, so the rendered image is displayed. If the display update mode is VisualizeEasyor SimulateSome,output primitives are always rendered into the front (displayed) buffer.

PEX Version 5.1, 31-August-1992

11.3.7. Map DC to WC

Name: PEXMapDCtoWC

Request:fp_format : FLOAT_FORMAT wks_id: PHIGS_WKS_ID dc_points : LISTofDEVICE_COORD

Reply: wc_points: LISTofCOORD_3D view_index: TABLE_INDEX

Errors: PhigsWKS, FloatingPointFormat

Description:This request maps the device coordinate points in dc_points to the world coordinate points in wc_points using the PHIGS workstation resource specified by wks_id. (The client must convert pointer position values in drawable coordinates into device coordinates.) Each view in the PHIGS workstation’s current view table, which has an inverse, is checked to see if it contains all the specified device coordinate points.

(If the view transform has no inverse then it is not considered). The index of the view with the highest view transformation input priority that contains all of the points is returned in view_index. If no view contains all of the points, the index of the view containing the most points is returned. The points are transformed to world coordinates by passing them through the inverse of the view transform associated with the view index and are returned in wc_points. Floating point values are passed and will be returned in the floating point format specified by fp_format. Points that are clipped (outside the viewport) will not be transformed and returned in the wc_pointslist, so the number of points returned may be less than the number sent.

11.3.8. Map WC to DC

Name: PEXMapWCtoDC wc_points: LISTofCOORD_3D

Reply: dc_points : LISTofDEVICE_COORD

Description:This request maps the world coordinate points in wc_pointsto the device coordinate points in dc_points using the PHIGS workstation resource specified by wks_idand the view specified by view_index. The points are transformed to device coordinates by passing them through the view transform associated with the view_index. Floating point values sent and received will be in the floating point format specified by fp_format. Points that are clipped will not be returned in the dc_points list, so the number of points

PEX Version 5.1, 31-August-1992 returned may be less than the number sent.

PEX Version 5.1, 31-August-1992

11.4. PHIGS Workstation Update

This section defines requests that can be used to set "requested" values for PHIGS workstation resources.

11.4.1. Set View Representation

Name: PEXSetViewRep

Request:fp_format : FLOAT_FORMAT wks_id: PHIGS_WKS_ID view_rep: VIEW_REP

Errors: PhigsWKS, FloatingPointFormat, Alloc

Description:This request sets the requested values of the specified view table entry of the view table in the PHIGS workstation specified by wks_idto the view representation indicated by view_rep. The view_update attribute in the PHIGS workstation is set to Pending if the change cannot be visualized immediately;

otherwise it is set to NotPending. If the view_updateattribute is NotPending, the current view table entry is set to the requested values; otherwise the current values are not changed until the PHIGS workstation is updated.

11.4.2. Set Workstation Window

Name: PEXSetWKSWindow

NPC_subvolume: NPC_SUBVOLUME

Errors: PhigsWKS, FloatingPointFormat

Description:This request sets the req_NPC_subvolumeof the PHIGS workstation specified by wks_idto the values in

NPC_subvolume. The wks_updateattribute in the PHIGS workstation is set to Pending if the change cannot be visualized immediately; otherwise it is set to NotPending. If the wks_updateattribute is

NotPending, the cur_NPC_subvolumeis set to the requested values; otherwise the current values are not changed until the PHIGS workstation is updated.

PEX Version 5.1, 31-August-1992

11.4.3. Set Workstation Viewport

Name: PEXSetWKSViewport

Request:fp_format : FLOAT_FORMAT wks_id: PHIGS_WKS_ID viewport: VIEWPORT

Errors: PhigsWKS, FloatingPointFormat, Value

Description:This request sets the req_wks_viewptof the PHIGS workstation specified by wks_idto the values in viewport. The wks_updateattribute in the PHIGS workstation is set to Pending if the change cannot be visualized immediately; otherwise it is set to NotPending. If the wks_updateattribute is NotPending, the cur_wks_viewptis set to the requested values; otherwise the current values are not changed until the PHIGS workstation is updated.

11.4.4. Set HLHSR Mode

Name: PEXSetHLHSRMode

Request:wks_id: PHIGS_WKS_ID mode: HLHSR_MODE

Errors: PhigsWKS, Value, Alloc

Description:This request sets the req_HLHSR_modeof the PHIGS workstation specified by wks_idto the values in mode. If the PHIGS workstation’s display_surface attribute is Empty,or if the dynamic modification for its

HLHSR_modeis IMM,its cur_HLHSR_modeattribute is modified with the value contained in modeand its

HLHSR_updateis set to NotPending; otherwise, its HLHSR_updateis set to Pending and the current value is not changed until the PHIGS workstation is updated.

PEX Version 5.1, 31-August-1992

11.4.5. Set Buffer Mode

Name: PEXSetWKSBufferMode

Request:wks_id: PHIGS_WKS_ID buffer_mode: BUFFER_MODE

Errors: PhigsWKS, Value, Alloc

Description:This request sets the req_buffer_modeof the PHIGS workstation specified by wks_idto the values in buffer_mode. If the PHIGS workstation’s display_surface attribute is Empty,or if the dynamic modification for its buffer_modeis IMM,its cur_buffer_modeattribute is modified with the value contained in buffer_modeand its buffer_update is set to NotPending; otherwise, its buffer_update is set to Pending and the current value is not changed until the PHIGS workstation is updated.

Buffer_modemay be one of the constants Single(rendering is to be single-buffered) or Double (rendering is to be double-buffered). An Allocerror will be returned if the requested mode is Double and the server cannot allocate any more image buffers.

PEX Version 5.1, 31-August-1992

11.5. Posting/Unposting Structures

This section describes the requests that can be used to post and unpost structures on a PHIGS workstation resource.

11.5.1. Post Structure

Name: PEXPostStructure

Request:fp_format : FLOAT_FORMAT wks_id: PHIGS_WKS_ID s_id : STRUCTURE_ID priority : FLOAT

Errors: PhigsWKS, Structure, FloatingPointFormat

Description:This request adds the structure specified by s_id to the list of posted structures in the PHIGS workstation wks_id. A priority is also provided to indicate the priority of the newly-posted structure with respect to the structures already in the posted structure list. If multiple structures are posted for display to the same display space location, the implementation will ensure the display of the higher priority structure. If two structures have the same priority, the last posted structure has the higher priority. If s_id is not a valid structure resource ID, the request is ignored, and an error is generated.

11.5.2. Unpost Structure

Name: PEXUnpostStructure

Request:wks_id: PHIGS_WKS_ID

Errors: PhigsWKS, Structure

Description:This request removes the structure specified by s_id from wks_id’sposted structure list. If s_id is not found in the posted structure list, the request is ignored, and an error is generated.

PEX Version 5.1, 31-August-1992

11.5.3. Unpost All Structures

Name: PEXUnpostAllStructures

Request:wks_id: PHIGS_WKS_ID

Errors: PhigsWKS

Description:This request removes all structures from wks_id’sposted structure list.

11.5.4. Get PHIGS Workstation Postings

Name: PEXGetWKSPostings

Request:s_id : STRUCTURE_ID

Reply: wks_id: LISTofPHIGS_WKS_ID

Errors: Structure

Description:This request returns a list of all of the PHIGS workstation resources to which s_id has been posted.

PEX Version 5.1, 31-August-1992

12. Workstation Picking

______________________________________________________________________________________________ The discussion of workstation picking includes pickdevicedescriptors which are found in PHIGS workstation resources and pickmeasures.

12.1. Pick Device Descriptors

Each PHIGS workstation resource maintains a list of pickdevicedescriptors. Each entry in this list maintains state values for a particular type of pick device, such as a mouse or a 3D tablet. Together, the entries in the pick device descriptor list maintain state values for all of the pick devices that are supported by the workstation resource. This list of values can be set or inquired for each of the supported pick devices.

Two of the pick device descriptor components are name set resource IDs. If a name set is created, bound to a pick device descriptor, and then freed, the contents of the name set will remain, since it is still being referenced by the pick device descriptor. However, when a pick device descriptor is queried, the value AlreadyFreed will be returned for the name set ID, since it no longer has a valid resource ID by which it can be referenced.

The pick device descriptor components, in order, are listed in the following table. The abbreviation "pick dev. dep."

stands for "pick-device-dependent", meaning that the default value is determined by the pick device type. The abbreviation "imp. dep." means that the default value is implementation-dependent.

Attribute Name Data Type Default Value pick_status {NoPick,Ok} NoPick pick_path LISTofPICK_ELEMENT_REF Null pick_path_order {TopFirst, BottomFirst} TopFirst pick_inclusion NAME_SET_ID Null pick_exclusion NAME_SET_ID Null pick_data_rec LISTofCARD8 pick dev. dep.

prompt_echo_type PROMPT_ECHO_TYPE pick dev. dep.

echo_volume VIEWPORT {imp. dep., imp. dep., True} echo_switch {NoEcho,Echo} NoEcho

The components of the pick device descriptor are defined as follows:

pick_statusThis attribute contains the initial pick status that will be bound to a pick measure resource.

pick_pathThis attribute contains the initial pick path that will be bound to a pick measure resource.

pick_path_order

This attribute specifies the order in which elements of the picked path are to be written into a pick measure resource. If the order is TopFirst, elements of the pick measure’s picked_path attribute will be listed in the order they would have been encountered during a traversal, while if the order is BottomFirst they will be listed in the opposite order.

pick_inclusion

This attribute specifies the resource ID of the name set resource that is to be used as the pick inclusion filter during picking operations.

pick_exclusion

This attribute specifies the resource ID of the name set resource that is to be used as the pick exclusion filter during picking operations. PEX Version 5.1, 31-August-1992 pick_data_rec

This attribute contains a pick-device-dependent data record used to initialize a pick measure resource when it is created.

prompt_echo_type

This attribute contains an enumerated type value that specifies the prompt/echo type to be used during picking operations. The allowable types are described in the "Extension Information" section.

echo_volume

This attribute specifies where prompting and/or echoing is to occur. The default is that the echo volume will be defined to be the size of the drawable that was bound to the the PHIGS workstation resource at the time it was created.

echo_switch

This attribute specifies the initial echo state for a pick measure.

The requests in this section allow clients to set and inquire the values of pick device descriptors that are stored in a

PHIGS workstation resource. PEX Version 5.1, 31-August-1992

12.1.1. Get Pick Device Descriptor

Name: PEXGetPickDevice

Request:fp_format : FLOAT_FORMAT wks_id: PHIGS_WKS_ID dev_type: PICK_DEVICE_TYPE item_mask: BITMASK

Reply: item_list: LISTofVALUE

Errors: PhigsWKS, Value, FloatingPointFormat

Description:This request will return components of a pick descriptor for the PHIGS workstation resource specified by wks_id. The descriptor returned will be the currently-defined descriptor for the pick device of the type specified by dev_type. The item_maskspecifies which components are to be inquired and returned. The specified attributes of the pick device descriptor will be returned in item_list. Floating point values in item_listwill be returned in the floating point format specified in fp_format.

12.1.2. Change Pick Device Descriptor

Name: PEXChangePickDevice item_list: LISTofVALUE

Errors: PhigsWKS, Value, FloatingPointFormat, Path, NameSet

Description:This request will modify components of a pick descriptor for the PHIGS workstation resource specified by wks_id. The descriptor to be modified will be the currently-defined descriptor for the pick device of the type specified by dev_type. The item_maskspecifies which components are to be changed. The specified attributes of the pick device descriptor will be set to the values contained in item_list. Floating point values in item_listwill be in the floating point format specified in fp_format.

PEX Version 5.1, 31-August-1992

12.2. Pick Measure

A pickmeasure resource must be created to actually perform a pick operation. A pick device type is specified at the time a pick measure resource is created in order to provide the parameters for the picking operation. The pick measure resource accepts input in the form of input records which are defined for each type of pick device. When a pick measure resource is passed a valid input record, its attributes will be updated. Operations on a pick measure resource are potentially lengthy since a great number of structure elements may have to be processed in order to produce the pick results.

The pick measure resource components, in order, are listed in the following table. The abbreviation "from wks" indicates that the default value is inherited from the pick device descriptor stored in the PHIGS workstation resource when the pick measure is created.

Attribute Name Data Type Default Value pick_status {NoPick,Ok} from wks picked_prim LISTofPICK_ELEMENT_REF from wks

The attributes of the pick measure resource are defined as follows:

pick_statusThis attribute contains the result of the last update operation that was performed. It is set to Okif a primitive was successfully picked, and NoPickif the pick operation was unsuccessful.

picked_prim

This attribute contains the path of the structure element that was picked as a result of the last update operation.

The pick measure is an X11 resource and carries all of the responsibilities and access rights of X11 resources. The requests in this section manage the creation and freeing of pick measures.

PEX Version 5.1, 31-August-1992

12.2.1. Create Pick Measure

Name: PEXCreatePickMeasure

Request:pm_id: PICK_MEASURE_ID wks_id: PHIGS_WKS_ID dev_type: PICK_DEVICE_TYPE

Errors: IDChoice, PhigsWKS, Alloc, Value

Description:This request creates a pick measure resource of the type specified by dev_type. The resource ID of the pick measure is specified by pm_id. The newly-created pick measure is initialized with the values contained in the appropriate pick device descriptor stored in the PHIGS workstation resource specified by wks_id.

12.2.2. Free Pick Measure

Name: PEXFreePickMeasure

Errors: PickMeasure

Description:This request deletes the pick measure resource and frees the storage associated with it.

12.2.3. Get Pick Measure Attributes

Name: PEXGetPickMeasure item_mask: BITMASK

Reply: item_list: LISTofVALUE

Errors: PickMeasure, Value

Description:This request will return components of the pick measure specified by pm_id. The item_maskspecifies which components are to be inquired and returned. The specified attributes of the pick measure will be returned in item_list. PEX Version 5.1, 31-August-1992

12.2.4. Update Pick Measure

Name: PEXUpdatePickMeasure

Request:pm_id: PICK_MEASURE_ID input_record : LISTofCARD8

Errors: PickMeasure, Path

Description:This request will update the pick measure specified by pm_idusing the information found in input_record.

If this update causes a primitive to be picked, the pick measure’s pick_status will be set to Okand the picked_primwill be set to the path of the picked primitive. If no primitive was picked, the pick_status will be set to NoPick.

picked_primcan be used for echoing when the pick measure is created. However it is not used as a start path from which to start picking.

The data in input_record is dependent on the type of pick device for which the pick measure resource was created, that is, the dev_typespecified to PEXCreatePickMeasure. PEXGetPickMeasure can be used to return the results of a PEXUpdatePickMeasure request.

The pick measure input data records for the registered pick device types are:

DC_HitBox : [pick_position : DEVICE_COORD_2D, pick_distance : FLOAT]

NPC_HitVolume : [pick_volume : NPC_SUBVOLUME]

PEX Version 5.1, 31-August-1992

13. PEX Fonts

______________________________________________________________________________________________ The PEX font manipulation mechanisms are the same mechanisms as those used for X11 fonts. The PEX font resource is very similar to the font resource created by (and managed by) X11. PEX fonts that are used with PEX stroke precision text contain more functionality than is currently found in X11 fonts. Specifically, stroke precision text requires scalable and rotatable text fonts. Because of the added capabilities of PEX fonts, PEX has defined its own PEX font open, close, and query requests. The X11 font manipulation requests and the corresponding PEX font manipulation requests are listed below:

OpenFont augmented by PEXOpenFont

CloseFont augmented by PEXCloseFont

ListFonts augmented by PEXListFonts

ListFontsWithInfo augmented by PEXListFontsWithInfo

QueryFont augmented by PEXQueryFont

QueryTextExtents augmented by PEXQueryTextExtents

X11 fonts and PEX fonts can be stored in the same location on the server. PEX uses the X11 font path in order to find where PEX font files are located. (The X11 request SetFontPath is used to set the current font path and the

X11 request GetFontPath is used to query the current font path.)

PEX Version 5.1, 31-August-1992

13.1. PEX Font Resource Management

The PEX font is an X11 resource and carries all of the responsibilities and access rights of X11 resources. These requests manage the opening and closing of PEX font resources.

13.1.1. Open PEX Font

Name: PEXOpenFont

Request:f_id: PEX_FONT_ID name : STRING

Errors: PEXFont, IDChoice, Alloc

Description:This request loads the specified PEX font, if necessary, and associates identifier f_idwith it. The font name should use the ISO Latin-1 encoding, and upper/lower case does not matter. PEX fonts are not associated with a particular screen, and can be used with any renderer or PHIGS workstation resources. An error will be generated if the specified font is not "PEX usable", that is, it is not capable of supporting the full range of PEX text attributes.

13.1.2. Close PEX Font

Name: PEXCloseFont

Errors: PEXFont

Description:This request deletes the association between the resource ID and the PEX font. The PEX font itself will be freed when no other resource references it.

PEX Version 5.1, 31-August-1992

13.2. PEX Font Inquiry

The PEX font requests generate replies with logical information specific to a font. The information is encoded in the following data structures.

PEX_FONTPROP is defined as:

name : ATOM value : CARD32

PEX_FONTINFO is defined as:

first_glyph : CARD32 last_glyph : CARD32 default_glyph : CARD32 all_glyphs_exist : BOOLEAN stroke_font : BOOLEAN properties : LISTofPEX_FONTPROP

The first_glyph, last_glyph, and default_glyphare indices to the first glyph, last glyph, and default glyph of the font.

The default_glyphspecifies the glyph that will be displayed when an undefined or non-existent glyph is used.

Default_glyphmay specify a nonexistent glyph. In this case, if a client tries to display an undefined or non-existent glyph, nothing is drawn by the server (rather than having a default glyph drawn). If all_glyphs_existis True, then all glyphs within the range of first_glyph and last_glyph have non-zero extents. Stroke_fontis a flag indicating if the font is a PEX font and is provided so that the client can build font groups that all have the same text precision.

A font is not guaranteed to have any properties. Whether a property value is a signed or unsigned, and what units it is in must be derived from a priori knowledge of the property. It is strongly recommended that all fonts have at least a CHARSET_REGISTRY property (e.g., "ISO8859") and a CHARSET_ENCODING property (e.g., "1").

PEX Version 5.1, 31-August-1992

13.2.1. Query PEX Font

Name: PEXQueryFont

Request:f_id: PEX_FONT_ID

Reply: font_info: PEX_FONTINFO

Errors: PEXFont

Description:This request generates a reply which contains the logical information about a PEX font.

13.2.2. List PEX Fonts

Name: PEXListFonts

Request:pattern : STRING max_names: CARD16

Reply: font_names: LISTofSTRING

Errors: None

Description:Like X11 ListFonts except that this request only returns the names of fonts that can support the full range of PEX text attributes (i.e., those fonts that are "PEX usable"). This list may or may not contain some of the same fonts returned by the X11 ListFonts request. This request returns a list of at most max_names entries, each of which contains information about a font matching the pattern. Pattern is a string that uses the ISO Latin-1 encoding, and upper/lower case does not matter. In the pattern, the ’?’ character (octal value 77) will match any single character, and the character ’*’ (octal value 52) will match any number of characters. The returned names are in lower case, and are also ISO Latin-1 encoded strings.

PEX Version 5.1, 31-August-1992

13.2.3. List PEX Fonts with Info

Name: PEXListFontsWithInfo

Request:pattern : STRING max_names: CARD16

Reply: font_names: LISTofSTRING fonts: LISTofPEX_FONTINFO

Errors: None

Description:Like X11 ListFontsWithInfo except that this request only returns information about fonts that can support the full range of PEX text attributes (i.e., those fonts that are "PEX usable"). This list may or may not contain some of the same fonts returned by the X11 ListFonts request. This request returns a list of at most max_namesentries, each of which contains information about a font matching the pattern. Pattern is a string that uses the ISO Latin-1 encoding, and upper/lower case does not matter. In the pattern, the ’?’

character (octal value 77) will match any single character, and the character ’*’ (octal value 52) will match any number of characters. The returned names are in lower case, and are also ISO Latin-1 encoded strings.

The information returned for each font is identical to what PEXQueryFont would return.

PEX Version 5.1, 31-August-1992

13.2.4. Query PEX Text Extents

Name: PEXQueryTextExtents

Request:fp_format : FLOAT_FORMAT resource_id : RESOURCE_ID font_group : TABLE_INDEX path : CARD16 expansion : FLOAT spacing : FLOAT height : FLOAT alignment : TEXT_ALIGNMENT strings : LISTofISTRING

Reply: extents: LISTofEXTENT_INFO

Errors: FloatingPointFormat, Value, Match

Description:This request generates a reply which contains extent information in the local 2D text coordinate system for each of the specified strings. The extents of each string in strings is computed independently of the other strings in the list. If resource_id is a renderer or PHIGS workstation resource, the TextFonttable used to perform the extents computation will be the TextFonttable associated with the renderer or PHIGS workstation. If resource_id is a lookup table resource of type TextFont,it is used directly. Font_group provides the index of the entry that is to be used to obtain the font group.

Stroke precision is assumed. The text position is (0,0) in the local 2D text coordinate system.

Concat_point returns the point where the next glyph should go if the string is to be extended. This position is given in the 2D text coordinate system. (A suitable modeling transformation to account for the character up vector will still need to be applied by the client.)

If a specified font has no defined default_glyph(that is, if default_glyphrefers to a non-existent glyph), then undefined glyphs in strings are taken to have all zero metrics.

PEX Version 5.1, 31-August-1992

Appendix A: Definition of Standard PEXSubsets

______________________________________________________________________________________________ PEXGetExtensionInfo returns a 32-bit value (subset_info)containing information about whether the PEX server is a full PEX implementation or whether it supports some combination of the standard subsets. The top 16 bits of this

32-bit value are reserved for use by vendors. The bottom 16 bits contain information about how fully the PEX extension implementation supports the PEX protocol. Three PEX subsets are currently defined: "immediate rendering", "PHIGS workstation" and "structure rendering".

If all of the 16 low-order bits of subset_infoare zero, then the extension is a complete PEX implementation, otherwise the bits are interpreted as follows:

bit 0 set - server supports all requests for "immediate rendering" bit 1 set - server supports all requests for "PHIGS workstation" bit 2 set - server supports all requests for "structure rendering"

For backward compatibility with PEX 5.0, a PEX implementation is not allowed to return with both bit 0 and bit 1 set.If a server is sent a request that is not part of the subset(s) it supports, it will return a Requesterror.

Immediate Rendering Subset

An "immediate rendering" subset should fully support the following PEX resources:

• lookup tables

• name sets

• pipeline contexts

• renderers

• PEX fonts and all of the output commands (the "execute structure" output command will be treated as a no-op). To qualify as an immediate rendering PEX subset, an implementation must support at least the protocol requests in the following list. Protocol requests that are not supported should return an Implementationerror.

PEXGetExtensionInfo PEXCreateRenderer

PEXGetEnumeratedTypeInfo PEXFreeRenderer

PEXGetImpDepConstants PEXChangeRenderer

PEXMatchRendererTargets PEXGetRendererAttributes

PEXGetRendererDynamics

PEXBeginRendering

PEXCreateLookupTable PEXEndRendering

PEXCopyLookupTable PEXBeginStructure

PEXFreeLookupTable PEXEndStructure

PEXGetTableInfo PEXRenderOutputCommands

PEXGetPredefinedEntries

PEXGetDefinedIndices PEXCreateNameSet

PEXGetTableEntry PEXCopyNameSet

PEXGetTableEntries PEXFreeNameSet

PEXSetTableEntries PEXGetNameSet

PEXDeleteTableEntries PEXChangeNameSet

PEXCreatePipelineContext PEXQueryFont

PEXCopyPipelineContext PEXListFontsWithInfo

PEXFreePipelineContext PEXQueryTextExtents

PEX Version 5.1, 31-August-1992

PEXGetPipelineContext PEXListFonts

PEXChangePipelineContext PEXOpenFont

PEXCloseFont

PEXBeginPickOne

PEXEndPickOne

PEXBeginPickAll

PEXEndPickAll PEX Version 5.1, 31-August-1992

PHIGSWorkstation Subset

A "PHIGS workstation" subset should fully support the following PEX resources:

• lookup tables

• name sets

• structures

• search contexts

• PHIGS workstations

• pick measures

• PEX fonts and all of the output commands. To qualify as a PHIGS workstation PEX subset, an implementation must support at least the protocol requests in the following list. Protocol requests that are not supported should return an

Implementationerror.

PEXGetExtensionInfo PEXCreateNameSet

PEXGetEnumeratedTypeInfo PEXCopyNameSet

PEXGetImpDepConstants PEXFreeNameSet

PEXMatchRendererTargets PEXGetNameSet

PEXChangeNameSet

PEXCreateLookupTable PEXCreateSearchContext

PEXCopyLookupTable PEXCopySearchContext

PEXFreeLookupTable PEXFreeSearchContext

PEXGetTableInfo PEXGetSearchContext

PEXGetPredefinedEntries PEXChangeSearchContext

PEXGetDefinedIndices PEXSearchNetwork

PEXGetTableEntry

PEXGetTableEntries

PEXSetTableEntries

PEXDeleteTableEntries PEXCreatePhigsWKS

PEXCreateStructure PEXFreePhigsWKS

PEXCopyStructure PEXGetWKSInfo

PEXDestroyStructures PEXGetDynamics

PEXGetStructureInfo PEXGetViewRep

PEXGetElementInfo PEXRedrawAllStructures

PEXGetStructuresInNetwork PEXUpdateWorkstation

PEXGetAncestors PEXRedrawClipRegion

PEXGetDescendants PEXExecuteDeferredActions

PEXFetchElements PEXSetViewPriority

PEXSetEditingMode PEXSetDisplayUpdateMode

PEXSetElementPointer PEXMapDCtoWC

PEXSetElementPointerAtLabel PEXMapWCtoDC

PEXElementSearch PEXSetViewRep

PEXStoreElements PEXSetWKSWindow

PEXDeleteElements PEXSetWKSViewport

PEXDeleteElementsToLabel PEXSetHLHSRMode

PEXDeleteElementsBetweenLabels PEXSetWKSBufferMode

PEXCopyElements PEXPostStructure

PEXChangeStructureReferences PEXUnpostStructure

PEXUnpostAllStructures

PEXGetWKSPostings

PEX Version 5.1, 31-August-1992

PEXGetPickDevice PEXQueryFont

PEXChangePickDevice PEXListFontsWithInfo

PEXCreatePickMeasure PEXQueryTextExtents

PEXFreePickMeasure PEXListFonts

PEXGetPickMeasure PEXOpenFont

PEXUpdatePickMeasure PEXCloseFont

PEX Version 5.1, 31-August-1992

Structure Rendering Subset

An "structure rendering" subset should fully support the following PEX resources:

• lookup tables

• name sets

• pipeline contexts

• renderers

• structures

• search contexts

• PEX fonts and all of the output commands. To qualify as an structure rendering PEX subset, an implementation must support at least the protocol requests in the following list. Protocol requests that are not supported should return an

Implementationerror.

PEXGetExtensionInfo PEXCreateStructure

PEXGetEnumeratedTypeInfo PEXCopyStructure

PEXGetImpDepConstants PEXDestroyStructures

PEXMatchRendererTargets PEXGetStructureInfo

PEXGetElementInfo

PEXGetStructuresInNetwork

PEXCreateLookupTable PEXGetAncestors

PEXCopyLookupTable PEXGetDescendants

PEXFreeLookupTable PEXFetchElements

PEXGetTableInfo PEXSetEditingMode

PEXGetPredefinedEntries PEXSetElementPointer

PEXGetDefinedIndices PEXSetElementPointerAtLabel

PEXGetTableEntry PEXElementSearch

PEXGetTableEntries PEXStoreElements

PEXSetTableEntries PEXDeleteElements

PEXDeleteTableEntries PEXDeleteElementsToLabel

PEXDeleteElementsBetweenLabels

PEXCreatePipelineContext PEXCopyElements

PEXCopyPipelineContext PEXChangeStructureReferences

PEXFreePipelineContext

PEXGetPipelineContext PEXCreateNameSet

PEXChangePipelineContext PEXCopyNameSet

PEXFreeNameSet

PEXCreateRenderer PEXGetNameSet

PEXFreeRenderer PEXChangeNameSet

PEXChangeRenderer

PEXGetRendererAttributes PEXCreateSearchContext

PEXGetRendererDynamics PEXCopySearchContext

PEXBeginRendering PEXFreeSearchContext

PEXEndRendering PEXGetSearchContext

PEXRenderNetwork PEXChangeSearchContext

PEXRenderElements PEXSearchNetwork

PEXAccumulateState PEXQueryFont

PEXBeginPickOne PEXListFontsWithInfo

PEXEndPickOne PEXQueryTextExtents

PEXPickOne PEXListFonts

PEXBeginPickAll PEXOpenFont

PEXEndPickAll PEXCloseFont

PEX Version 5.1, 31-August-1992

PEXPickAll PEX Version 5.1, 31-August-1992

Appendix B: Minimum Support for PHIGS/PHIGS-PLUS

______________________________________________________________________________________________ In order to fully support a PHIGS client-side implementation and the targeted PHIGS-PLUS functionality, a PEX extension implementation must meet or exceed the following support criteria. Other than the minimum support criteria listed here and the subset information listed in Appendix A, a PEX extension implementation must fully support the functionality described in the PEXProtocol Specification document.

Enumerated Types

MarkerType at least types 1-5 (Dot, Cross, Asterisk,Circle, X)must be supported

ATextStyle at least types 1-2 (NotConnected,Connected) must be supported

InteriorStyle at least types 1,2,5 (Hollow,Solid,Empty)must be supported

HatchStyle it is not required that an implementation support any hatch styles

LineType at least types 1-4 (Solid,Dashed, Dotted, DashDot) must be supported

SurfaceEdgeType at least type 1 (Solid)must be supported

PickDeviceType at least pick device type 1 (DC_HitBox)must be supported (for full implementation or for the "PHIGS workstation only" subset)

PolylineInterpMethod at least types 1-2 (None,Color) must be supported

CurveApproxMethod at least types 1-8 (imp.dep., ConstantBetweenKnots,WCS_ChordalSize,

NPC_ChordalSize, DC_ChordalSize, WCS_ChordalDev,NPC_ChordalDev,

DC_ChordalDev) must be supported

ReflectionModel at least types 1-4 (NoShading,Ambient,Diffuse,Specular) must be supported

SurfaceInterpMethod at least types 1-2 (None,Color) must be supported

SurfaceApproxMethod at least types 1-8 (imp.dep., ConstantBetweenKnots,WCS_ChordalSize,

NPC_ChordalSize, DC_ChordalSize, WCS_PlanarDev, NPC_PlanarDev,

DC_PlanarDev) must be supported

TrimCurveApproxMethod at least types 1-2 (imp.dep., ConstantBetweenKnots)must be supported

ModelClipOperator at least types 1-2 (Replace, Intersection) must be supported

LightType at least types 1-4 (Ambient,WCS_Vector,WCS_Point,WCS_Spot) must be supported

ColorType type 0 (Indexed)and types 1 (RGBFloat) must be supported

FloatFormat at least one of types 1-2 (IEEE_754_32, DEC_F_Floating) must be supported

HLHSRMode at least type 1 (Off)and one other type (ZBuffer,Painters, Scanline,

HiddenLineOnly,or an implementation-dependent type) must be supported

PromptEchoType at least type 1 (EchoPrimitive) must be supported

DisplayUpdateMode at least types 1-3 (VisualizeEach,VisualizeEasy,VisualizeNone)must be supported

ColorApproxType at least one of types 1-2 {ColorSpace, ColorRange} must be supported

ColorApproxModel at least one of types 1-5 {RGB,HSV,HLS,CIE, YIQ}must be supported

RenderingColorModel at least type 0 (implementation-dependent) must be supported

ParametricSurfaceCharacteristics at least types 1-3 (None,imp.dep., IsoparametricCurves) must be supported

BufferMode it is not required that an implementation support double buffering

GDP it is not required that an implementation support any GDPs

GDP3 it is not required that an implementation support any GDP3s

GSE it is not required that an implementation support any GSEs

Output Primitive Attributes marker_scale marker scale factors other than 1.0 may be ignored text_precision all types (Stroke,Char, String) must be supported char_expansion character expansion other than 1.0 may be ignored char_height character height other than 0.01 may be ignored atext_height annotation text character height other than 0.01 may be ignored

PEX Version 5.1, 31-August-1992 line_width line widths other than 1.0 may be ignored interior_style_index this attribute may be ignored if neither Pattern nor Hatch style is supported reflection_attr transmission coefficient attribute may be ignored bf_interior_style_index this attribute may be ignored if neither Pattern nor Hatch style is supported bf_reflection_attr transmission coefficient attribute may be ignored pattern_size this attribute may be ignored if Pattern style is not supported pattern_ref_pt this attribute may be ignored if Pattern style is not supported pattern_ref_vec1 this attribute may be ignored if Pattern style is not supported pattern_ref_vec2 this attribute may be ignored if Pattern style is not supported surface_edge_width surface edge widths other than 1.0 may be ignored model_clip_volume must support the combining of at least six halfspaces to compute the modeling clipping volume depth_cue attributes depth cue attributes other than the default (depth cue off) may be ignored

HLHSR_identifier at least one must be available specific GSEs may be ignored

Output Primitives

NURB surfaces must be supported up to order six

NURB curves must be supported up to order six trim curves must be supported up to order four cell arrays may be simulated by drawing the outline of the cell array specific GDPs may be ignored

Lookup Tables

LineBundle must support at least 5 entries

MarkerBundle must support at least 5 entries

TextBundle must support at least 6 entries

InteriorBundle must support at least 5 entries

EdgeBundle must support at least 5 entries

Pattern must support at least 10 entries (if interior style Pattern supported)

Color must support at least 2 entries

TextFont must support at least 2 entries

View must support at least 6 entries

Light must support at least 2 entries

DepthCue must support at least 2 entries

ColorApprox must support at least 1 entry

Miscellaneous fonts an implementation need not support drawing text primitives with X11 fonts font one must be mono-spaced namesets at least 64 names must be supported search contexts at least one normal and one inverted filter list must be supported ws display priorities at least two ws display priorities must be supported

PEX Version 5.1, 31-August-1992

Appendix C: Definition of PEX Errors

______________________________________________________________________________________________ PEXGetExtensionInfo none

PEXGetEnumeratedTypeInfo

Drawable: specified drawable resource ID is invalid

Value: specified enumerated type number is invalid

Match: specified drawable is not supported

PEXGetImpDepConstants

Value: a specified constant name is invalid

FloatingPointFormat: device does not support the specified fp format

PEXMatchRendererTargets

Value: specified visual is invalid

PEXEscapeValue: a specified constant name is invalid

PEXEscapeWithReply

PEXCreateLookupTable

IDChoice: ID already in use or not in range assigned to client

Value: table_type value does not name a valid table type

Alloc: server failed to allocate the requested resource

LookupTable: table type not supported by implementation

PEXCopyLookupTable

LookupTable: either src_lut_id or dest_lut_id is an invalid resource ID

Match: src_lut_id and dest_lut_id must have been created for use on the same class of drawables, and must be the same type of lookup table

PEXFreeLookupTable

LookupTable: lut_id contains an invalid lut resource ID

PEXGetTableInfo

PEXGetPredefinedEntries

PEX Version 5.1, 31-August-1992

Match: specified drawable is not supported

Value: table_type value does not name a valid table type

Value: start < min predefined entry

Value: start + count > max predefined entry

Value: entry 0 not valid for this table type

FloatingPointFormat: device does not support the specified fp format

LookupTable: table type not supported by implementation

PEXGetDefinedIndices

LookupTable: lut_id contains an invalid lut resource ID

PEXGetTableEntry

PEXGetTableEntries

Value: start + count is greater than 65535

PEXSetTableEntries

Value: illegal value in one of the fields of a table entry

ColorType: device does not support the specified color type

ColorType: color type may not be Indexedfor color lookup table

Alloc: table is full

PEXDeleteTableEntries

PEXCreatePipelineContext

IDChoice: ID already in use or not in range assigned to client

Value: an item in the item_list is out of range

Value: illegal bit set in item mask parameter

Alloc: server failed to allocate the requested resource

NameSet: a specified name set resource ID is invalid

PEXCopyPipelineContext

PipelineContext: pc_id contains an invalid pipeline context ID

PEX Version 5.1, 31-August-1992

Value: illegal bit set in item mask parameter

PEXFreePipelineContext

PipelineContext: pc_id contains an invalid pipeline context ID

PEXGetPipelineContext

FloatingPointFormat: device does not support the specified fp format

Value: illegal bit set in item mask parameter

PEXChangePipelineContext

Value: an item in the item_list is out of range

ColorType: device does not support the specified color type

NameSet: a specified name set resource ID is invalid

PEXCreateRenderer

IDChoice: ID already in use or not in range assigned to client

Drawable: specified drawable resource ID is invalid

PipelineContext: specified pipeline context resource ID is invalid

LookupTable: a specified lookup table resource ID is invalid

Alloc: server failed to allocate the requested resource

Match: lookup table root/depth does not match example drawable’s root/depth

Match: specified drawable is not supported

PEXFreeRenderer

Renderer: specified renderer resource ID is invalid

PEXChangeRenderer

Match: specified lookup table resource was not created for drawables of the same root and depth as the specified renderer

PEXGetRendererAttributes

PEXGetRendererDynamics

PEX Version 5.1, 31-August-1992

PEXBeginRendering

Renderer: specified renderer resource ID is invalid

Drawable: specified drawable resource ID is invalid

Match: specified renderer resource was not created for drawables of the same root and depth as the specified drawable

Match: specified drawable is not supported

Alloc: server was unable to allocate the resources necessary to do rendering

RendererState: renderer was in the Rendering or Picking state

PEXEndRendering

RendererState: renderer was in the Picking state

PEXBeginStructure

PEXEndStructure

RendererState: no matching begin structure

PEXRenderOutputCommands

FloatingPointFormat: device does not support the specified fp format

OutputCommand: illegal value in output commands

PEXRenderElements

Structure: specified structure resource ID is invalid

Value: bad value for "whence" parameter

PEXAccumulateState

Path: illegal or poorly-formed search path (includes invalid structure

IDs, invalid element offset values)

PEXRenderNetwork

PEXBeginPickOne

Alloc: server was unable to allocate the resources necessary to do picking

PEX Version 5.1, 31-August-1992

Value: bad value given for "pick_type" or "pick_data"

PEXEndPickOne

Renderer: specified renderer resource ID is invalid

RendererState: renderer was in the Rendering state

PEXPickOne

Drawable: specified drawable resource ID is invalid

Structure: specified structure resource ID is invalid

Match: specified renderer resource was not created for drawables of the same root and depth as the specified drawable

Match: specified drawable is not supported

Alloc: server was unable to allocate the resources necessary to do picking

RendererState: renderer was in the Rendering or Picking state

Value: bad value given for "pick_type" or "pick_data"

PEXBeginPickAll

Value: bad value given for "pick_data"

PEXEndPickAll

PEXPickAll

Path: initial pick path is invalid

PEXCreateStructure

IDChoice: ID already in use or not in range assigned to client

Alloc: server failed to allocate the requested resource

PEXCopyStructure

PEXDestroyStructures

PEX Version 5.1, 31-August-1992

PEXGetStructureInfo

Structure: specified structure resource ID is invalid

FloatingPointFormat: device does not support the specified fp format

Value: illegal bit set in item_mask parameter

PEXGetElementInfo

Value: bad value for "whence" parameter

PEXGetStructuresInNetwork

Value: bad value for "which" parameter

PEXGetAncestors

Value: bad value for "path_part" parameter

PEXGetDescendants

PEXFetchElements

PEXSetEditingMode

Value: bad value for "mode" parameter

PEXSetElementPointer

PEXSetElementPointerAtLabel

Label: no occurrences of specified label in structure

PEXElementSearch

Value: bad value for "whence" or "direction" parameters

PEXStoreElements

OutputCommand: illegal value in output commands

PEXDeleteElements

PEXDeleteElementsToLabel PEX Version 5.1, 31-August-1992

Structure: specified structure resource ID is invalid

Label: no occurrences of specified label in structure

Value: bad value for "whence" parameter

PEXDeleteElementsBetweenLabels

Structure: specified structure resource ID is invalid

PEXCopyElements

PEXChangeStructureReferences

PEXCreateNameSet

IDChoice: ID already in use or not in range assigned to client

Alloc: server failed to allocate the requested resource

PEXCopyNameSet

NameSet: specified name set resource ID is invalid

PEXFreeNameSet

PEXGetNameSet

PEXChangeNameSet

Value: bad value for "action" parameter

PEXCreateSearchContext

Value: an item in the item_list is out of range

Value: illegal bit set in item mask parameter

FloatingPointFormat: device does not support the specified fp format

Path: illegal or poorly-formed search path (includes invalid structure

IDs, invalid element offset values)

PEXCopySearchContext

SearchContext: specified search context resource ID is invalid

PEXFreeSearchContext

PEXGetSearchContext

PEX Version 5.1, 31-August-1992

PEXChangeSearchContext

SearchContext: specified search context resource ID is invalid

Value: an item in the item_list is out of range

Value: illegal bit set in item mask parameter

FloatingPointFormat: device does not support the specified fp format

Path: illegal or poorly-formed search path (includes invalid structure

IDs, invalid element offset values)

NameSet: specified name set resource ID is invalid

PEXSearchNetwork

PEXCreatePhigsWKS

IDChoice: ID already in use or not in range assigned to client

Drawable: specified drawable resource ID is invalid

Match: specified lookup table resource was not created for drawables of the same root and depth as the specified drawable

Match: specified drawable is not supported

LookupTable: a specified lookup table resource ID is invalid

NameSet: a specified name set resource ID is invalid

Alloc: server failed to allocate the requested resource

Alloc: server cannot allocate resources necessary for double-buffering

Value: bad value for buffer_mode parameter

PEXFreePhigsWKS

PhigsWKS: specified PHIGS workstation resource ID is invalid

PEXGetWKSInfo

PEXGetDynamics

PEXGetViewRep

Value: specified view table entry is not defined

PEXRedrawAllStructures

PEXUpdateWorkstation

PEXRedrawClipRegion

PEXExecuteDeferredActions PEX Version 5.1, 31-August-1992

PhigsWKS: specified PHIGS workstation resource ID is invalid

PEXSetViewPriority

PhigsWKS: specified PHIGS workstation resource ID is invalid

Value: bad value for "priority" parameter

Value: specified table entry is not defined

PEXSetDisplayUpdateMode

Value: bad value for "display_update" parameter

PEXMapWCtoDC

FloatingPointFormat: device does not support the specified fp format

PEXMapDCtoWC

PEXSetViewRep

Alloc: table is full

PEXSetWKSWindow

PEXSetWKSViewport

Value: bad value for "use_drawable" parameter

PEXSetHLHSRMode

Value: bad value for "mode" parameter

Alloc: server cannot allocate necessary resources

PEXSetWKSBufferMode

Value: bad or unsupported value for "buffer_mode" parameter

Alloc: server cannot allocate resources necessary for double-buffering

PEXPostStructure

Structure: specified structure resource ID is invalid

PEXUnpostStructure

PEXUnpostAllStructures PEX Version 5.1, 31-August-1992

PhigsWKS: specified PHIGS workstation resource ID is invalid

PEXGetWKSPostings

Structure: specified structure resource ID is invalid

PEXGetPickDevice

PhigsWKS: specified PHIGS workstation resource ID is invalid

Value: bad value for "dev_type" parameter

Value: illegal bit set in item mask parameter

FloatingPointFormat: device does not support the specified fp format

PEXChangePickDevice

Value: an item in the item_list is out of range

Path: illegal or poorly-formed pick path (includes invalid structure

IDs, invalid element offset values)

NameSet: a specified name set resource ID is invalid

PEXCreatePickMeasure

IDChoice: ID already in use or not in range assigned to client

Alloc: server failed to allocate the requested resource

PEXFreePickMeasure

PickMeasure: specified pick measure resource ID is invalid

PEXGetPickMeasure

PEXUpdatePickMeasure

Path: illegal or poorly-formed search path (includes invalid structure

PEXOpenFont

PEXFont: string does not name a useable PEX font

PEXCloseFont

PEXFont: specified PEX font resource ID is invalid

PEXQueryFont

PEXListFonts none PEX Version 5.1, 31-August-1992

PEXListFontsWithInfo none

PEXQueryTextExtents

FloatingPointFormat: device does not support the specified fp format

Value: input text attribute values are illegal or out of range

Value: resource ID does not name a valid renderer, PHIGS workstation or lookup table

Match: resource ID specifies a table of type other than TextFont

PEX Version 5.1, 31-August-1992

Appendix D: Definition of Table Default Values

______________________________________________________________________________________________ If a table entry that is not defined is referenced, the contents of the default table entry will be used. The default entry for all tables is one, except for the view, depth cue, and color approximation tables whose default entry is zero. If the contents of the default table entry is not defined, then the default attribute values listed below will be used to define a default table entry that will be used instead. For each type of table, the attribute name, data type, and default value are listed. Each PEX implementation should provide documentation describing the choices it made for those attributes listed as "implementation-dependent".

LineBundle (1..65535, default entry = 1) line_type LINE_TYPE LineTypeSolid polyline_interp POLYLINE_INTERP PolylineInterpNone curve_approx CURVE_APPROX {1, 1.0}† line_width FLOAT 1.0 line_color COLOR_SPECIFIER {Indexed,1}

MarkerBundle (1..65535, default entry = 1) marker_type MARKER_TYPE MarkerAsterisk marker_scale FLOAT 1.0 marker_color COLOR_SPECIFIER {Indexed,1}

TextBundle (1..65535, default entry = 1) text_font_index TABLE_INDEX 1 text_precision TEXT_PRECISION String char_expansion FLOAT 1.0 char_spacing FLOAT 0.0 text_color COLOR_SPECIFIER {Indexed,1}

InteriorBundle (1..65535, default entry = 1) interior_style INTERIOR_STYLE InteriorStyleHollow interior_style_index TYPE_OR_TABLE_INDEX 1 surface_color COLOR_SPECIFIER {Indexed,1} reflection_attr REFLECTION_ATTR {1.0, 1.0, 1.0, 0.0, 0.0, (Indexed,1)} reflection_model REFLECTION_MODEL ReflectionNoShading surface_interp SURFACE_INTERP SurfaceInterpNone bf_interior_style INTERIOR_STYLE InteriorStyleHollow bf_interior_style_index TYPE_OR_TABLE_INDEX 1 bf_surface_color COLOR_SPECIFIER {Indexed,1} bf_reflection_attr REFLECTION_ATTR {1.0, 1.0, 1.0, 0.0, 0.0, (Indexed,1)} bf_reflection_model REFLECTION_MODEL ReflectionNoShading bf_surface_interp SURFACE_INTERP SurfaceInterpNone surface_approx SURFACE_APPROX {1, 1.0, 1.0}

__________________ † PHIGS-PLUS defines the default curve approximation type to be 1, which is an implementation-dependent method.

PEX Version 5.1, 31-August-1992

EdgeBundle (1..65535, default entry = 1) surface_edges SWITCH Off surface_edge_type SURFACE_EDGE_TYPE SurfaceEdgeSolid surface_edge_width FLOAT 1.0 surface_edge_color COLOR_SPECIFIER {Indexed,1}

Pattern (1..65535, default entry = 1) color_type COLOR_TYPE implementation-dependent numx CARD16 implementation-dependent numy CARD16 implementation-dependent colors LISTofCOLOR implementation-dependent

Color (0..65534, default entry = 1) color DIRECT_COLOR implementation-dependent

TextFont (1..65535, default entry = 1) font LISTofFONT_ID implementation-dependent

View (0..65534, default entry = 0) clip_flags BITMASK_SHORT all On clip_limits NPC_SUBVOLUME (0,0,0),(1,1,1) orientation MATRIX identity matrix mapping MATRIX identity matrix

Light (1..65535, default entry = 1) light_type LIGHT_TYPE implementation-dependent direction VECTOR_3D implementation-dependent point COORD_3D implementation-dependent concentration FLOAT implementation-dependent spread_angle FLOAT implementation-dependent attenuation [factor1, factor2 : FLOAT] implementation-dependent color COLOR_SPECIFIER implementation-dependent

Depending on the type of light, some of the values in a table entry may be ignored. Undefined entries in the light table that are referenced are treated as lights that are set to Off.

DepthCue (0..65534, default entry = 0) mode SWITCH Off front_plane FLOAT implementation-dependent back_plane FLOAT implementation-dependent front_scaling FLOAT implementation-dependent back_scaling FLOAT implementation-dependent

PEX Version 5.1, 31-August-1992

ColorApprox (0..65534, default entry = 0) type COLOR_APPROX_TYPE implementation-dependent color_model COLOR_APPROX_MODEL implementation-dependent max1 CARD16 implementation-dependent max2 CARD16 implementation-dependent max3 CARD16 implementation-dependent mult1 CARD32 implementation-dependent mult2 CARD32 implementation-dependent mult3 CARD32 implementation-dependent weight1 FLOAT implementation-dependent weight2 FLOAT implementation-dependent weight3 FLOAT implementation-dependent base_pixel CARD32 implementation-dependent dither SWITCH implementation-dependent

It is suggested that PEX implementations provide default entries that correlate with the X definition of

RGB_DEFAULT_MAP for the device. For instance, if a device has eight-bit pixels which index into a 24-bit hardware colormap, and its notion of an RGB_DEFAULT_MAP is a 6×6×6 color cube encoded in 216 colormap entries starting with cell number 16, then the suggested values might be:

type COLOR_APPROX_TYPE ColorSpace color_model COLOR_APPROX_MODEL RGB max1 CARD16 5 max2 CARD16 5 max3 CARD16 5 mult1 CARD32 1 mult2 CARD32 6 mult3 CARD32 36 weight1 FLOAT 1.0 weight2 FLOAT 1.0 weight3 FLOAT 1.0 base_pixel CARD32 16 dither SWITCH Off

PEX Version 5.1, 31-August-1992

Appendix E: Registered PEX Escapes

______________________________________________________________________________________________ A PEX implementation is not required to support any of the registered PEX escapes. The list of supported escapes which a particular PEX implementation supports can be inquired by calling PEXGetEnumeratedTypeInfo. All registered escapes contain an escape_id-- this is a positive number which identifies the escape request.

Set Echo Color

Name: PEXSetEchoColor

Request:escape_id : CARD32 fp_format : FLOAT_FORMAT rdr_id : RENDERER_ID echo_color : COLOR_SPECIFIER

Errors: Renderer, ColorType, FloatingPointFormat

Description:This request changes the renderer’s echo_color attribute. The modification is dynamic and takes effect immediately. The echo color is used to renderer primitives when the renderer’s echo_modeis set to Echo.

The lighting and shading for echoed primitives is implementation-dependent.

echo_color is a new renderer attribute introduced by this request and the concept of an echo color may not be supported by PEX implementations which do not support this escape. The echo_color renderer attribute cannot be inquired and the default value is implementation-dependent.

If the specified renderer identifier is invalid then a Renderer error is generated. A ColorTypeerror is returned if the specified color type (in the echo_color) is not supported and a FloatingPointFormat error is returned if the specified floating point format is not supported. The supported color types and floating point formats can be inquired by calling PEXGetEnumeratedTypeInfo.

PEX Version 5.1, 31-August-1992